---
title: "Preparation of input data: geomorphological analysis with whitebox"
author: "Alban de Lavenne & Antoine Casquin"
date: "`r Sys.Date()`"
bibliography: "../inst/REFERENCES.bib"
output: rmarkdown::html_vignette
vignette: >
  %\VignetteIndexEntry{Preparation of input data: geomorphological analysis with whitebox}
  %\VignetteEngine{knitr::rmarkdown}
  %\VignetteEncoding{UTF-8}
fig_width: 8 
fig_height: 4 
---

```{r setup, include = FALSE}
library(transfR)
knitr::opts_chunk$set(
  collapse = TRUE,
  comment = "#>"
)
```

The hydrological modelling of the `transfR` package is based on a geomorphological analysis of the studied catchments. In this vignette, we give some guidance on how to perform this geomorphological analysis. More specifically, we extract the catchment delineation and hydraulic length maps from a digital elevation model (DEM). This analysis is one of the two inputs needed (together with the time series of flow observations) to build a `transfR` object and start using the `transfR` package (see the *Get started with transfR* vignette). 

Hydraulic length is defined as the distance within the river network along an identified flow path to the outlet. It can be extracted from a DEM in many different ways, such as with the GRASS toolkits [@Jasiewicz2011], Whitebox GAT (see @Lindsay2016 or [WhiteboxTools](https://github.com/jblindsay/whitebox-tools)), TauDEM (D. Tarboton, Utah State University) or online services (@Squividant2015 for catchment delineation only). This vignette presents one possible workflow by making use of two main R packages: 

* [`elevatr`](https://cran.r-project.org/package=elevatr) that provides elevation data worldwide from Various APIs. 
* [`whitebox`](https://cran.r-project.org/package=whitebox), an R frontend for the 'WhiteboxTools' library, which is an advanced geospatial data analysis platform.

Functions of the `whitebox` package generally do not work with objects in R memory, but with files written on the disk storage. It is therefore advised to define the working directory where these files will be written.


```{r, echo=TRUE, message=FALSE, warning=FALSE, results='hide'}
wbt_wd <- tempdir(check = TRUE)
```

## 1. Retrieve elevation data with `elevatr`

The `elevatr` package allows retrieving grids (rasters) of elevation data worldwide for various zoom levels and data sources. It uses the [Open Topography Global Datasets API](https://opentopography.org/developers) for accessing Shuttle Radar Topography Mission (SRTM) data.

It is necessary to assign a geographic projection for the catchment delineation and hydraulic length maps with the `whitebox` package. We chose to use the Lambert93 projection, the official projection for maps of metropolitan France, for which the [EPSG code is 2154](https://epsg.io/2154).

```{r, download_dem, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE, results='hide'}
library(elevatr)
library(progress) # Needed by elevatr

# Set up a projection (French Lambert-93 projection)
EPSG <- 2154 

# Define a bbox that will encompass the catchments of the study area
blavet_bbox <- st_bbox(c(xmin = -3.3, xmax = -2.7, ymax = 48.11, ymin = 47.77), 
                           crs = st_crs(4326))
blavet_loc <- st_as_sfc(blavet_bbox) |> st_sf()

# Retrieve elevation data as raster
dem_raw <- elevatr::get_elev_raster(blavet_loc, z = 10) # ~76m resolution

# Project and define spatial resolution: 
dem_100m  <- st_warp(st_as_stars(dem_raw), cellsize = 100, crs = st_crs(EPSG))
names(dem_100m) <- "warp"

# Set negative values (ocean) to NA
dem_100m[dem_100m < 0] <- NA

# Write to file
write_stars(dem_100m["warp"], file.path(wbt_wd,"dem_100m.tif"))
```

```{r, echo=FALSE, message=FALSE, warning=TRUE, eval=TRUE, results='hide'}
try_chunk <- try({
<<download_dem>>
}, silent = TRUE)
if(inherits(try_chunk, "try-error")){
  warning("\nIssue when downloading elevation data. \nThe vignette will not be fully built.")
  running <- FALSE
}else{
  running <- TRUE
}
```

## 2. Retrieve a known river network and burn it into DEM (optional)

The hydrological modelling distinguish the hillslope from the river network. Both will have very different transfer dynamics, and the `transfR` package aims to describe the transfer function of the river network only. Defining where this river network begins and the flow path it takes is a key, and non-trivial, issue for hydrogeomorphologists. The easiest way to draw a drainage network from a DEM is usually to define a minimum drainage area threshold at which the drainage network is assumed to start. However, defining this threshold can be difficult as it may vary spatially, especially with the geology of the region. It may therefore be better to use a known river network and force the flow paths to follow it. Here we will use the [French TOPAGE river network](http://www.sandre.eaufrance.fr/?urn=urn:sandre:ensembledonnees:BDTopage:FRA:::ressource:latest:::html) as a reference (see the description of the `Blavet` dataset to download it from the Web Feature Service (WFS) "Sandre - Eau France"). We will implement a stream burning technique into the DEM using the function [`whitebox::wbt_burn_streams_at_roads()`](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#BurnStreamsAtRoads) and following @Lindsay2016a.

```{r, install_whitebox, echo=FALSE, message=FALSE, warning=TRUE, eval=running, results='hide'}
# If WhiteboxTools executable are not present, install it in the temporary directory
library(whitebox)
if(!wbt_init()){
  wbt_inst <- try(install_whitebox(pkg_dir = wbt_wd), silent = TRUE)
  if(!inherits(wbt_inst, "try-error")){
    exe_path <- file.path(wbt_wd, "WBT", "whitebox_tools") # Unix
    if(!file.exists(exe_path)) exe_path <- paste0(exe_path,".exe") # Windows
    if(!file.exists(exe_path)){
      warning("WhiteboxTools executable not found")
      running <- FALSE
    }else{
        wbt_options(exe_path = exe_path,
                max_procs = 2,
                wd = wbt_wd,
                verbose = TRUE)
      }
    }else{running <- FALSE}
  }else{
    wbt_options(max_procs = 2,
                wd = wbt_wd,
                verbose = TRUE)
  }
```

```{r, burn_stream, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE, results='hide'}
library(transfR)
library(whitebox)

# Get the French Topage river network from the Blavet dataset
data(Blavet)
CoursEau_Topage2019 <- Blavet$network

# Change projection and write files
network_topage <- st_transform(CoursEau_Topage2019, EPSG)
st_write(network_topage, file.path(wbt_wd, "network_topage.shp"), 
             delete_layer = TRUE, quiet = TRUE)
whitebox::wbt_rasterize_streams("network_topage.shp", 
                                base = "dem_100m.tif", 
                                output = "network_topage.tif", 
                                nodata = 0, 
                                wd = wbt_wd)

# Burn this river network on the DEM
# We will neglect the effect of the road embankments at this DEM resolution of 100m 
# by creating an empty shapefile for roads
st_write(st_sfc(st_multilinestring(),crs = EPSG), file.path(wbt_wd,"roads.shp"), 
             delete_layer = TRUE, quiet = TRUE)
whitebox::wbt_burn_streams_at_roads(dem = "dem_100m.tif", 
                        streams = "network_topage.shp", 
                        roads = "roads.shp",
                        output = "dem_100m_burn.tif", 
                        wd = wbt_wd)
```
```{r, echo=FALSE, message=FALSE, warning=TRUE, eval=running, results='hide'}
try_chunk <- try({
<<burn_stream>>
}, silent = TRUE)
if(inherits(try_chunk, "try-error")){
  warning("\nIssue when burning the river network on the DEM. \nThe vignette will not be fully built.")
  running <- FALSE
}
```

## 3. Delineate catchments from their outlets coordinates

The `whitebox` package provides all the tools to perform a usual catchment delineation workflow from a DEM and outlet's coordinates. It can be done in 6 different steps:

* [Fill the depressions](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#FillDepressions),
* [Compute flow direction](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#D8Pointer) using D8 algorithm,
* [Compute flow accumulation](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#D8FlowAccumulation) according to flow direction,
* [Extract a river network](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/stream_network_analysis.html?highlight=extract%20stream#extractstreams) using a threshold in flow accumulation,
* [Snap the outlets](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#jensonsnappourpoints) to this river network,
* [Delimit the catchments](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#Watershed).


```{r, extract_stream, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE, results='hide'}
# Remove the depressions on the DEM
whitebox::wbt_fill_depressions(dem = "dem_100m_burn.tif",
                               output = "dem_fill.tif",
                               wd = wbt_wd)

# Flow direction raster
whitebox::wbt_d8_pointer(dem = "dem_fill.tif",
                         output = "d8.tif",
                         wd = wbt_wd)

# Compute flow accumulation
whitebox::wbt_d8_flow_accumulation(input = "d8.tif",
                                   pntr = TRUE,
                                   output ="facc.tif",
                                   wd = wbt_wd)

# Extract a stream network (threshold = 1 km2) consistent with flow direction
whitebox::wbt_extract_streams(flow_accum =  "facc.tif",
                              threshold = 100, # 100 cells for 1 km2
                              output = "network_1km2.tif",
                              zero_background = TRUE,
                              wd = wbt_wd)
whitebox::wbt_remove_short_streams(d8_pntr = "d8.tif",
                                   streams = "network_1km2.tif",
                                   output = "network_d8.tif",
                                   min_length= 200,
                                   wd = wbt_wd)
```

```{r, echo=FALSE, message=FALSE, warning=TRUE, eval=running, results='hide'}
try_chunk <- try({
<<extract_stream>>
}, silent = TRUE)
if(inherits(try_chunk, "try-error")){
  warning("\nIssue when extracting the river network from the DEM. \nThe vignette will not be fully built.")
  running <- FALSE
}
```

Coordinates of the outlets are retrieved from [hydro.eaufrance.fr](https://www.hydro.eaufrance.fr/) and snapped to the pixel of the river network that is consistent with the previously defined flow directions.

```{r, delineate_catchments, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE, results='hide'}
# Localize the outlets of the studied catchments (with manual adjustments to help snapping)
outlets_coordinates <- data.frame(id = names(Blavet$hl),
                             X = c(254010.612,255940-100,255903,237201,273672,265550),
                             Y = c(6772515.474,6776418-200,6776495,6774304-200,6762681,6783313))
outlets <- st_as_sf(outlets_coordinates, coords = c("X", "Y"), crs=2154)
st_write(outlets, dsn = file.path(wbt_wd, "outlets.shp"), 
             delete_layer = TRUE, quiet = TRUE)

# Snap the outlets on the stream raster
whitebox::wbt_jenson_snap_pour_points(pour_pts = "outlets.shp",
                                      streams = "network_d8.tif",
                                      output = "outlets_snapped.shp",
                                      snap_dist = 200,
                                      wd = wbt_wd) 
outlets_snapped <- st_read(file.path(wbt_wd, "outlets_snapped.shp"), quiet = TRUE)

# Delineate catchments 
catchments <- st_sfc(crs = EPSG)
for(id in outlets_snapped$id){
  st_write(outlets_snapped[outlets_snapped$id==id,], 
               file.path(wbt_wd, paste0(id, "_outlet.shp")), delete_layer = TRUE, quiet = TRUE)
  whitebox::wbt_watershed(d8_pntr = "d8.tif",
                          pour_pts = paste0(id, "_outlet.shp"),
                          output = paste0(id, "_catchment.tif"),
                          wd = wbt_wd)
  # Vectorize catchments
  drainage <- read_stars(file.path(wbt_wd, paste0(id, "_catchment.tif")))
  contours <- st_contour(drainage, breaks = 1) |> st_geometry() |> st_cast("POLYGON")
  contours <- contours[which.max(st_area(contours))]
  catchments <- rbind(catchments, st_sf(data.frame(id, geom = contours)))
}
```

```{r, echo=FALSE, message=FALSE, warning=TRUE, eval=running, results='hide'}
try_chunk <- try({
<<delineate_catchments>>
}, silent = TRUE)
if(inherits(try_chunk, "try-error")){
  warning("\nIssue when delineating catchments. \nThe vignette will not be fully built.")
  running <- FALSE
}
```

Resulting catchments delineation can be plotted and checked.

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=running}
# Compare drainage areas to the dataset provided with transfR
compare_areas <- data.frame(
  name = names(Blavet$hl),
  expected_area =  st_area(st_geometry(Blavet$obs)) |> units::set_units("km^2") |> round(1),
  computed_area = st_area(catchments) |> units::set_units("km^2") |> round(1)
)

print(compare_areas)
```

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=running, results='hide', fig.width=7, fig.height=4}
# Plot catchment delineation
par(oma = c(0, 0, 0, 6))
plot(catchments[,"id"], main = "Catchments delineation", key.pos = 4, reset = FALSE)
plot(st_geometry(st_intersection(network_topage,catchments)), 
     col = "white", lwd = 1.5, add = TRUE)
plot(outlets_snapped, col = "black", pch = 16, add = TRUE)
```


## 4. Compute flow path length and hydraulic length for each catchments

The `whitebox` package does not provide a function to compute hydraulic length directly. However, it can compute the total [downslope flow path length to the outlet](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#DownslopeFlowpathLength) using `whitebox::wbt_downslope_flowpath_length()` function and the [downslope distance to the stream](https://www.whiteboxgeo.com/manual/wbt_book/available_tools/hydrological_analysis.html#DownslopeDistanceToStream) using `whitebox::wbt_downslope_distance_to_stream()` function. The hydraulic length does not take into account the length of the flow path over the hillslopes, so it can be calculated simply by the difference of these two flow distances.

Flow path lengths are computed once for all the study area. For each catchment, this raster is then trimmed (i.e. removing NA values outside the bounding box of the catchment) and the values of flow path lengths are corrected such as the minimum flow path length is equal to half a pixel width/height. The hydraulic lengths are finally gathered in a list as expected by the `as_transfr()` function.


```{r, hydraulic_length, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE, results='hide'}
# Compute hydraulic length
whitebox::wbt_downslope_flowpath_length(d8_pntr = "d8.tif",
                                        output = "fpl.tif",
                                        wd = wbt_wd)
whitebox::wbt_downslope_distance_to_stream(dem = "dem_fill.tif",
                                           streams = "network_topage.tif",
                                           output = "d2s.tif",
                                           wd = wbt_wd)
fpl <- read_stars(file.path(wbt_wd, "fpl.tif"))
d2s <- read_stars(file.path(wbt_wd, "d2s.tif"))
hl_region <- fpl-d2s
names(hl_region) <- "hl"

# Crop hydraulic length for each catchment
hl <- list()
for(id in catchments$id){
  crop <- st_crop(hl_region, catchments[catchments$id==id,])
  crop <- crop-min(crop$hl, na.rm = TRUE)
  crop$hl <- units::set_units(crop$hl, "m")
  hl[[id]] <- crop
}

```


```{r, echo=FALSE, message=FALSE, warning=TRUE, eval=running, results='hide'}
try_chunk <- try({
<<hydraulic_length>>
}, silent = TRUE)
if(inherits(try_chunk, "try-error")){
  warning("\nIssue when computing hydraulic length. \nThe vignette will not be fully built.")
  running <- FALSE
}
```

Resulting maps of hydraulic length can be plotted and checked.

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=running, results='hide', fig.width=7, fig.height=4}
i <- 1
network <- st_geometry(st_intersection(network_topage,catchments[i,]))
plot(hl[[i]], main = paste("Hydraulic length of catchment", i,"[m]"), 
     col = hcl.colors(20, palette = "Teal"), key.pos = 1, reset = FALSE)
plot(network, col = "white", lwd = 1.5, add = TRUE)
```


## 5. Creating a transfR object and running a simulation

Catchment delineations can be used as the spatial dimension of `stars` objects to georeference the observed flow time series of gauged catchments and locate ungauged catchments (see vignette *Preparation of input data: creation of a stars object* for details). Here we will create a `stars` object using the observed discharge of the `Blavet` dataset and the delineations that we just computed with `whitebox`.

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=running, results='hide'}
obs_st <- st_as_stars(list(Qobs = Blavet$obs$Qobs), 
                            dimensions = st_dimensions(
                              time = st_get_dimension_values(Blavet$obs,1),
                              space = st_geometry(catchments)))
```

The maps of hydraulic length can finally be used to create an object of class `transfR` by using the function `as_transfr()` (argument `hl`) and perform simulations.

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=running, results='hide'}
obs <- as_transfr(st = obs_st, hl = hl)
```

A transfer of hydrograph from the gauged catchments to the ungauged catchments can then quickly be implemented using the `quick_transfr()` function.

```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE}
obs <- quick_transfr(obs, velocity = "brittany2013", parallel = TRUE, cores = 2, cv = TRUE)
```

The simulated time series will be available in its stars object as new attributes.
```{r, echo=TRUE, message=FALSE, warning=FALSE, eval=FALSE}
obs$st
```

## References

<div id="refs"></div>

```{r, echo=FALSE, message=FALSE, warning=FALSE, eval=TRUE, results='hide'}
# Cleaning temporary directory
unlink(wbt_wd, recursive = TRUE)
```
