mediastreamer2 2.11.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

Howto 1: build a sample audio graph.
Introduction to mediastreamer2 concepts

# Initialize mediastreamer2

When using mediastreamer2, your first task is to initialize the library:

            #include <mediastreamer2/mscommon.h>

            int i;

            i=ms_init();
            if (i!=0)
              return -1;

Mediastreamer2 provides internal components which are called filters. Those filters must be linked together so that OUTPUT from one filter is sent to INPUT of the other filters.

Usually, filters are used for processing audio or video data. They could capture data, play/draw data, encode/decode data, mix data (conference), transform data (echo canceller). One of the most important filter is the RTP filters that are able to send and receive RTP data.

# Graph sample

If you are using mediastreamer2, you probably want to do Voice Over IP and get a graph providing a 2 way communication. This 2 graphs are very simple:

This first graph shows the filters needed to capture data from a sound card, encode them and send it through an RTP session.

                 AUDIO    ->    ENCODER   ->   RTP
                CAPTURE   ->              ->  SENDER

This second graph shows the filters needed to receive data from an RTP session decode it and send it to the playback device.

            RTP      ->    DECODER   ->   DTMF       ->   AUDIO
           RECEIVER  ->              ->  GENERATION  ->  PLAYBACK

# Code to initiate the filters of the Graph sample

Note that the NULL/error checks are not done for better reading. To build the graph, you'll need some information: you need to select the sound card and of course have an RTP session created with oRTP.

            MSSndCard *sndcard;
            sndcard=ms_snd_card_manager_get_default_card(ms_snd_card_manager_get());

            /* audio capture filter */
            MSFilter *soundread=ms_snd_card_create_reader(captcard);
            MSFilter *soundwrite=ms_snd_card_create_writer(playcard);

            MSFilter *encoder=ms_filter_create_encoder("PCMU");
            MSFilter *decoder=ms_filter_create_decoder("PCMU");

            MSFilter *rtpsend=ms_filter_new(MS_RTP_SEND_ID);
            MSFilter *rtprecv=ms_filter_new(MS_RTP_RECV_ID);

            RtpSession *rtp_session = *** your_ortp_session *** ;

            ms_filter_call_method(rtpsend,MS_RTP_SEND_SET_SESSION,rtp_session);
            ms_filter_call_method(rtprecv,MS_RTP_RECV_SET_SESSION,rtp_session);

            MSFilter *dtmfgen=ms_filter_new(MS_DTMF_GEN_ID);

In most cases, the above graph is not enough: you'll need to configure filter's options. As an example, you need to set sampling rate of sound cards' filters:

            int sr = 8000;
            int chan=1;
            ms_filter_call_method(soundread,MS_FILTER_SET_SAMPLE_RATE,&sr);
            ms_filter_call_method(soundwrite,MS_FILTER_SET_SAMPLE_RATE,&sr);
            ms_filter_call_method(stream->encoder,MS_FILTER_SET_SAMPLE_RATE,&sr);
            ms_filter_call_method(stream->decoder,MS_FILTER_SET_SAMPLE_RATE,&sr);

            ms_filter_call_method(soundwrite,MS_FILTER_SET_NCHANNELS, &chan);

            /* if you have some fmtp parameters (from SDP for example!) */
            char *fmtp1 = ** get your fmtp line **;
            char *fmtp2 = ** get your fmtp line **;
            ms_filter_call_method(stream->encoder,MS_FILTER_ADD_FMTP, (void*)fmtp1);
            ms_filter_call_method(stream->decoder,MS_FILTER_ADD_FMTP,(void*)fmtp2);

# Code to link the filters and run the graph sample

            ms_filter_link(stream->soundread,0,stream->encoder,0);
            ms_filter_link(stream->encoder,0,stream->rtpsend,0);

            ms_filter_link(stream->rtprecv,0,stream->decoder,0);
            ms_filter_link(stream->decoder,0,stream->dtmfgen,0);
            ms_filter_link(stream->dtmfgen,0,stream->soundwrite,0);

Then you need to 'attach' the filters to a ticker. A ticker is a graph manager responsible for running filters.

In the above case, there is 2 independant graph within the ticker: you need to attach the first element of each graph (the one that does not contains any INPUT pins)

            /* create ticker */
            MSTicker *ticker=ms_ticker_new();

            ms_ticker_attach(ticker,soundread);
            ms_ticker_attach(ticker,rtprecv);

# Code to unlink the filters and stop the graph sample

            ms_ticker_detach(ticker,soundread);
            ms_ticker_detach(ticker,rtprecv);

            ms_filter_unlink(stream->soundread,0,stream->encoder,0);
            ms_filter_unlink(stream->encoder,0,stream->rtpsend,0);

            ms_filter_unlink(stream->rtprecv,0,stream->decoder,0);
            ms_filter_unlink(stream->decoder,0,stream->dtmfgen,0);
            ms_filter_unlink(stream->dtmfgen,0,stream->soundwrite,0);

            if (rtp_session!=NULL) rtp_session_destroy(rtp_session);
            if (rtpsend!=NULL) ms_filter_destroy(rtpsend);
            if (rtprecv!=NULL) ms_filter_destroy(rtprecv);
            if (soundread!=NULL) ms_filter_destroy(soundread);
            if (soundwrite!=NULL) ms_filter_destroy(soundwrite);
            if (encoder!=NULL) ms_filter_destroy(encoder);
            if (decoder!=NULL) ms_filter_destroy(decoder);
            if (dtmfgen!=NULL) ms_filter_destroy(dtmfgen);
            if (ticker!=NULL) ms_ticker_destroy(ticker);