Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language | Libraries | Comparison | Changes

## tone()

#### Description

Generates a square wave of the specified frequency (and 50% duty cycle) on a pin. A duration can be specified, otherwise the wave continues until a call to noTone(). The pin can be connected to a piezo buzzer or other speaker to play tones.

Only one tone can be generated at a time. If a tone is already playing on a different pin, the call to tone() will have no effect. If the tone is playing on the same pin, the call will set its frequency.

Use of the tone() function will interfere with PWM output on pins 3 and 11 (on boards other than the Mega).

NOTE: if you want to play different pitches on multiple pins, you need to call noTone() on one pin before calling tone() on the next pin.

#### Syntax

tone(pin, frequency)
tone(pin, frequency, duration)

#### Parameters

pin: the pin on which to generate the tone

frequency: the frequency of the tone in hertz

duration: the duration of the tone in milliseconds (optional)

#### Returns

nothing

#### See also

- noTone()
- analogWrite()
- Tutorial:Tone
- Tutorial:Pitch follower
- Tutorial:Simple Keyboard
- Tutorial: multiple tones

- Tutorial: PWM

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
Edit Page | Page History | Printable View | All Recent Site Changes