Next: PowerPC Features, Previous: MIPS Features, Up: Standard Target Features

#### F.4.3 M68K Features

`````org.gnu.gdb.m68k.core`'`
`````org.gnu.gdb.coldfire.core`'`
`````org.gnu.gdb.fido.core`'`
  One of those features must be always present. The feature that is present determines which flavor of m68k is used. The feature that is present should contain registers ``d0`' through ``d7`', ``a0`' through ``a5`', ``fp`', ``sp`', ``ps`' and ``pc`'.
`````org.gnu.gdb.coldfire.fp`'`
  This feature is optional. If present, it should contain registers ``fp0`' through ``fp7`', ``fpcontrol`', ``fpstatus`' and ``fpiaddr`'.