Next: Part Definitions, Previous: AVRDUDE Defaults, Up: Configuration File

### 4.2 Programmer Definitions

The format of the programmer definition is as follows:

         programmer
             id     = <id1> [, <id2> [, <id3>] ...] ;  # <idN> are quoted strings
             desc     = <description> ;                  # quoted string
             type     = par | stk500 ;                   # programmer type
             baudrate = <num> ;                          # baudrate for serial ports
             vcc      = <num1> [, <num2> ... ] ;         # pin number(s)
             reset    = <num> ;                          # pin number
             sck      = <num> ;                          # pin number
             mosi     = <num> ;                          # pin number
             miso     = <num> ;                          # pin number
             errled   = <num> ;                          # pin number
             rdyled   = <num> ;                          # pin number
             pgmled   = <num> ;                          # pin number
             vfyled   = <num> ;                          # pin number
           ;