Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Serial

## available()

#### Description

Get the number of bytes (characters) available for reading from the serial port. This is data that's already arrived and stored in the serial receive buffer (which holds 128 bytes).

#### Syntax

Serial.available()

Arduino Mega only:
Serial1.available()
Serial2.available()
Serial3.available()

### Parameters

none

#### Returns

the number of bytes available to read

### Example

    int incomingByte = 0;	// for incoming serial data

    void setup() {
    	Serial.begin(9600);	// opens serial port, sets data rate to 9600 bps
    }

    void loop() {

    	// send data only when you receive data:
    	if (Serial.available() > 0) {
    		// read the incoming byte:
    		incomingByte = Serial.read();

    		// say what you got:
    		Serial.print("I received: ");
    		Serial.println(incomingByte, DEC);
    	}
    }

Arduino Mega example:

    void setup() {
      Serial.begin(9600);
      Serial1.begin(9600);

    }

    void loop() {
      // read from port 0, send to port 1:
      if (Serial.available()) {
        int inByte = Serial.read();
        Serial1.print(inByte, BYTE);

      }
      // read from port 1, send to port 0:
      if (Serial1.available()) {
        int inByte = Serial1.read();
        Serial.print(inByte, BYTE);
      }
    }

#### See also

- Serial.read()
- Serial.flush()

Reference Home

Share|
Edit Page | Page History | Printable View | All Recent Site Changes