AVR Libc Home Page |  | AVR Libc Development Pages
Main Page | User Manual | Library Reference | FAQ | Alphabetical Index | Example Projects

# Todo List

Group avr_boot
  From email with Marek: On smaller devices (all except ATmega64/128), __SPM_REG is in the I/O space, accessible with the shorter "in" and "out" instructions - since the boot loader has a limited size, this could be an important optimization.

Automatically generated by Doxygen 1.5.6 on 6 Jan 2010.