Next: Type Attributes, Previous: Character Escapes, Up: C Extensions

### 5.34 Specifying Attributes of Variables

The keyword `__attribute__` allows you to specify special attributes of variables or structure fields. This keyword is followed by an attribute specification inside double parentheses. Some attributes are currently defined generically for variables. Other attributes are defined for variables on particular target systems. Other attributes are available for functions (see Function Attributes) and for types (see Type Attributes). Other front ends might define more attributes (see Extensions to the C++ Language).

You may also specify attributes with __ preceding and following each keyword. This allows you to use them in header files without being concerned about a possible macro of the same name. For example, you may use `__aligned__` instead of `aligned`.

See Attribute Syntax, for details of the exact syntax for using attributes.

`aligned (`alignment`)`
  This attribute specifies a minimum alignment for the variable or structure field, measured in bytes. For example, the declaration:

                int x __attribute__ ((aligned (16))) = 0;

  causes the compiler to allocate the global variable `x` on a 16-byte boundary. On a 68040, this could be used in conjunction with an `asm` expression to access the `move16` instruction which requires 16-byte aligned operands.

  You can also specify the alignment of structure fields. For example, to create a double-word aligned `int` pair, you could write:

                struct foo { int x[2] __attribute__ ((aligned (8))); };

  This is an alternative to creating a union with a `double` member that forces the union to be double-word aligned.

  As in the preceding examples, you can explicitly specify the alignment (in bytes) that you wish the compiler to use for a given variable or structure field. Alternatively, you can leave out the alignment factor and just ask the compiler to align a variable or field to the maximum useful alignment for the target machine you are compiling for. For example, you could write:

                short array[3] __attribute__ ((aligned));

  Whenever you leave out the alignment factor in an `aligned` attribute specification, the compiler automatically sets the alignment for the declared variable or field to the largest alignment which is ever used for any data type on the target machine you are compiling for. Doing this can often make copy operations more efficient, because the compiler can use whatever instructions copy the biggest chunks of memory when performing copies to or from the variables or fields that you have aligned this way.

  When used on a struct, or struct member, the `aligned` attribute can only increase the alignment; in order to decrease it, the `packed` attribute must be specified as well. When used as part of a typedef, the `aligned` attribute can both increase and decrease alignment, and specifying the `packed` attribute will generate a warning.

  Note that the effectiveness of `aligned` attributes may be limited by inherent limitations in your linker. On many systems, the linker is only able to arrange for variables to be aligned up to a certain maximum alignment. (For some linkers, the maximum supported alignment may be very very small.) If your linker is only able to align variables up to a maximum of 8 byte alignment, then specifying `aligned(16)` in an `__attribute__` will still only provide you with 8 byte alignment. See your linker documentation for further information.

  The `aligned` attribute can also be used for functions (see Function Attributes.)

`cleanup (`cleanup_function`)`
  The `cleanup` attribute runs a function when the variable goes out of scope. This attribute can only be applied to auto function scope variables; it may not be applied to parameters or variables with static storage duration. The function must take one parameter, a pointer to a type compatible with the variable. The return value of the function (if any) is ignored.

  If -fexceptions is enabled, then cleanup_function will be run during the stack unwinding that happens during the processing of the exception. Note that the `cleanup` attribute does not allow the exception to be caught, only to perform an action. It is undefined what happens if cleanup_function does not return normally.

`common`
`nocommon`
  The `common` attribute requests GCC to place a variable in “common” storage. The `nocommon` attribute requests the opposite—to allocate space for it directly.

  These attributes override the default chosen by the -fno-common and -fcommon flags respectively.

`deprecated`
  The `deprecated` attribute results in a warning if the variable is used anywhere in the source file. This is useful when identifying variables that are expected to be removed in a future version of a program. The warning also includes the location of the declaration of the deprecated variable, to enable users to easily find further information about why the variable is deprecated, or what they should do instead. Note that the warning only occurs for uses:

                extern int old_var __attribute__ ((deprecated));
                extern int old_var;
                int new_fn () { return old_var; }

  results in a warning on line 3 but not line 2.

  The `deprecated` attribute can also be used for functions and types (see Function Attributes, see Type Attributes.)

`mode (`mode`)`
  This attribute specifies the data type for the declaration—whichever type corresponds to the mode mode. This in effect lets you request an integer or floating point type according to its width.

  You may also specify a mode of byte or __byte__ to indicate the mode corresponding to a one-byte integer, word or __word__ for the mode of a one-word integer, and pointer or __pointer__ for the mode used to represent pointers.

`packed`
  The `packed` attribute specifies that a variable or structure field should have the smallest possible alignment—one byte for a variable, and one bit for a field, unless you specify a larger value with the `aligned` attribute.

  Here is a structure in which the field `x` is packed, so that it immediately follows `a`:

                struct foo
                {
                  char a;
                  int x[2] __attribute__ ((packed));
                };

`section ("`section-name`")`
  Normally, the compiler places the objects it generates in sections like `data` and `bss`. Sometimes, however, you need additional sections, or you need certain particular variables to appear in special sections, for example to map to special hardware. The `section` attribute specifies that a variable (or function) lives in a particular section. For example, this small program uses several specific section names:

                struct duart a __attribute__ ((section ("DUART_A"))) = { 0 };
                struct duart b __attribute__ ((section ("DUART_B"))) = { 0 };
                char stack[10000] __attribute__ ((section ("STACK"))) = { 0 };
                int init_data __attribute__ ((section ("INITDATA"))) = 0;

                main()
                {
                  /* Initialize stack pointer */
                  init_sp (stack + sizeof (stack));

                  /* Initialize initialized data */
                  memcpy (&init_data, &data, &edata - &data);

                  /* Turn on the serial ports */
                  init_duart (&a);
                  init_duart (&b);
                }

  Use the `section` attribute with an initialized definition of a global variable, as shown in the example. GCC issues a warning and otherwise ignores the `section` attribute in uninitialized variable declarations.

  You may only use the `section` attribute with a fully initialized global definition because of the way linkers work. The linker requires each object be defined once, with the exception that uninitialized variables tentatively go in the `common` (or `bss`) section and can be multiply “defined”. You can force a variable to be initialized with the -fno-common flag or the `nocommon` attribute.

  Some file formats do not support arbitrary sections so the `section` attribute is not available on all platforms. If you need to map the entire contents of a module to a particular section, consider using the facilities of the linker instead.

`shared`
  On Microsoft Windows, in addition to putting variable definitions in a named section, the section can also be shared among all running copies of an executable or DLL. For example, this small program defines shared data by putting it in a named section `shared` and marking the section shareable:

                int foo __attribute__((section ("shared"), shared)) = 0;

                int
                main()
                {
                  /* Read and write foo.  All running
                     copies see the same value.  */
                  return 0;
                }

  You may only use the `shared` attribute along with `section` attribute with a fully initialized global definition because of the way linkers work. See `section` attribute for more information.

  The `shared` attribute is only available on Microsoft Windows.

`tls_model ("`tls_model`")`
  The `tls_model` attribute sets thread-local storage model (see Thread-Local) of a particular `__thread` variable, overriding -ftls-model= command line switch on a per-variable basis. The tls_model argument should be one of `global-dynamic`, `local-dynamic`, `initial-exec` or `local-exec`.

  Not all targets support this attribute.

`unused`
  This attribute, attached to a variable, means that the variable is meant to be possibly unused. GCC will not produce a warning for this variable.
`used`
  This attribute, attached to a variable, means that the variable must be emitted even if it appears that the variable is not referenced.
`vector_size (`bytes`)`
  This attribute specifies the vector size for the variable, measured in bytes. For example, the declaration:

                int foo __attribute__ ((vector_size (16)));

  causes the compiler to set the mode for `foo`, to be 16 bytes, divided into `int` sized units. Assuming a 32-bit int (a vector of 4 units of 4 bytes), the corresponding mode of `foo` will be V4SI.

  This attribute is only applicable to integral and float scalars, although arrays, pointers, and function return values are allowed in conjunction with this construct.

  Aggregates with this attribute are invalid, even if they are of the same size as a corresponding scalar. For example, the declaration:

                struct S { int a; };
                struct S  __attribute__ ((vector_size (16))) foo;

  is invalid even if the size of the structure is the same as the size of the `int`.

`selectany`
  The `selectany` attribute causes an initialized global variable to have link-once semantics. When multiple definitions of the variable are encountered by the linker, the first is selected and the remainder are discarded. Following usage by the Microsoft compiler, the linker is told not to warn about size or content differences of the multiple definitions.

  Although the primary usage of this attribute is for POD types, the attribute can also be applied to global C++ objects that are initialized by a constructor. In this case, the static initialization and destruction code for the object is emitted in each translation defining the object, but the calls to the constructor and destructor are protected by a link-once guard variable.

  The `selectany` attribute is only available on Microsoft Windows targets. You can use `__declspec (selectany)` as a synonym for `__attribute__ ((selectany))` for compatibility with other compilers.

`weak`
  The `weak` attribute is described in See Function Attributes.
`dllimport`
  The `dllimport` attribute is described in See Function Attributes.
`dllexport`
  The `dllexport` attribute is described in See Function Attributes.

#### 5.34.1 Blackfin Variable Attributes

Three attributes are currently defined for the Blackfin.

`l1_data`
`l1_data_A`
`l1_data_B`
  Use these attributes on the Blackfin to place the variable into L1 Data SRAM. Variables with `l1_data` attribute will be put into the specific section named `.l1.data`. Those with `l1_data_A` attribute will be put into the specific section named `.l1.data.A`. Those with `l1_data_B` attribute will be put into the specific section named `.l1.data.B`.

#### 5.34.2 M32R/D Variable Attributes

One attribute is currently defined for the M32R/D.

`model (`model-name`)`
  Use this attribute on the M32R/D to set the addressability of an object. The identifier model-name is one of `small`, `medium`, or `large`, representing each of the code models.

  Small model objects live in the lower 16MB of memory (so that their addresses can be loaded with the `ld24` instruction).

  Medium and large model objects may live anywhere in the 32-bit address space (the compiler will generate `seth/add3` instructions to load their addresses).

#### 5.34.3 i386 Variable Attributes

Two attributes are currently defined for i386 configurations: `ms_struct` and `gcc_struct`

`ms_struct`
`gcc_struct`
  If `packed` is used on a structure, or if bit-fields are used it may be that the Microsoft ABI packs them differently than GCC would normally pack them. Particularly when moving packed data between functions compiled with GCC and the native Microsoft compiler (either via function call or as data in a file), it may be necessary to access either format.

  Currently -m[no-]ms-bitfields is provided for the Microsoft Windows X86 compilers to match the native Microsoft compiler.

  The Microsoft structure layout algorithm is fairly simple with the exception of the bitfield packing:

  The padding and alignment of members of structures and whether a bit field can straddle a storage-unit boundary

  1. Structure members are stored sequentially in the order in which they are declared: the first member has the lowest memory address and the last member the highest.
  2. Every data object has an alignment-requirement. The alignment-requirement for all data except structures, unions, and arrays is either the size of the object or the current packing size (specified with either the aligned attribute or the pack pragma), whichever is less. For structures, unions, and arrays, the alignment-requirement is the largest alignment-requirement of its members. Every object is allocated an offset so that:

     offset % alignment-requirement == 0

  3. Adjacent bit fields are packed into the same 1-, 2-, or 4-byte allocation unit if the integral types are the same size and if the next bit field fits into the current allocation unit without crossing the boundary imposed by the common alignment requirements of the bit fields.

  Handling of zero-length bitfields:

  MSVC interprets zero-length bitfields in the following ways:

  1. If a zero-length bitfield is inserted between two bitfields that would normally be coalesced, the bitfields will not be coalesced.

     For example:

                        struct
                         {
                           unsigned long bf_1 : 12;
                           unsigned long : 0;
                           unsigned long bf_2 : 12;
                         } t1;

     The size of `t1` would be 8 bytes with the zero-length bitfield. If the zero-length bitfield were removed, `t1`'s size would be 4 bytes.

  2. If a zero-length bitfield is inserted after a bitfield, `foo`, and the alignment of the zero-length bitfield is greater than the member that follows it, `bar`, `bar` will be aligned as the type of the zero-length bitfield.

     For example:

                        struct
                         {
                           char foo : 4;
                           short : 0;
                           char bar;
                         } t2;

                        struct
                         {
                           char foo : 4;
                           short : 0;
                           double bar;
                         } t3;

     For `t2`, `bar` will be placed at offset 2, rather than offset 1. Accordingly, the size of `t2` will be 4. For `t3`, the zero-length bitfield will not affect the alignment of `bar` or, as a result, the size of the structure.

     Taking this into account, it is important to note the following:

     1. If a zero-length bitfield follows a normal bitfield, the type of the zero-length bitfield may affect the alignment of the structure as whole. For example, `t2` has a size of 4 bytes, since the zero-length bitfield follows a normal bitfield, and is of type short.
     2. Even if a zero-length bitfield is not followed by a normal bitfield, it may still affect the alignment of the structure:

                                struct
                                 {
                                   char foo : 6;
                                   long : 0;
                                 } t4;

        Here, `t4` will take up 4 bytes.

  3. Zero-length bitfields following non-bitfield members are ignored:

                        struct
                         {
                           char foo;
                           long : 0;
                           char bar;
                         } t5;

     Here, `t5` will take up 2 bytes.

#### 5.34.4 PowerPC Variable Attributes

Three attributes currently are defined for PowerPC configurations: `altivec`, `ms_struct` and `gcc_struct`.

For full documentation of the struct attributes please see the documentation in the See i386 Variable Attributes, section.

For documentation of `altivec` attribute please see the documentation in the See PowerPC Type Attributes, section.

#### 5.34.5 SPU Variable Attributes

The SPU supports the `spu_vector` attribute for variables. For documentation of this attribute please see the documentation in the See SPU Type Attributes, section.

#### 5.34.6 Xstormy16 Variable Attributes

One attribute is currently defined for xstormy16 configurations: `below100`

`below100`
  If a variable has the `below100` attribute (`BELOW100` is allowed also), GCC will place the variable in the first 0x100 bytes of memory and use special opcodes to access it. Such variables will be placed in either the `.bss_below100` section or the `.data_below100` section.

#### 5.34.7 AVR32 Variable Attributes

One attribute is currently defined for AVR32 configurations: `rmw_addressable`

`rmw_addressable`
  This attribute can be used to signal that a variable can be accessed with the addressing mode of the AVR32 Atomic Read-Modify-Write memory instructions and hence make it possible for gcc to generate these instructions without using built-in functions or inline assembly statements. Variables used within the AVR32 Atomic Read-Modify-Write built-in functions will automatically get the `rmw_addressable` attribute.

#### 5.34.8 AVR Variable Attributes

`progmem`
  The `progmem` attribute is used on the AVR to place data in the Program Memory address space. The AVR is a Harvard Architecture processor and data normally resides in the Data Memory address space.