Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language | Libraries | Comparison | Changes

## constrain(x, a, b)

#### Description

Constrains a number to be within a range.

#### Parameters

x: the number to constrain, all data types

a: the lower end of the range, all data types

b: the upper end of the range, all data types

#### Returns

x: if x is between a and b

a: if x is less than a

b: if x is greater than b

#### Example

    sensVal = constrain(sensVal, 10, 150);
    // limits range of sensor values to between 10 and 150

#### See also

- min()
- max()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
Edit Page | Page History | Printable View | All Recent Site Changes