Next: i386-Regs, Previous: i386-Syntax, Up: i386-Dependent

#### 9.14.4 Instruction Naming

Instruction mnemonics are suffixed with one character modifiers which specify the size of operands. The letters b, w, l and q specify byte, word, long and quadruple word operands. If no suffix is specified by an instruction then `as` tries to fill in the missing suffix based on the destination register operand (the last one by convention). Thus, mov %ax, %bx is equivalent to movw %ax, %bx; also, mov $1, %bx is equivalent to movw $1, bx. Note that this is incompatible with the AT&T Unix assembler which assumes that a missing mnemonic suffix implies long operand size. (This incompatibility does not affect compiler output since compilers always explicitly specify the mnemonic suffix.)

Almost all instructions have the same names in AT&T and Intel format. There are a few exceptions. The sign extend and zero extend instructions need two sizes to specify them. They need a size to sign/zero extend from and a size to zero extend to. This is accomplished by using two instruction mnemonic suffixes in AT&T syntax. Base names for sign extend and zero extend are movs... and movz... in AT&T syntax (movsx and movzx in Intel syntax). The instruction mnemonic suffixes are tacked on to this base name, the from suffix before the to suffix. Thus, movsbl %al, %edx is AT&T syntax for “move sign extend from %al to %edx.” Possible suffixes, thus, are bl (from byte to long), bw (from byte to word), wl (from word to long), bq (from byte to quadruple word), wq (from word to quadruple word), and lq (from long to quadruple word).

The Intel-syntax conversion instructions

- cbw — sign-extend byte in %al to word in %ax,
- cwde — sign-extend word in %ax to long in %eax,
- cwd — sign-extend word in %ax to long in %dx:%ax,
- cdq — sign-extend dword in %eax to quad in %edx:%eax,
- cdqe — sign-extend dword in %eax to quad in %rax (x86-64 only),
- cqo — sign-extend quad in %rax to octuple in %rdx:%rax (x86-64 only),

are called cbtw, cwtl, cwtd, cltd, cltq, and cqto in AT&T naming. `as` accepts either naming for these instructions.

Far call/jump instructions are lcall and ljmp in AT&T syntax, but are call far and jump far in Intel convention.

#### 9.14.5 AT&T Mnemonic versus Intel Mnemonic

`as` supports assembly using Intel mnemonic. `.intel_mnemonic` selects Intel mnemonic with Intel syntax, and `.att_mnemonic` switches back to the usual AT&T mnemonic with AT&T syntax for compatibility with the output of `gcc`. Several x87 instructions, fadd, fdiv, fdivp, fdivr, fdivrp, fmul, fsub, fsubp, fsubr and fsubrp, are implemented in AT&T System V/386 assembler with different mnemonics from those in Intel IA32 specification. `gcc` generates those instructions with AT&T mnemonic.