Next: Other Notes, Previous: Programmer Definitions, Up: Configuration File

### 4.3 Part Definitions

         part
             id               = <id> ;                 # quoted string
             desc             = <description> ;        # quoted string
             devicecode       = <num> ;                # numeric
             chip_erase_delay = <num> ;                # micro-seconds
             pagel            = <num> ;                # pin name in hex, i.e., 0xD7
             bs2              = <num> ;                # pin name in hex, i.e., 0xA0
             reset            = dedicated | io;
             retry_pulse      = reset | sck;
             pgm_enable       = <instruction format> ;
             chip_erase       = <instruction format> ;
             memory <memtype>
                 paged           = <yes/no> ;          # yes / no
                 size            = <num> ;             # bytes
                 page_size       = <num> ;             # bytes
                 num_pages       = <num> ;             # numeric
                 min_write_delay = <num> ;             # micro-seconds
                 max_write_delay = <num> ;             # micro-seconds
                 readback_p1     = <num> ;             # byte value
                 readback_p2     = <num> ;             # byte value
                 pwroff_after_write = <yes/no> ;       # yes / no
                 read            = <instruction format> ;
                 write           = <instruction format> ;
                 read_lo         = <instruction format> ;
                 read_hi         = <instruction format> ;
                 write_lo        = <instruction format> ;
                 write_hi        = <instruction format> ;
                 loadpage_lo     = <instruction format> ;
                 loadpage_hi     = <instruction format> ;
                 writepage       = <instruction format> ;
               ;
           ;