Next: D30V-Addressing, Previous: D30V-Guarded, Up: D30V-Syntax

##### 9.10.2.5 Register Names

You can use the predefined symbols r0 through r63 to refer to the D30V registers. You can also use sp as an alias for r63 and link as an alias for r62. The accumulators are a0 and a1.

The D30V also has predefined symbols for these control registers and status bits:

`psw`
  Processor Status Word
`bpsw`
  Backup Processor Status Word
`pc`
  Program Counter
`bpc`
  Backup Program Counter
`rpt_c`
  Repeat Count
`rpt_s`
  Repeat Start address
`rpt_e`
  Repeat End address
`mod_s`
  Modulo Start address
`mod_e`
  Modulo End address
`iba`
  Instruction Break Address
`f0`
  Flag 0
`f1`
  Flag 1
`f2`
  Flag 2
`f3`
  Flag 3
`f4`
  Flag 4
`f5`
  Flag 5
`f6`
  Flag 6
`f7`
  Flag 7
`s`
  Same as flag 4 (saturation flag)
`v`
  Same as flag 5 (overflow flag)
`va`
  Same as flag 6 (sticky overflow flag)
`c`
  Same as flag 7 (carry/borrow flag)
`b`
  Same as flag 7 (carry/borrow flag)