Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language | Libraries | Comparison | Changes

## break

break is used to exit from a do, for, or while loop, bypassing the normal loop condition. It is also used to exit from a switch statement.

#### Example

    for (x = 0; x < 255; x ++)
    {
        digitalWrite(PWMpin, x);
        sens = analogRead(sensorPin);
        if (sens > threshold){      // bail out on sensor detect
           x = 0;
           break;
        }
        delay(50);
    }

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
Edit Page | Page History | Printable View | All Recent Site Changes