This is avrdude.info, produced by makeinfo version 4.7 from
avrdude.texi.

INFO-DIR-SECTION AVR Programming & development tools.
START-INFO-DIR-ENTRY
* AvrDude: (avrdude).            AVR program downloader/uploader.
END-INFO-DIR-ENTRY

   This file documents the avrdude program.

   For avrdude version 5.8cvs, 8 January 2010.

   Copyright (C) 2003, 2005 Brian Dean

   Copyright (C) 2006 - 2009 Jo"rg Wunsch

   Permission is granted to make and distribute verbatim copies of this
manual provided the copyright notice and this permission notice are
preserved on all copies.

   Permission is granted to copy and distribute modified versions of
this manual under the conditions for verbatim copying, provided that
the entire resulting derived work is distributed under the terms of a
permission notice identical to this one.

   Permission is granted to copy and distribute translations of this
manual into another language, under the above conditions for modified
versions, except that this permission notice may be stated in a
translation approved by the Free Software Foundation.


File: avrdude.info,  Node: Top,  Next: Introduction,  Prev: (dir),  Up: (dir)

   This file documents the avrdude program for downloading/uploading
programs to Atmel AVR microcontrollers.

   For avrdude version 5.8cvs, 8 January 2010.

   Send comments on AVRDUDE to <avrdude-dev@nongnu.org>.

   Use `http://savannah.nongnu.org/bugs/?group=avrdude' to report bugs.

   Copyright (C) 2003,2005 Brian S. Dean

   Copyright (C) 2006 Jo"rg Wunsch

* Menu:

* Introduction::
* Command Line Options::
* Terminal Mode Operation::
* Configuration File::
* Programmer Specific Information::
* Platform Dependent Information::
* Troubleshooting::


File: avrdude.info,  Node: Introduction,  Next: Command Line Options,  Prev: Top,  Up: Top

1 Introduction
**************

AVRDUDE - AVR Downloader Uploader - is a program for downloading and
uploading the on-chip memories of Atmel's AVR microcontrollers. It can
program the Flash and EEPROM, and where supported by the serial
programming protocol, it can program fuse and lock bits. AVRDUDE also
supplies a direct instruction mode allowing one to issue any programming
instruction to the AVR chip regardless of whether AVRDUDE implements
that specific feature of a particular chip.

   AVRDUDE can be used effectively via the command line to read or write
all chip memory types (eeprom, flash, fuse bits, lock bits, signature
bytes) or via an interactive (terminal) mode. Using AVRDUDE from the
command line works well for programming the entire memory of the chip
from the contents of a file, while interactive mode is useful for
exploring memory contents, modifing individual bytes of eeprom,
programming fuse/lock bits, etc.

   AVRDUDE supports the following basic programmer types: Atmel's
STK500, Atmel's AVRISP and AVRISP mkII devices, Atmel's STK600, Atmel's
JTAG ICE (both mkI and mkII, the latter also in ISP mode), appnote
avr910, appnote avr109 (including the AVR Butterfly), serial bit-bang
adapters, and the PPI (parallel port interface). PPI represents a class
of simple programmers where the programming lines are directly
connected to the PC parallel port. Several pin configurations exist for
several variations of the PPI programmers, and AVRDUDE can be be
configured to work with them by either specifying the appropriate
programmer on the command line or by creating a new entry in its
configuration file. All that's usually required for a new entry is to
tell AVRDUDE which pins to use for each programming function.

   A number of equally simple bit-bang programming adapters that connect
to a serial port are supported as well, among them the popular Ponyprog
serial adapter, and the DASA and DASA3 adapters that used to be
supported by uisp(1).  Note that these adapters are meant to be
attached to a physical serial port.  Connecting to a serial port
emulated on top of USB is likely to not work at all, or to work
abysmally slow.

   The STK500, JTAG ICE, avr910, and avr109/butterfly use the serial
port to communicate with the PC.  The STK600, JTAG ICE mkII, AVRISP
mkII, USBasp, and USBtinyISP programmers communicate through the USB,
using `libusb' as a platform abstraction layer.  The STK500, STK600,
JTAG ICE, and avr910 contain on-board logic to control the programming
of the target device.  The avr109 bootloader implements a protocol
similar to avr910, but is actually implemented in the boot area of the
target's flash ROM, as opposed to being an external device.  The
fundamental difference between the two types lies in the protocol used
to control the programmer. The avr910 protocol is very simplistic and
can easily be used as the basis for a simple, home made programer since
the firmware is available online. On the other hand, the STK500
protocol is more robust and complicated and the firmware is not openly
available.  The JTAG ICE also uses a serial communication protocol
which is similar to the STK500 firmware version 2 one.  However, as the
JTAG ICE is intented to allow on-chip debugging as well as memory
programming, the protocol is more sophisticated.  (The JTAG ICE mkII
protocol can also be run on top of USB.)  Only the memory programming
functionality of the JTAG ICE is supported by AVRDUDE.  For the JTAG
ICE mkII, JTAG, debugWire and ISP mode are supported.  See below for
the limitations of debugWire.

   The Arduino (which is very similar to the STK500 1.x) is supported
via its own programmer type specification "arduino".

   The AVR Dragon is supported in all modes (ISP, JTAG, HVSP, PP,
debugWire).  When used in JTAG and debugWire mode, the AVR Dragon
behaves similar to a JTAG ICE mkII, so all device-specific comments for
that device will apply as well.  When used in ISP mode, the AVR Dragon
behaves similar to an AVRISP mkII (or JTAG ICE mkII in ISP mode), so
all device-specific comments will apply there.  In particular, the
Dragon starts out with a rather fast ISP clock frequency, so the `-B
BITCLOCK' option might be required to achieve a stable ISP
communication.

   The USBasp ISP and USBtinyISP adapters are also supported, provided
AVRDUDE has been compiled with libusb support.  They both feature
simple firwmare-only USB implementations, running on an ATmega8 (or
ATmega88), or ATtiny2313, respectively.

* Menu:

* History::


File: avrdude.info,  Node: History,  Prev: Introduction,  Up: Introduction

1.1 History and Credits
=======================

AVRDUDE was written by Brian S. Dean under the name of AVRPROG to run on
the FreeBSD Operating System.  Brian renamed the software to be called
AVRDUDE when interest grew in a Windows port of the software so that the
name did not conflict with AVRPROG.EXE which is the name of Atmel's
Windows programming software.

   The AVRDUDE source now resides in the public CVS repository on
savannah.gnu.org (`http://savannah.gnu.org/projects/avrdude/'), where
it continues to be enhanced and ported to other systems.  In addition
to FreeBSD, AVRDUDE now runs on Linux and Windows.  The developers
behind the porting effort primarily were Ted Roth, Eric Weddington, and
Joerg Wunsch.

   And in the spirit of many open source projects, this manual also
draws on the work of others.  The initial revision was composed of
parts of the original Unix manual page written by Joerg Wunsch, the
original web site documentation by Brian Dean, and from the comments
describing the fields in the AVRDUDE configuration file by Brian Dean.
The texi formatting was modeled after that of the Simulavr
documentation by Ted Roth.


File: avrdude.info,  Node: Command Line Options,  Next: Terminal Mode Operation,  Prev: Introduction,  Up: Top

2 Command Line Options
**********************

* Menu:

* Option Descriptions::
* Programmers accepting extended parameters::
* Example Command Line Invocations::


File: avrdude.info,  Node: Option Descriptions,  Next: Programmers accepting extended parameters,  Prev: Command Line Options,  Up: Command Line Options

2.1 Option Descriptions
=======================

AVRDUDE is a command line tool, used as follows:

     avrdude -p partno OPTIONS ...

Command line options are used to control AVRDUDE's behaviour.  The
following options are recognized:

`-p PARTNO'
     This is the only mandatory option and it tells AVRDUDE what type
     of part (MCU) that is connected to the programmer.  The PARTNO
     parameter is the part's id listed in the configuration file.
     Specify -p ? to list all parts in the configuration file.  If a
     part is unknown to AVRDUDE, it means that there is no config file
     entry for that part, but it can be added to the configuration file
     if you have the Atmel datasheet so that you can enter the
     programming specifications.  Currently, the following MCU types
     are understood:

     `c128'     AT90CAN128
     `pwm2'     AT90PWM2
     `pwm3'     AT90PWM3
     `1200'     AT90S1200
     `2313'     AT90S2313
     `2333'     AT90S2333
     `2343'     AT90S2343 (*)
     `4414'     AT90S4414
     `4433'     AT90S4433
     `4434'     AT90S4434
     `8515'     AT90S8515
     `8535'     AT90S8535
     `m103'     ATmega103
     `m128'     ATmega128
     `m1280'    ATmega1280
     `m1281'    ATmega1281
     `m1284p'   ATmega1284P
     `m128rfa1' ATmega128RFA1
     `m16'      ATmega16
     `m161'     ATmega161
     `m162'     ATmega162
     `m163'     ATmega163
     `m164'     ATmega164
     `m169'     ATmega169
     `m2560'    ATmega2560 (**)
     `m2561'    ATmega2561 (**)
     `m32'      ATmega32
     `m324'     ATmega324
     `m329'     ATmega329
     `m3290'    ATmega3290
     `m48'      ATmega48
     `m64'      ATmega64
     `m640'     ATmega640
     `m644'     ATmega644
     `m649'     ATmega649
     `m6490'    ATmega6490
     `m8'       ATmega8
     `m8515'    ATmega8515
     `m8535'    ATmega8535
     `m88'      ATmega88
     `t12'      ATtiny12
     `t13'      ATtiny13
     `t15'      ATtiny15
     `t2313'    ATtiny2313
     `t25'      ATtiny25
     `t26'      ATtiny26
     `t45'      ATtiny45
     `t85'      ATtiny85
     `x128a1'   ATxmega128A1
     `x128a1d'  ATxmega128A1revD

     (*)   The AT90S2323 and ATtiny22 use the same algorithm.

     (**)  Flash addressing above 128 KB is not supported by all
     programming hardware.  Known to work are jtag2, stk500v2, and
     bit-bang programmers.

`-b BAUDRATE'
     Override the RS-232 connection baud rate specified in the
     respective programmer's entry of the configuration file.

`-B BITCLOCK'
     Specify the bit clock period for the JTAG interface or the ISP
     clock (JTAG ICE only).  The value is a floating-point number in
     microseconds.  The default value of the JTAG ICE results in about
     1 microsecond bit clock period, suitable for target MCUs running
     at 4 MHz clock and above.  Unlike certain parameters in the
     STK500, the JTAG ICE resets all its parameters to default values
     when the programming software signs off from the ICE, so for MCUs
     running at lower clock speeds, this parameter must be specified on
     the command-line.

`-c PROGRAMMER-ID'
     Specify the programmer to be used.  AVRDUDE knows about several
     common programmers.  Use this option to specify which one to use.
     The PROGRAMMER-ID parameter is the programmer's id listed in the
     configuration file.  Specify -c ? to list all programmers in the
     configuration file.  If you have a programmer that is unknown to
     AVRDUDE, and the programmer is controlled via the PC parallel port,
     there's a good chance that it can be easily added to the
     configuration file without any code changes to AVRDUDE.  Simply
     copy an existing entry and change the pin definitions to match
     that of the unknown programmer.  Currently, the following
     programmer ids are understood and supported:

     `abcmini'      ABCmini Board, aka Dick Smith HOTCHIP
     `alf'          Nightshade ALF-PgmAVR,
                   `http://nightshade.homeip.net/'
     `arduino'     
     Arduino       
     board,        
     protocol      
     similar to    
     STK500 1.x    
     `atisp'        AT-ISP V1.1 programming cable for
                   AVR-SDK1 from,
                   `http://micro-research.co.th/'
     `avr109'       Atmel AppNote AVR109 Boot Loader
     `avr910'       Atmel Low Cost Serial Programmer
     `avr911'       Atmel AppNote AVR911 AVROSP (an alias
                   for avr109)
     `avrisp'       Atmel AVR ISP (an alias for stk500)
     `avrisp2'      Atmel AVR ISP mkII (alias for stk500v2)
     `avrispmkII'   Atmel AVR ISP mkII (alias for stk500v2)
     `avrispv2'     Atmel AVR ISP, running a version 2.x
                   firmware (an alias for stk500v2)
     `bascom'       Bascom SAMPLE programming cable
     `blaster'      Altera ByteBlaster
     `bsd'          Brian Dean's Programmer,
                   `http://www.bsdhome.com/avrdude/'
     `butterfly'    Atmel Butterfly Development Board
     `c2n232i'      C2N232I, reset=dtr sck=!rts mosi=!txd
                   miso=!cts,
                   `http://www.ktverkko.fi/~msmakela/8bit/c2n232/hardware/index.en.html'
     `dapa'         Direct AVR Parallel Access cable
     `dasa'         serial port banging, reset=rts sck=dtr
                   mosi=txd miso=cts
     `dasa3'        serial port banging, reset=!dtr
                   sck=rts mosi=txd miso=cts
     `dragon_dw'    AVR Dragon in debugWire mode
     `dragon_hvsp'  AVR Dragon in high-voltage serial
                   programming mode
     `dragon_isp'   AVR Dragon in ISP mode
     `dragon_jtag'  AVR Dragon in JTAG mode
     `dragon_pp'    AVR Dragon in (high-voltage) parallel
                   programming mode
     `dt006'        Dontronics DT006
     `ere-isp-avr'  ERE ISP-AVR,
                   `http://www.ere.co.th/download/sch050713.pdf'
     `frank-stk200' Frank's STK200 clone,
                   `http://electropol.free.fr/spip/spip.php?article15'
     `futurlec'     Futurlec.com programming cable
     `jtag1'        Atmel JTAG ICE mkI, running at 115200
                   Bd
     `jtag1slow'    Atmel JTAG ICE mkI, running at 19200 Bd
     `jtag2slow'    Atmel JTAG ICE mkII (default speed
                   19200 Bd)
     `jtag2'        Atmel JTAG ICE mkII, running at 115200
                   Bd
     `jtag2fast'    Atmel JTAG ICE mkII, running at 115200
                   Bd
     `jtag2isp'     Atmel JTAG ICE mkII in ISP mode.
     `jtag2dw'      Atmel JTAG ICE mkII in debugWire mode.
     `jtagmkI'      Atmel JTAG ICE mkI, running at 115200
                   Bd
     `jtagmkII'     Atmel JTAG ICE mkII (default speed
                   19200 Bd)
     `mib510'       Crossbow MIB510 programming board
     `pavr'         Jason Kyle's pAVR Serial Programmer
     `picoweb'      Picoweb Programming Cable,
                   `http://www.picoweb.net/'
     `pony-stk200'  Pony Prog STK200
     `ponyser'      design ponyprog serial, reset=!txd
                   sck=rts mosi=dtr miso=cts
     `siprog'       Lancos SI-Prog,
                   `http://www.lancos.com/siprogsch.html'
     `sp12'         Steve Bolt's Programmer
     `stk200'       STK200
     `stk500'       Atmel STK500, probing for either
                   version 1.x or 2.x firmware
     `stk500hvsp'   Atmel STK500 in high-voltage serial
                   programming mode(version 2.x firmware
                   only)
     `stk500pp'     Atmel STK500 in parallel programming
                   mode (version 2.xfirmware only)
     `stk500v1'     Atmel STK500, running a version 1.x
                   firmware
     `stk500v2'     Atmel STK500, running a version 2.x
                   firmware
     `stk600'       Atmel STK600 in ISP mode, or in PDI
                   mode for ATxmega devices
     `stk600hvsp'   Atmel STK600 in high-voltage serial
                   programming mode
     `stk600pp'     Atmel STK600 in parallel programming
                   mode
     `usbasp'       USBasp,
                   `http://www.fischl.de/usbasp/'
     `usbtiny'      USBtiny simple USB programmer,
                   `http://www.ladyada.net/make/usbtinyisp/'
     `xil'          Xilinx JTAG cable

`-C CONFIG-FILE'
     Use the specified config file for configuration data.  This file
     contains all programmer and part definitions that AVRDUDE knows
     about.  If you have a programmer or part that AVRDUDE does not
     know about, you can add it to the config file (be sure and submit
     a patch back to the author so that it can be incorporated for the
     next version).  If not specified, AVRDUDE reads the configuration
     file from /usr/local/etc/avrdude.conf (FreeBSD and Linux). See
     Appendix A for the method of searching for the configuration file
     for Windows.

`-D'
     Disable auto erase for flash.  When the -U option with flash
     memory is specified, avrdude will perform a chip erase before
     starting any of the programming operations, since it generally is
     a mistake to program the flash without performing an erase first.
     This option disables that.  Auto erase is not used for ATxmega
     devices as these devices can use page erase before writing each
     page so no explicit chip erase is required.  Note however that any
     page not affected by the current operation will retain its
     previous contents.

`-e'
     Causes a chip erase to be executed.  This will reset the contents
     of the flash ROM and EEPROM to the value `0xff', and clear all
     lock bits.  Except for ATxmega devices which can use page erase,
     it is basically a prerequisite command before the flash ROM can be
     reprogrammed again.  The only exception would be if the new
     contents would exclusively cause bits to be programmed from the
     value `1' to `0'.  Note that in order to reprogram EERPOM cells,
     no explicit prior chip erase is required since the MCU provides an
     auto-erase cycle in that case before programming the cell.

`-E EXITSPEC[,...]'
     By default, AVRDUDE leaves the parallel port in the same state at
     exit as it has been found at startup.  This option modifies the
     state of the `/RESET' and `Vcc' lines the parallel port is left
     at, according to the exitspec arguments provided, as follows:

    `reset'
          The `/RESET' signal will be left activated at program exit,
          that is it will be held low, in order to keep the MCU in
          reset state afterwards.  Note in particular that the
          programming algorithm for the AT90S1200 device mandates that
          the `/RESET' signal is active before powering up the MCU, so
          in case an external power supply is used for this MCU type, a
          previous invocation of AVRDUDE with this option specified is
          one of the possible ways to guarantee this condition.

    `noreset'
          The `/RESET' line will be deactivated at program exit, thus
          allowing the MCU target program to run while the programming
          hardware remains connected.

    `vcc'
          This option will leave those parallel port pins active (i. e.
          high) that can be used to supply `Vcc' power to the MCU.

    `novcc'
          This option will pull the `Vcc' pins of the parallel port
          down at program exit.


     Multiple EXITSPEC arguments can be separated with commas.

`-F'
     Normally, AVRDUDE tries to verify that the device signature read
     from the part is reasonable before continuing.  Since it can
     happen from time to time that a device has a broken (erased or
     overwritten) device signature but is otherwise operating normally,
     this options is provided to override the check.  Also, for
     programmers like the Atmel STK500 and STK600 which can adjust
     parameters local to the programming tool (independent of an actual
     connection to a target controller), this option can be used
     together with `-t' to continue in terminal mode.

`-i DELAY'
     For bitbang-type programmers, delay for approximately DELAY
     microseconds between each bit state change.  If the host system is
     very fast, or the target runs off a slow clock (like a 32 kHz
     crystal, or the 128 kHz internal RC oscillator), this can become
     necessary to satisfy the requirement that the ISP clock frequency
     must not be higher than 1/4 of the CPU clock frequency.  This is
     implemented as a spin-loop delay to allow even for very short
     delays.  On Unix-style operating systems, the spin loop is
     initially calibrated against a system timer, so the number of
     microseconds might be rather realistic, assuming a constant system
     load while AVRDUDE is running.  On Win32 operating systems, a
     preconfigured number of cycles per microsecond is assumed that
     might be off a bit for very fast or very slow machines.

`-n'
     No-write - disables actually writing data to the MCU (useful for
     debugging AVRDUDE).

`-O'
     Perform a RC oscillator run-time calibration according to Atmel
     application note AVR053.  This is only supported on the STK500v2,
     AVRISP mkII, and JTAG ICE mkII hardware.  Note that the result
     will be stored in the EEPROM cell at address 0.

`-P PORT'
     Use port to identify the device to which the programmer is
     attached.  Normally, the default parallel port is used, but if the
     programmer type normally connects to the serial port, the default
     serial port will be used. See Appendix A, Platform Dependent
     Information, to find out the default port names for your platform.
     If you need to use a different parallel or serial port, use this
     option to specify the alternate port name.

     On Win32 operating systems, the parallel ports are referred to as
     lpt1 through lpt3, referring to the addresses 0x378, 0x278, and
     0x3BC, respectively.  If the parallel port can be accessed through
     a different address, this address can be specified directly, using
     the common C language notation (i. e., hexadecimal values are
     prefixed by 0X).

     For the JTAG ICE mkII, if AVRDUDE has been built with libusb
     support, PORT may alternatively be specified as `usb'[:SERIALNO].
     In that case, the JTAG ICE mkII will be looked up on USB.  If
     SERIALNO is also specified, it will be matched against the serial
     number read from any JTAG ICE mkII found on USB.  The match is
     done after stripping any existing colons from the given serial
     number, and right-to-left, so only the least significant bytes
     from the serial number need to be given.  For a trick how to find
     out the serial numbers of all JTAG ICEs attached to USB, see *Note
     Example Command Line Invocations::.

     As the AVRISP mkII device can only be talked to over USB, the very
     same method of specifying the port is required there.

     For the USB programmer "AVR-Doper" running in HID mode, the port
     must be specified as AVRDOPER. Libusb support is required on Unix
     but not on Windows. For more information about AVR-Doper see
     `http://www.obdev.at/avrusb/avrdoper.html'.

     For programmers that attach to a serial port using some kind of
     higher level protocol (as opposed to bit-bang style programmers),
     PORT can be specified as `net':HOST:PORT.  In this case, instead
     of trying to open a local device, a TCP network connection to
     (TCP) PORT on HOST is established.  The remote endpoint is assumed
     to be a terminal or console server that connects the network
     stream to a local serial port where the actual programmer has been
     attached to.  The port is assumed to be properly configured, for
     example using a transparent 8-bit data connection without parity
     at 115200 Baud for a STK500.

     _This feature is currently not implemented for Win32 systems._

`-q'
     Disable (or quell) output of the progress bar while reading or
     writing to the device.  Specify it a second time for even quieter
     operation.

`-u'
     Disables the default behaviour of reading out the fuses three
     times before programming, then verifying at the end of programming
     that the fuses have not changed. If you want to change fuses you
     will need to specify this option, as avrdude will see the fuses
     have changed (even though you wanted to) and will change them back
     for your "saftey". This option was designed to prevent cases of
     fuse bits magically changing (usually called _safemode_).

`-t'
     Tells AVRDUDE to enter the interactive "terminal" mode instead of
     up- or downloading files.  See below for a detailed description of
     the terminal mode.

`-U MEMTYPE:OP:FILENAME[:FORMAT]'
     Perform a memory operation, equivalent to specifing the `-m', `-i'
     or `-o', and `-f' options, except that multiple `-U' optins can be
     specified in order to operate on mulitple memories on the same
     command-line invocation.  The MEMTYPE field specifies the memory
     type to operate on. Use the `-v' option on the command line or the
     `part' command from terminal mode to display all the memory types
     supported by a particular device.  Typically, a device's memory
     configuration at least contains the memory types `flash' and
     `eeprom'.  All memory types currently known are:
    `calibration'
          One or more bytes of RC oscillator calibration data.

    `eeprom'
          The EEPROM of the device.

    `efuse'
          The extended fuse byte.

    `flash'
          The flash ROM of the device.

    `fuse'
          The fuse byte in devices that have only a single fuse byte.

    `hfuse'
          The high fuse byte.

    `lfuse'
          The low fuse byte.

    `lock'
          The lock byte.

    `signature'
          The three device signature bytes (device ID).

     The OP field specifies what operation to perform:

    `r'
          read the specified device memory and write to the specified
          file

    `w'
          read the specified file and write it to the specified device
          memory

    `v'
          read the specified device memory and the specified file and
          perform a verify operation


     The FILENAME field indicates the name of the file to read or
     write.  The FORMAT field is optional and contains the format of
     the file to read or write.  Possible values are:

    `i'
          Intel Hex

    `s'
          Motorola S-record

    `r'
          raw binary; little-endian byte order, in the case of the
          flash ROM data

    `m'
          immediate mode; actual byte values specified on the command
          line, seperated by commas or spaces in place of the FILENAME
          field of the `-i', `-o', or `-U' options.  This is useful for
          programming fuse bytes without having to create a single-byte
          file or enter terminal mode.  If the number specified begins
          with `0x', it is treated as a hex value.  If the number
          otherwise begins with a leading zero (`0') it is treated as
          octal.  Otherwise, the value is treated as decimal.

    `a'
          auto detect; valid for input only, and only if the input is
          not provided at stdin.

    `d'
          decimal; this and the following formats are only valid on
          output.  They generate one line of output for the respective
          memory section, forming a comma-separated list of the values.
          This can be particularly useful for subsequent processing,
          like for fuse bit settings.

    `h'
          hexadecimal; each value will get the string _0x_ prepended.

    `o'
          octal; each value will get a _0_ prepended unless it is less
          than 8 in which case it gets no prefix.

    `b'
          binary; each value will get the string _0b_ prepended.


     The default is to use auto detection for input files, and raw
     binary format for output files.

     Note that if FILENAME contains a colon, the FORMAT field is no
     longer optional since the filename part following the colon would
     otherwise be misinterpreted as FORMAT.

     As an abbreviation, the form `-U' FILENAME is equivalent to
     specifying `-U' _flash:w:_FILENAME_:a_.  This will only work if
     FILENAME does not have a colon in it.

`-v'
     Enable verbose output.

`-V'
     Disable automatic verify check when uploading data.

`-x EXTENDED_PARAM'
     Pass EXTENDED_PARAM to the chosen programmer implementation as an
     extended parameter.  The interpretation of the extended parameter
     depends on the programmer itself.  See below for a list of
     programmers accepting extended parameters.

`-y'
     Tells AVRDUDE to use the last four bytes of the connected parts'
     EEPROM memory to track the number of times the device has been
     erased.  When this option is used and the `-e' flag is specified
     to generate a chip erase, the previous counter will be saved
     before the chip erase, it is then incremented, and written back
     after the erase cycle completes.  Presumably, the device would
     only be erased just before being programmed, and thus, this can be
     utilized to give an indication of how many erase-rewrite cycles
     the part has undergone.  Since the FLASH memory can only endure a
     finite number of erase-rewrite cycles, one can use this option to
     track when a part is nearing the limit.  The typical limit for
     Atmel AVR FLASH is 1000 cycles.  Of course, if the application
     needs the last four bytes of EEPROM memory, this option should not
     be used.

`-Y CYCLES'
     Instructs AVRDUDE to initialize the erase-rewrite cycle counter
     residing at the last four bytes of EEPROM memory to the specified
     value.  If the application needs the last four bytes of EEPROM
     memory, this option should not be used.



File: avrdude.info,  Node: Programmers accepting extended parameters,  Next: Example Command Line Invocations,  Prev: Option Descriptions,  Up: Command Line Options

2.2 Programmers accepting extended parameters
=============================================

`JTAG ICE mkII'
`AVR Dragon'
     When using the JTAG ICE mkII or AVR Dragon in JTAG mode, the
     following extended parameter is accepted:
    ``jtagchain=UB,UA,BB,BA''
          Setup the JTAG scan chain for UB units before, UA units
          after, BB bits before, and BA bits after the target AVR,
          respectively.  Each AVR unit within the chain shifts by 4
          bits.  Other JTAG units might require a different bit shift
          count.

`AVR910'
     The AVR910 programmer type accepts the following extended
     parameter:
    ``devcode=VALUE''
          Override the device code selection by using VALUE as the
          device code.  The programmer is not queried for the list of
          supported device codes, and the specified VALUE is not
          verified but used directly within the `T' command sent to the
          programmer.  VALUE can be specified using the conventional
          number notation of the C programming language.

    ``no_blockmode''
          Disables the default checking for block transfer capability.
          Use `no_blockmode' only if your `AVR910' programmer creates
          errors during initial sequence.



File: avrdude.info,  Node: Example Command Line Invocations,  Prev: Programmers accepting extended parameters,  Up: Command Line Options

2.3 Example Command Line Invocations
====================================

Download the file `diag.hex' to the ATmega128 chip using the STK500
programmer connected to the default serial port:

     % avrdude -p m128 -c stk500 -e -U flash:w:diag.hex

     avrdude: AVR device initialized and ready to accept instructions

     Reading | ################################################## | 100% 0.03s

     avrdude: Device signature = 0x1e9702
     avrdude: erasing chip
     avrdude: done.
     avrdude: performing op: 1, flash, 0, diag.hex
     avrdude: reading input file "diag.hex"
     avrdude: input file diag.hex auto detected as Intel Hex
     avrdude: writing flash (19278 bytes):

     Writing | ################################################## | 100% 7.60s

     avrdude: 19456 bytes of flash written
     avrdude: verifying flash memory against diag.hex:
     avrdude: load data flash data from input file diag.hex:
     avrdude: input file diag.hex auto detected as Intel Hex
     avrdude: input file diag.hex contains 19278 bytes
     avrdude: reading on-chip flash data:

     Reading | ################################################## | 100% 6.83s

     avrdude: verifying ...
     avrdude: 19278 bytes of flash verified

     avrdude: safemode: Fuses OK

     avrdude done.  Thank you.

     %

Upload the flash memory from the ATmega128 connected to the STK500
programmer and save it in raw binary format in the file named `c:/diag
flash.bin':

     % avrdude -p m128 -c stk500 -U flash:r:"c:/diag flash.bin":r

     avrdude: AVR device initialized and ready to accept instructions

     Reading | ################################################## | 100% 0.03s

     avrdude: Device signature = 0x1e9702
     avrdude: reading flash memory:

     Reading | ################################################## | 100% 46.10s

     avrdude: writing output file "c:/diag flash.bin"

     avrdude: safemode: Fuses OK

     avrdude done.  Thank you.

     %

Using the default programmer, download the file `diag.hex' to flash,
`eeprom.hex' to EEPROM, and set the Extended, High, and Low fuse bytes
to 0xff, 0x89, and 0x2e respectively:


     % avrdude -p m128 -u -U flash:w:diag.hex \
     >                 -U eeprom:w:eeprom.hex \
     >                 -U efuse:w:0xff:m      \
     >                 -U hfuse:w:0x89:m      \
     >                 -U lfuse:w:0x2e:m

     avrdude: AVR device initialized and ready to accept instructions

     Reading | ################################################## | 100% 0.03s

     avrdude: Device signature = 0x1e9702
     avrdude: NOTE: FLASH memory has been specified, an erase cycle will be performed
              To disable this feature, specify the -D option.
     avrdude: erasing chip
     avrdude: reading input file "diag.hex"
     avrdude: input file diag.hex auto detected as Intel Hex
     avrdude: writing flash (19278 bytes):

     Writing | ################################################## | 100% 7.60s

     avrdude: 19456 bytes of flash written
     avrdude: verifying flash memory against diag.hex:
     avrdude: load data flash data from input file diag.hex:
     avrdude: input file diag.hex auto detected as Intel Hex
     avrdude: input file diag.hex contains 19278 bytes
     avrdude: reading on-chip flash data:

     Reading | ################################################## | 100% 6.84s

     avrdude: verifying ...
     avrdude: 19278 bytes of flash verified

     [ ... other memory status output skipped for brevity ... ]

     avrdude done.  Thank you.

     %

Connect to the JTAG ICE mkII which serial number ends up in 1C37 via
USB, and enter terminal mode:


     % avrdude -c jtag2 -p m649 -P usb:1c:37 -t

     avrdude: AVR device initialized and ready to accept instructions

     Reading | ################################################## | 100% 0.03s

     avrdude: Device signature = 0x1e9603

     [ ... terminal mode output skipped for brevity ... ]

     avrdude done.  Thank you.

List the serial numbers of all JTAG ICEs attached to USB.  This is done
by specifying an invalid serial number, and increasing the verbosity
level.


     % avrdude -c jtag2 -p m128 -P usb:xx -v
     [...]
              Using Port            : usb:xxx
              Using Programmer      : jtag2
     avrdude: usbdev_open(): Found JTAG ICE, serno: 00A000001C6B
     avrdude: usbdev_open(): Found JTAG ICE, serno: 00A000001C3A
     avrdude: usbdev_open(): Found JTAG ICE, serno: 00A000001C30
     avrdude: usbdev_open(): did not find any (matching) USB device "usb:xxx"


File: avrdude.info,  Node: Terminal Mode Operation,  Next: Configuration File,  Prev: Command Line Options,  Up: Top

3 Terminal Mode Operation
*************************

AVRDUDE has an interactive mode called TERMINAL MODE that is enabled by
the `-t' option.  This mode allows one to enter interactive commands to
display and modify the various device memories, perform a chip erase,
display the device signature bytes and part parameters, and to send raw
programming commands.  Commands and parameters may be abbreviated to
their shortest unambiguous form.  Terminal mode also supports a command
history so that previously entered commands can be recalled and edited.

* Menu:

* Terminal Mode Commands::
* Terminal Mode Examples::


File: avrdude.info,  Node: Terminal Mode Commands,  Next: Terminal Mode Examples,  Prev: Terminal Mode Operation,  Up: Terminal Mode Operation

3.1 Terminal Mode Commands
==========================

The following commands are implemented:

`dump MEMTYPE ADDR NBYTES'
     Read NBYTES from the specified memory area, and display them in
     the usual hexadecimal and ASCII form.

`dump'
     Continue dumping the memory contents for another NBYTES where the
     previous dump command left off.

`write MEMTYPE ADDR BYTE1 ... BYTEN'
     Manually program the respective memory cells, starting at address
     addr, using the values BYTE1 through BYTEN.  This feature is not
     implemented for bank-addressed memories such as the flash memory of
     ATMega devices.

`erase'
     Perform a chip erase.

`send B1 B2 B3 B4'
     Send raw instruction codes to the AVR device.  If you need access
     to a feature of an AVR part that is not directly supported by
     AVRDUDE, this command allows you to use it, even though AVRDUDE
     does not implement the command.   When using direct SPI mode, up
     to 3 bytes can be omitted.

`sig'
     Display the device signature bytes.

`spi'
     Enter direct SPI mode.  The _pgmled_ pin acts as slave select.
     _Only supported on parallel bitbang programmers._

`part'
     Display the current part settings and parameters.  Includes chip
     specific information including all memory types supported by the
     device, read/write timing, etc.

`pgm'
     Return to programming mode (from direct SPI mode).

`?'
`help'
     Give a short on-line summary of the available commands.

`quit'
     Leave terminal mode and thus AVRDUDE.


In addition, the following commands are supported on the STK500 and
STK600 programmer:

`vtarg VOLTAGE'
     Set the target's supply voltage to VOLTAGE Volts.

`varef [CHANNEL] VOLTAGE'
     Set the adjustable voltage source to VOLTAGE Volts.  This voltage
     is normally used to drive the target's _Aref_ input on the STK500
     and STK600.  The STK600 offers two reference voltages, which can be
     selected by the optional parameter CHANNEL (either 0 or 1).

`fosc FREQ[`M'|`k']'
     Set the master oscillator to FREQ Hz.  An optional trailing letter
     `M' multiplies by 1E6, a trailing letter `k' by 1E3.

`fosc off'
     Turn the master oscillator off.

`sck PERIOD'
     _STK500 and STK600 only:_ Set the SCK clock period to PERIOD
     microseconds.

     _JTAG ICE only:_ Set the JTAG ICE bit clock period to PERIOD
     microseconds.  Note that unlike STK500 settings, this setting will
     be reverted to its default value (approximately 1 microsecond)
     when the programming software signs off from the JTAG ICE.  This
     parameter can also be used on the JTAG ICE mkII to specify the ISP
     clock period when operating the ICE in ISP mode.

`parms'
     _STK500 and STK600 only:_ Display the current voltage and master
     oscillator parameters.

     _JTAG ICE only:_ Display the current target supply voltage and
     JTAG bit clock rate/period.



File: avrdude.info,  Node: Terminal Mode Examples,  Prev: Terminal Mode Commands,  Up: Terminal Mode Operation

3.2 Terminal Mode Examples
==========================

Display part parameters, modify eeprom cells, perform a chip erase:

     % avrdude -p m128 -c stk500 -t

     avrdude: AVR device initialized and ready to accept instructions
     avrdude: Device signature = 0x1e9702
     avrdude: current erase-rewrite cycle count is 52 (if being tracked)
     avrdude> part
     >>> part

     AVR Part              : ATMEGA128
     Chip Erase delay      : 9000 us
     PAGEL                 : PD7
     BS2                   : PA0
     RESET disposition     : dedicated
     RETRY pulse           : SCK
     serial program mode   : yes
     parallel program mode : yes
     Memory Detail         :

                                 Page                       Polled
       Memory Type Paged  Size   Size #Pages MinW  MaxW   ReadBack
       ----------- ------ ------ ---- ------ ----- ----- ---------
       eeprom      no       4096    8     0  9000  9000 0xff 0xff
       flash       yes    131072  256   512  4500  9000 0xff 0x00
       lfuse       no          1    0     0     0     0 0x00 0x00
       hfuse       no          1    0     0     0     0 0x00 0x00
       efuse       no          1    0     0     0     0 0x00 0x00
       lock        no          1    0     0     0     0 0x00 0x00
       calibration no          1    0     0     0     0 0x00 0x00
       signature   no          3    0     0     0     0 0x00 0x00

     avrdude> dump eeprom 0 16
     >>> dump eeprom 0 16
     0000  ff ff ff ff ff ff ff ff  ff ff ff ff ff ff ff ff  |................|

     avrdude> write eeprom 0 1 2 3 4
     >>> write eeprom 0 1 2 3 4

     avrdude> dump eeprom 0 16
     >>> dump eeprom 0 16
     0000  01 02 03 04 ff ff ff ff  ff ff ff ff ff ff ff ff  |................|

     avrdude> erase
     >>> erase
     avrdude: erasing chip
     avrdude> dump eeprom 0 16
     >>> dump eeprom 0 16
     0000  ff ff ff ff ff ff ff ff  ff ff ff ff ff ff ff ff  |................|

     avrdude>

Program the fuse bits of an ATmega128 (disable M103 compatibility,
enable high speed external crystal, enable brown-out detection, slowly
rising power).  Note since we are working with fuse bits the -u (unsafe)
option is specified, which allows you to modify the fuse bits. First
display the factory defaults, then reprogram:

     % avrdude -p m128 -u -c stk500 -t

     avrdude: AVR device initialized and ready to accept instructions
     avrdude: Device signature = 0x1e9702
     avrdude: current erase-rewrite cycle count is 52 (if being tracked)
     avrdude> d efuse
     >>> d efuse
     0000  fd                                                |.               |

     avrdude> d hfuse
     >>> d hfuse
     0000  99                                                |.               |

     avrdude> d lfuse
     >>> d lfuse
     0000  e1                                                |.               |

     avrdude> w efuse 0 0xff
     >>> w efuse 0 0xff

     avrdude> w hfuse 0 0x89
     >>> w hfuse 0 0x89

     avrdude> w lfuse 0 0x2f
     >>> w lfuse 0 0x2f

     avrdude>


File: avrdude.info,  Node: Configuration File,  Next: Programmer Specific Information,  Prev: Terminal Mode Operation,  Up: Top

4 Configuration File
********************

AVRDUDE reads a configuration file upon startup which describes all of
the parts and programmers that it knows about.  The advantage of this is
that if you have a chip that is not currently supported by AVRDUDE, you
can add it to the configuration file without waiting for a new release
of AVRDUDE.  Likewise, if you have a parallel port programmer that is
not supported by AVRDUDE, chances are good that you can copy and
existing programmer definition, and with only a few changes, make your
programmer work with AVRDUDE.

   AVRDUDE first looks for a system wide configuration file in a
platform dependent location.  On Unix, this is usually
`/usr/local/etc/avrdude.conf', while on Windows it is usally in the
same location as the executable file.  The name of this file can be
changed using the `-C' command line option.  After the system wide
configuration file is parsed, AVRDUDE looks for a per-user configuration
file to augment or override the system wide defaults.  On Unix, the
per-user file is `.avrduderc' within the user's home directory.  On
Windows, this file is the `avrdude.rc' file located in the same
directory as the executable.

* Menu:

* AVRDUDE Defaults::
* Programmer Definitions::
* Part Definitions::
* Other Notes::


File: avrdude.info,  Node: AVRDUDE Defaults,  Next: Programmer Definitions,  Prev: Configuration File,  Up: Configuration File

4.1 AVRDUDE Defaults
====================

`default_parallel = "DEFAULT-PARALLEL-DEVICE";'
     Assign the default parallel port device.  Can be overidden using
     the `-P' option.

`default_serial = "DEFAULT-SERIAL-DEVICE";'
     Assign the default serial port device.  Can be overidden using the
     `-P' option.

`default_programmer = "DEFAULT-PROGRAMMER-ID";'
     Assign the default programmer id.  Can be overidden using the `-c'
     option.



File: avrdude.info,  Node: Programmer Definitions,  Next: Part Definitions,  Prev: AVRDUDE Defaults,  Up: Configuration File

4.2 Programmer Definitions
==========================

The format of the programmer definition is as follows:

     programmer
         id     = <id1> [, <id2> [, <id3>] ...] ;  # <idN> are quoted strings
         desc     = <description> ;                  # quoted string
         type     = par | stk500 ;                   # programmer type
         baudrate = <num> ;                          # baudrate for serial ports
         vcc      = <num1> [, <num2> ... ] ;         # pin number(s)
         reset    = <num> ;                          # pin number
         sck      = <num> ;                          # pin number
         mosi     = <num> ;                          # pin number
         miso     = <num> ;                          # pin number
         errled   = <num> ;                          # pin number
         rdyled   = <num> ;                          # pin number
         pgmled   = <num> ;                          # pin number
         vfyled   = <num> ;                          # pin number
       ;


File: avrdude.info,  Node: Part Definitions,  Next: Other Notes,  Prev: Programmer Definitions,  Up: Configuration File

4.3 Part Definitions
====================

     part
         id               = <id> ;                 # quoted string
         desc             = <description> ;        # quoted string
         devicecode       = <num> ;                # numeric
         chip_erase_delay = <num> ;                # micro-seconds
         pagel            = <num> ;                # pin name in hex, i.e., 0xD7
         bs2              = <num> ;                # pin name in hex, i.e., 0xA0
         reset            = dedicated | io;
         retry_pulse      = reset | sck;
         pgm_enable       = <instruction format> ;
         chip_erase       = <instruction format> ;
         memory <memtype>
             paged           = <yes/no> ;          # yes / no
             size            = <num> ;             # bytes
             page_size       = <num> ;             # bytes
             num_pages       = <num> ;             # numeric
             min_write_delay = <num> ;             # micro-seconds
             max_write_delay = <num> ;             # micro-seconds
             readback_p1     = <num> ;             # byte value
             readback_p2     = <num> ;             # byte value
             pwroff_after_write = <yes/no> ;       # yes / no
             read            = <instruction format> ;
             write           = <instruction format> ;
             read_lo         = <instruction format> ;
             read_hi         = <instruction format> ;
             write_lo        = <instruction format> ;
             write_hi        = <instruction format> ;
             loadpage_lo     = <instruction format> ;
             loadpage_hi     = <instruction format> ;
             writepage       = <instruction format> ;
           ;
       ;

* Menu:

* Instruction Format::


File: avrdude.info,  Node: Instruction Format,  Prev: Part Definitions,  Up: Part Definitions

4.3.1 Instruction Format
------------------------

Instruction formats are specified as a comma seperated list of string
values containing information (bit specifiers) about each of the 32 bits
of the instruction.  Bit specifiers may be one of the following formats:

`1'
     The bit is always set on input as well as output

`0'
     the bit is always clear on input as well as output

`x'
     the bit is ignored on input and output

`a'
     the bit is an address bit, the bit-number matches this bit
     specifier's position within the current instruction byte

`aN'
     the bit is the Nth address bit, bit-number = N, i.e., `a12' is
     address bit 12 on input, `a0' is address bit 0.

`i'
     the bit is an input data bit

`o'
     the bit is an output data bit


   Each instruction must be composed of 32 bit specifiers.  The
instruction specification closely follows the instruction data provided
in Atmel's data sheets for their parts.  For example, the EEPROM read
and write instruction for an AT90S2313 AVR part could be encoded as:


     read  = "1  0  1  0   0  0  0  0   x x x x  x x x x",
             "x a6 a5 a4  a3 a2 a1 a0   o o o o  o o o o";

     write = "1  1  0  0   0  0  0  0   x x x x  x x x x",
             "x a6 a5 a4  a3 a2 a1 a0   i i i i  i i i i";


File: avrdude.info,  Node: Other Notes,  Prev: Part Definitions,  Up: Configuration File

4.4 Other Notes
===============

   * The `devicecode' parameter is the device code used by the STK500
     and is obtained from the software section (`avr061.zip') of
     Atmel's AVR061 application note available from
     `http://www.atmel.com/atmel/acrobat/doc2525.pdf'.

   * Not all memory types will implement all instructions.

   * AVR Fuse bits and Lock bits are implemented as a type of memory.

   * Example memory types are: `flash', `eeprom', `fuse', `lfuse' (low
     fuse), `hfuse' (high fuse), `efuse' (extended fuse), `signature',
     `calibration', `lock'.

   * The memory type specified on the AVRDUDE command line must match
     one of the memory types defined for the specified chip.

   * The `pwroff_after_write' flag causes AVRDUDE to attempt to power
     the device off and back on after an unsuccessful write to the
     affected memory area if VCC programmer pins are defined.  If VCC
     pins are not defined for the programmer, a message indicating that
     the device needs a power-cycle is printed out.  This flag was
     added to work around a problem with the at90s4433/2333's; see the
     at90s4433 errata at:

     `http://www.atmel.com/atmel/acrobat/doc1280.pdf'

   * The boot loader from application note AVR109 (and thus also the AVR
     Butterfly) does not support writing of fuse bits.  Writing lock
     bits is supported, but is restricted to the boot lock bits
     (BLBxx).  These are restrictions imposed by the underlying SPM
     instruction that is used to program the device from inside the
     boot loader.  Note that programming the boot lock bits can result
     in a "shoot-into-your-foot" scenario as the only way to unprogram
     these bits is a chip erase, which will also erase the boot loader
     code.

     The boot loader implements the "chip erase" function by erasing the
     flash pages of the application section.

     Reading fuse and lock bits is fully supported.

     Note that due to the unability to write the fuse bits, the safemode
     functionality does not make sense for these boot loaders.



File: avrdude.info,  Node: Programmer Specific Information,  Next: Platform Dependent Information,  Prev: Configuration File,  Up: Top

5 Programmer Specific Information
*********************************

* Menu:

* Atmel STK600::


File: avrdude.info,  Node: Atmel STK600,  Prev: Programmer Specific Information,  Up: Programmer Specific Information

5.1 Atmel STK600
================

The following devices are supported by the respective STK600 routing
and socket card:

Routing card       Socket card        Devices
--------------------------------------------------------------------------- 
`STK600-RC008T-2'  `STK600-DIP'       ATtiny11 ATtiny12 ATtiny13 ATtiny25
                                      ATtiny45 ATtiny85
`STK600-RC008T-7'  `STK600-DIP'       ATtiny15
`STK600-RC020T-1'  `STK600-DIP'       ATtiny2313
`'                 `STK600-TinyX3U'   ATtiny43U
`STK600-RC014T-12' `STK600-DIP'       ATtiny24 ATtiny44 ATtiny84
`STK600-RC020T-8'  `STK600-DIP'       ATtiny26 ATtiny261 ATtiny461
                                      ATtiny861
`STK600-RC020T-23' `STK600-SOIC'      ATtiny167
`STK600-RC028T-3'  `STK600-DIP'       ATtiny28
`STK600-RC028M-6'  `STK600-DIP'       ATtiny48 ATtiny88 ATmega8 ATmega48
                                      ATmega88 ATmega168 ATmega48P
                                      ATmega88P ATmega168P ATmega328P
`STK600-RC040M-4'  `STK600-DIP'       ATmega8515 ATmega162
`STK600-RC040M-5'  `STK600-DIP'       ATmega8535 ATmega16 ATmega32
                                      ATmega164P ATmega324P ATmega644
                                      ATmega644P ATmega1284P
`STK600-RC064M-9'  `STK600-TQFP64'    ATmega64 ATmega128 ATmega1281
                                      ATmega2561 AT90CAN32 AT90CAN64
                                      AT90CAN128
`STK600-RC064M-10' `STK600-TQFP64'    ATmega165 ATmega165P ATmega169
                                      ATmega169P ATmega325 ATmega325P
                                      ATmega329 ATmega329P ATmega645
                                      ATmega649
`STK600-RC100M-11' `STK600-TQFP100'   ATmega640 ATmega1280 ATmega2560
`'                 `STK600-ATMEGA2560'ATmega2560
`STK600-RC100M-18' `STK600-TQFP100'   ATmega3250 ATmega3250P ATmega3290
                                      ATmega3290P ATmega6450 ATmega6490
`STK600-RC32U-20'  `STK600-TQFP32'    AT90USB82 AT90USB162
`STK600-RC044U-25' `STK600-TQFP44'    ATmega32U4
`STK600-RC064U-17' `STK600-TQFP64'    AT90USB646 AT90USB1286 AT90USB647
                                      AT90USB1287
`STK600-RCPWM-22'  `STK600-TQFP32'    ATmega32C1 ATmega32M1
`STK600-RCPWM-19'  `STK600-SOIC'      AT90PWM2 AT90PWM3 AT90PWM2B
                                      AT90PWM3B AT90PWM216 AT90PWM316
`STK600-RC044M-24' `STK600-TSSOP44'   ATmega32HVB
`STK600-RC100X-13' `STK600-TQFP100'   ATxmega128A1 ATxmega128A1_revD
                                      ATxmega64A1
`'                 `STK600-uC3-144'   AT32UC3A0512 AT32UC3A0256
                                      AT32UC3A0128
`STK600-RCuC3B0-21'`STK600-TQFP64-2'  AT32UC3B0256 AT32UC3B0128
                                      AT32UC3B064

   Ensure the correct socket and routing card are mounted _before_
powering on the STK600.  While the STK600 firmware ensures the socket
and routing card mounted match each other (using a table stored
internally in nonvolatile memory), it cannot handle the case where a
wrong routing card is used, e. g. the routing card `STK600-RC040M-5'
(which is meant for 40-pin DIP AVRs that have an ADC, with the power
supply pins in the center of the package) was used but an ATmega8515
inserted (which uses the "industry standard" pinout with Vcc and GND at
opposite corners).

   Note that for devices that use the routing card `STK600-RC008T-2',
in order to use ISP mode, the jumper for `AREF0' must be removed as it
would otherwise block one of the ISP signals.  High-voltage serial
programming can be used even with that jumper installed.

   The ISP system of the STK600 contains a detection against shortcuts
and other wiring errors.  AVRDUDE initiates a connection check before
trying to enter ISP programming mode, and display the result if the
target is not found ready to be ISP programmed.

   High-voltage programming requires the target voltage to be set to at
least 4.5 V in order to work.  This can be done using _Terminal Mode_,
see *Note Terminal Mode Operation::.


File: avrdude.info,  Node: Platform Dependent Information,  Next: Troubleshooting,  Prev: Programmer Specific Information,  Up: Top

Appendix A Platform Dependent Information
*****************************************

* Menu:

* Unix::
* Windows::


File: avrdude.info,  Node: Unix,  Next: Windows,  Prev: Platform Dependent Information,  Up: Platform Dependent Information

A.1 Unix
========

* Menu:

* Unix Installation::
* Unix Configuration Files::
* Unix Port Names::
* Unix Documentation::


File: avrdude.info,  Node: Unix Installation,  Next: Unix Configuration Files,  Prev: Unix,  Up: Unix

A.1.1 Unix Installation
-----------------------

To build and install from the source tarball on Unix like systems:

     $ gunzip -c avrdude-5.8cvs.tar.gz | tar xf -
     $ cd avrdude-5.8cvs
     $ ./configure
     $ make
     $ su root -c 'make install'

   The default location of the install is into `/usr/local' so you will
need to be sure that `/usr/local/bin' is in your `PATH' environment
variable.

   If you do not have root access to your system, you can do the the
following instead:

     $ gunzip -c avrdude-5.8cvs.tar.gz | tar xf -
     $ cd avrdude-5.8cvs
     $ ./configure --prefix=$HOME/local
     $ make
     $ make install

* Menu:

* FreeBSD Installation::
* Linux Installation::


File: avrdude.info,  Node: FreeBSD Installation,  Next: Linux Installation,  Prev: Unix Installation,  Up: Unix Installation

A.1.1.1 FreeBSD Installation
............................

AVRDUDE is installed via the FreeBSD Ports Tree as follows:

     % su - root
     # cd /usr/ports/devel/avrdude
     # make install

   If you wish to install from a pre-built package instead of the
source, you can use the following instead:

     % su - root
     # pkg_add -r avrdude

   Of course, you must be connected to the Internet for these methods to
work, since that is where the source as well as the pre-built package is
obtained.


File: avrdude.info,  Node: Linux Installation,  Prev: FreeBSD Installation,  Up: Unix Installation

A.1.1.2 Linux Installation
..........................

On rpm based linux systems (such as RedHat, SUSE, Mandrake, etc), you
can build and install the rpm binaries directly from the tarball:

     $ su - root
     # rpmbuild -tb avrdude-5.8cvs.tar.gz
     # rpm -Uvh /usr/src/redhat/RPMS/i386/avrdude-5.8cvs-1.i386.rpm

   Note that the path to the resulting rpm package, differs from system
to system. The above example is specific to RedHat.


File: avrdude.info,  Node: Unix Configuration Files,  Next: Unix Port Names,  Prev: Unix Installation,  Up: Unix

A.1.2 Unix Configuration Files
------------------------------

When AVRDUDE is build using the default `--prefix' configure option,
the default configuration file for a Unix system is located at
`/usr/local/etc/avrdude.conf'.  This can be overridden by using the
`-C' command line option.  Additionally, the user's home directory is
searched for a file named `.avrduderc', and if found, is used to
augment the system default configuration file.

* Menu:

* FreeBSD Configuration Files::
* Linux Configuration Files::


File: avrdude.info,  Node: FreeBSD Configuration Files,  Next: Linux Configuration Files,  Prev: Unix Configuration Files,  Up: Unix Configuration Files

A.1.2.1 FreeBSD Configuration Files
...................................

When AVRDUDE is installed using the FreeBSD ports system, the system
configuration file is always `/usr/local/etc/avrdude.conf'.


File: avrdude.info,  Node: Linux Configuration Files,  Prev: FreeBSD Configuration Files,  Up: Unix Configuration Files

A.1.2.2 Linux Configuration Files
.................................

When AVRDUDE is installed using from an rpm package, the system
configuration file will be always be `/etc/avrdude.conf'.


File: avrdude.info,  Node: Unix Port Names,  Next: Unix Documentation,  Prev: Unix Configuration Files,  Up: Unix

A.1.3 Unix Port Names
---------------------

The parallel and serial port device file names are system specific.
The following table lists the default names for a given system.

*System*               *Default Parallel      *Default Serial Port*
                       Port*                  
FreeBSD                `/dev/ppi0'            `/dev/cuaa0'
Linux                  `/dev/parport0'        `/dev/ttyS0'
Solaris                `/dev/printers/0'      `/dev/term/a'

   On FreeBSD systems, AVRDUDE uses the ppi(4) interface for accessing
the parallel port and the sio(4) driver for serial port access.

   On Linux systems, AVRDUDE uses the ppdev interface for accessing the
parallel port and the tty driver for serial port access.

   On Solaris systems, AVRDUDE uses the ecpp(7D) driver for accessing
the parallel port and the asy(7D) driver for serial port access.


File: avrdude.info,  Node: Unix Documentation,  Prev: Unix Port Names,  Up: Unix

A.1.4 Unix Documentation
------------------------

AVRDUDE installs a manual page as well as info, HTML and PDF
documentation.  The manual page is installed in `/usr/local/man/man1'
area, while the HTML and PDF documentation is installed in
`/usr/local/share/doc/avrdude' directory.  The info manual is installed
in `/usr/local/info/avrdude.info'.

   Note that these locations can be altered by various configure options
such as `--prefix'.


File: avrdude.info,  Node: Windows,  Prev: Unix,  Up: Platform Dependent Information

A.2 Windows
===========

* Menu:

* Windows Installation::
* Windows Configuration Files::
* Windows Port Names::
* Using the parallel port::
* Documentation::
* Credits.::


File: avrdude.info,  Node: Windows Installation,  Next: Windows Configuration Files,  Prev: Windows,  Up: Windows

A.2.1 Installation
------------------

A Windows executable of avrdude is included in WinAVR which can be
found at `http://sourceforge.net/projects/winavr'. WinAVR is a suite of
executable, open source software development tools for the AVR for the
Windows platform.

   To build avrdude from the source You must have Cygwin
(`http://www.cygwin.com/').

   To build and install from the source tarball for Windows (using
Cygwin):

     $ set PREFIX=<your install directory path>
     $ export PREFIX
     $ gunzip -c avrdude-5.8cvs.tar.gz | tar xf -
     $ cd avrdude-5.8cvs
     $ ./configure LDFLAGS="-static" --prefix=$PREFIX --datadir=$PREFIX
     --sysconfdir=$PREFIX/bin --enable-versioned-doc=no
     $ make
     $ make install


File: avrdude.info,  Node: Windows Configuration Files,  Next: Windows Port Names,  Prev: Windows Installation,  Up: Windows

A.2.2 Configuration Files
-------------------------

* Menu:

* Configuration file names::
* How AVRDUDE finds the configuration files.::


File: avrdude.info,  Node: Configuration file names,  Next: How AVRDUDE finds the configuration files.,  Prev: Windows Configuration Files,  Up: Windows Configuration Files

A.2.2.1 Configuration file names
................................

AVRDUDE on Windows looks for a system configuration file name of
`avrdude.conf' and looks for a user override configuration file of
`avrdude.rc'.


File: avrdude.info,  Node: How AVRDUDE finds the configuration files.,  Prev: Configuration file names,  Up: Windows Configuration Files

A.2.2.2 How AVRDUDE finds the configuration files.
..................................................

AVRDUDE on Windows has a different way of searching for the system and
user configuration files. Below is the search method for locating the
configuration files:

  1. The directory from which the application loaded.

  2. The current directory.

  3. The Windows system directory. On Windows NT, the name of this
     directory is `SYSTEM32'.

  4. Windows NT: The 16-bit Windows system directory. The name of this
     directory is `SYSTEM'.

  5. The Windows directory.

  6. The directories that are listed in the PATH environment variable.



File: avrdude.info,  Node: Windows Port Names,  Next: Using the parallel port,  Prev: Windows Configuration Files,  Up: Windows

A.2.3 Port Names
----------------

* Menu:

* Serial Ports::
* Parallel Ports::


File: avrdude.info,  Node: Serial Ports,  Next: Parallel Ports,  Prev: Windows Port Names,  Up: Windows Port Names

A.2.3.1 Serial Ports
....................

When you select a serial port (i.e. when using an STK500) use the
Windows serial port device names such as: com1, com2, etc.


File: avrdude.info,  Node: Parallel Ports,  Prev: Serial Ports,  Up: Windows Port Names

A.2.3.2 Parallel Ports
......................

AVRDUDE will accept 3 Windows parallel port names: lpt1, lpt2, or lpt3.
Each of these names corresponds to a fixed parallel port base address:

`lpt1'
     0x378

`lpt2'
     0x278

`lpt3'
     0x3BC


   On your desktop PC, lpt1 will be the most common choice. If you are
using a laptop, you might have to use lpt3 instead of lpt1. Select the
name of the port the corresponds to the base address of the parallel
port that you want.

   If the parallel port can be accessed through a different address,
this address can be specified directly, using the common C language
notation (i. e., hexadecimal values are prefixed by `0x').


File: avrdude.info,  Node: Using the parallel port,  Next: Documentation,  Prev: Windows Port Names,  Up: Windows

A.2.4 Using the parallel port
-----------------------------

* Menu:

* Windows NT/2K/XP::
* Windows 95/98::


File: avrdude.info,  Node: Windows NT/2K/XP,  Next: Windows 95/98,  Prev: Using the parallel port,  Up: Using the parallel port

A.2.4.1 Windows NT/2K/XP
........................

On Windows NT, 2000, and XP user applications cannot directly access the
parallel port. However, kernel mode drivers can access the parallel
port.  giveio.sys is a driver that can allow user applications to set
the state of the parallel port pins.

   Before using AVRDUDE, the giveio.sys driver must be loaded. The
accompanying command-line program, loaddrv.exe, can do just that.

   To make things even easier there are 3 batch files that are also
included:

  1. install_giveio.bat Install and start the giveio driver.

  2. status_giveio.bat Check on the status of the giveio driver.

  3. remove_giveio.bat Stop and remove the giveio driver from memory.

   These 3 batch files calls the loaddrv program with various options to
install, start, stop, and remove the driver.

   When you first execute install_giveio.bat, loaddrv.exe and giveio.sys
must be in the current directory. When install_giveio.bat is executed it
will copy giveio.sys from your current directory to your Windows
directory. It will then load the driver from the Windows directory. This
means that after the first time install_giveio is executed, you should
be able to subsequently execute the batch file from any directory and
have it successfully start the driver.

   Note that you must have administrator privilege to load the giveio
driver.


File: avrdude.info,  Node: Windows 95/98,  Prev: Windows NT/2K/XP,  Up: Using the parallel port

A.2.4.2 Windows 95/98
.....................

On Windows 95 and 98 the giveio.sys driver is not needed.


File: avrdude.info,  Node: Documentation,  Next: Credits.,  Prev: Using the parallel port,  Up: Windows

A.2.5 Documentation
-------------------

AVRDUDE installs a manual page as well as info, HTML and PDF
documentation.  The manual page is installed in `/usr/local/man/man1'
area, while the HTML and PDF documentation is installed in
`/usr/local/share/doc/avrdude' directory.  The info manual is installed
in `/usr/local/info/avrdude.info'.

   Note that these locations can be altered by various configure options
such as `--prefix' and `--datadir'.


File: avrdude.info,  Node: Credits.,  Prev: Documentation,  Up: Windows

A.2.6 Credits.
--------------

Thanks to:

   * Dale Roberts for the giveio driver.

   * Paula Tomlinson for the loaddrv sources.

   * Chris Liechti <cliechti@gmx.net> for modifying loaddrv to be
     command line driven and for writing the batch files.



File: avrdude.info,  Node: Troubleshooting,  Prev: Platform Dependent Information,  Up: Top

Appendix B Troubleshooting
**************************

In general, please report any bugs encountered via
`http://savannah.nongnu.org/bugs/?group=avrdude'.

   * Problem: I'm using a serial programmer under Windows and get the
     following error:

     `avrdude: serial_open(): can't set attributes for device "com1"',

     Solution: This problem seems to appear with certain versions of
     Cygwin. Specifying `"/dev/com1"' instead of `"com1"' should help.

   * Problem: I'm using linux and my AVR910 programmer is really slow.

     Solution (short): `setserial PORT low_latency'

     Solution (long): There are two problems here. First, the system
     may wait some time before it passes data from the serial port to
     the program. Under Linux the following command works around this
     (you may need root privileges for this).

     `setserial PORT low_latency'

     Secondly, the serial interface chip may delay the interrupt for
     some time.  This behaviour can be changed by setting the
     FIFO-threshold to one. Under Linux this can only be done by
     changing the kernel source in `drivers/char/serial.c'.  Search the
     file for `UART_FCR_TRIGGER_8' and replace it with
     `UART_FCR_TRIGGER_1'. Note that overall performance might suffer
     if there is high throughput on serial lines. Also note that you
     are modifying the kernel at your own risk.

   * Problem: I'm not using linux and my AVR910 programmer is really
     slow.

     Solutions: The reasons for this are the same as above.  If you
     know how to work around this on your OS, please let us know.

   * Problem: Updating the flash ROM from terminal mode does not work
     with the JTAG ICEs.

     Solution: None at this time.  Currently, the JTAG ICE code cannot
     write to the flash ROM one byte at a time.

   * Problem: Page-mode programming the EEPROM (using the -U option)
     does not erase EEPROM cells before writing, and thus cannot
     overwrite any previous value != 0xff.

     Solution: None.  This is an inherent feature of the way JTAG EEPROM
     programming works, and is documented that way in the Atmel AVR
     datasheets.  In order to successfully program the EEPROM that way,
     a prior chip erase (with the EESAVE fuse unprogrammed) is required.
     This also applies to the STK500 and STK600 in high-voltage
     programming mode.

   * Problem: How do I turn off the DWEN fuse?

     Solution: If the DWEN (debugWire enable) fuse is activated, the
     /RESET pin is not functional anymore, so normal ISP communication
     cannot be established.  There are two options to deactivate that
     fuse again: high-voltage programming, or getting the JTAG ICE mkII
     talk debugWire, and prepare the target AVR to accept normal ISP
     communication again.

     The first option requires a programmer that is capable of
     high-voltage programming (either serial or parallel, depending on
     the AVR device), for example the STK500.  In high-voltage
     programming mode, the /RESET pin is activated initially using a 12
     V pulse (thus the name _high voltage_), so the target AVR can
     subsequently be reprogrammed, and the DWEN fuse can be cleared.
     Typically, this operation cannot be performed while the AVR is
     located in the target circuit though.

     The second option requires a JTAG ICE mkII that can talk the
     debugWire protocol.  The ICE needs to be connected to the target
     using the JTAG-to-ISP adapter, so the JTAG ICE mkII can be used as
     a debugWire initiator as well as an ISP programmer.  AVRDUDE will
     then be activated using the JTAG2ISP programmer type.  The initial
     ISP communication attempt will fail, but AVRDUDE then tries to
     iniate a debugWire reset.  When successful, this will leave the
     target AVR in a state where it can accept standard ISP
     communication.  The ICE is then signed off (which will make it
     signing off from the USB as well), so AVRDUDE has to be called
     again afterwards.  This time, standard ISP communication can work,
     so the DWEN fuse can be cleared.

     The pin mapping for the JTAG-to-ISP adapter is:

     *JTAG pin*    *ISP pin*
     1             3
     2             6
     3             1
     4             2
     6             5
     9             4

   * Problem: Multiple USBasp or USBtinyISP programmers connected
     simultaneously are not found.

     Solution: none at this time.  The simplicity of these programmers
     doesn't offer a method to distinguish multiple programmers that are
     connected simultaneously, so effectively only one of them is
     supported.

   * Problem: I cannot do ... when the target is in debugWire mode.

     Solution: debugWire mode imposes several limitations.

     The debugWire protocol is Atmel's proprietary one-wire (plus
     ground) protocol to allow an in-circuit emulation of the smaller
     AVR devices, using the /RESET line.  DebugWire mode is initiated
     by activating the DWEN fuse, and then power-cycling the target.
     While this mode is mainly intented for debugging/emulation, it
     also offers limited programming capabilities.  Effectively, the
     only memory areas that can be read or programmed in this mode are
     flash ROM and EEPROM.  It is also possible to read out the
     signature.  All other memory areas cannot be accessed.  There is no
     _chip erase_ functionality in debugWire mode; instead, while
     reprogramming the flash ROM, each flash ROM page is erased right
     before updating it.  This is done transparently by the JTAG ICE
     mkII (or AVR Dragon).  The only way back from debugWire mode is to
     initiate a special sequence of commands to the JTAG ICE mkII (or
     AVR Dragon), so the debugWire mode will be temporarily disabled,
     and the target can be accessed using normal ISP programming.  This
     sequence is automatically initiated by using the JTAG ICE mkII or
     AVR Dragon in ISP mode, when they detect that ISP mode cannot be
     entered.




Tag Table:
Node: Top1086
Node: Introduction1728
Node: History6348
Node: Command Line Options7581
Node: Option Descriptions7859
Node: Programmers accepting extended parameters29919
Node: Example Command Line Invocations31358
Node: Terminal Mode Operation36063
Node: Terminal Mode Commands36800
Node: Terminal Mode Examples39867
Node: Configuration File43051
Node: AVRDUDE Defaults44470
Node: Programmer Definitions45054
Node: Part Definitions46215
Node: Instruction Format48135
Node: Other Notes49522
Node: Programmer Specific Information51700
Node: Atmel STK60051934
Node: Platform Dependent Information56120
Node: Unix56371
Node: Unix Installation56621
Node: FreeBSD Installation57429
Node: Linux Installation58061
Node: Unix Configuration Files58608
Node: FreeBSD Configuration Files59242
Node: Linux Configuration Files59601
Node: Unix Port Names59916
Node: Unix Documentation60907
Node: Windows61434
Node: Windows Installation61696
Node: Windows Configuration Files62549
Node: Configuration file names62816
Node: How AVRDUDE finds the configuration files.63206
Node: Windows Port Names63996
Node: Serial Ports64208
Node: Parallel Ports64495
Node: Using the parallel port65264
Node: Windows NT/2K/XP65491
Node: Windows 95/9866997
Node: Documentation67200
Node: Credits.67756
Node: Troubleshooting68089

End Tag Table
