Defines

# board_ict230.h File Reference

Definition 2.4G Module from In-Circquit with AT86RF230 and Atmega1281 (V1.0). More...

Go to the source code of this file.

## Defines
#define | BOARD_NAME "ict230"
#define | BOARD_TYPE (BOARD_ICT230)
#define | CUSTOM_RESET_TIME_MS (10)
#define | DDR_KEY DDRD
#define | DDR_SPI (DDRB)
#define | DDR_TRX_RESET DDRB
#define | DDR_TRX_SLPTR DDRB
#define | DEFAULT_SPI_RATE (SPI_RATE_1_2)
#define | DI_TRX_IRQ() {EIMSK &= (~(TRX_IRQ));}
#define | EI_TRX_IRQ() {EIMSK |= (TRX_IRQ);}
#define | HIF_TYPE HIF_UART_1
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (1000UL)
#define | HWTMR_PRESCALE (8)
#define | INVERSE_KEYS (1)
#define | LED_DDR DDRD
#define | LED_MASK (0xc0)
#define | LED_NUMBER (2)
#define | LED_PORT PORTD
#define | LED_SHIFT (6)
#define | LEDS_INVERSE (1)
#define | MASK_KEY (0x01)
#define | MASK_TRX_RESET (_BV(PB6))
#define | MASK_TRX_SLPTR (_BV(PB5))
#define | PB0 (0)
#define | PB1 (1)
#define | PB2 (2)
#define | PB3 (3)
#define | PB4 (4)
#define | PB5 (5)
#define | PB6 (6)
#define | PB7 (7)
#define | PIN_KEY PIND
#define | PORT_KEY PORTD
#define | PORT_SPI (PORTB)
#define | PORT_TRX_RESET PORTB
#define | PORT_TRX_SLPTR PORTB
#define | PULLUP_KEYS (1)
#define | RADIO_TYPE (RADIO_AT86RF230)
#define | SHIFT_KEY (0)
#define | SPI_DATA_REG SPDR
#define | SPI_MISO _BV(PB3)
#define | SPI_MOSI _BV(PB2)
#define | SPI_SCK _BV(PB1)
#define | SPI_SELN_HIGH() PORT_SPI |= SPI_SS; SREG = sreg
#define | SPI_SELN_LOW() uint8_t sreg = SREG; cli(); PORT_SPI &=~SPI_SS
#define | SPI_SS _BV(PB4)
#define | SPI_WAITFOR() do { while((SPSR & _BV(SPIF)) == 0);} while(0)
#define | TIMER_INIT()
| Initialisation of TIMER1 (16bit timer).
#define | TIMER_IRQ_vect TIMER1_COMPA_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_IRQ _BV(INT4)
#define | TRX_IRQ_INIT()
#define | TRX_IRQ_vect INT4_vect
#define | TRX_TSTAMP_REG TCNT1

## Detailed Description

Definition 2.4G Module from In-Circquit with AT86RF230 and Atmega1281 (V1.0).

The wiring of the radio and the ATmega is shown below:

      ATmega1281    AT86RF230
      ----------    ---------
         PB1    --> SCK
         PB2    <-- MOSI
         PB3    --> MISO
     PB0/PB4    --> SEL        (you need to drive both pins)
         PB5    --> SLP_TR
         PB6    --> TRX_RESET
    INT4/PE4    --> IRQ
        XTAL2   <-- CLKM

        PD0     --> KEY Interface
        PD6:7   --> LED Interface

        Fuses:
          LF: 0xe2 - 8MHz internal RC Osc.
          HF: 0x11 - without boot loader
          HF: 0x10 - with boot loader
          EF: 0xff
          LOCK: 0xef - protection of boot section

    Bootloader:
        Start at byte=0x1e000, address=0xf000, size = 4096 instructions/ 8192 bytes

Build Options

- ict230 : Incirquit Module

Definition in file board_ict230.h.

## Define Documentation

#define CUSTOM_RESET_TIME_MS (10)

additional delay needed by hardware

Definition at line 101 of file board_ict230.h.

#define DDR_SPI (DDRB)

DDR register for SPI port

Definition at line 125 of file board_ict230.h.

#define DDR_TRX_RESET DDRB

DDR register for RESET pin

Definition at line 98 of file board_ict230.h.

#define DDR_TRX_SLPTR DDRB

PORT register for SLEEP_TR pin

Definition at line 104 of file board_ict230.h.

#define DI_TRX_IRQ | ( |  | ) | {EIMSK &= (~(TRX_IRQ));}

rising edge triggers INT4 disable TRX interrupt

Definition at line 117 of file board_ict230.h.

#define EI_TRX_IRQ | ( |  | ) | {EIMSK |= (TRX_IRQ);}

enable TRX interrupt

Definition at line 119 of file board_ict230.h.

#define MASK_TRX_RESET (_BV(PB6))

PIN mask for RESET pin

Definition at line 100 of file board_ict230.h.

#define MASK_TRX_SLPTR (_BV(PB5))

PIN mask for SLEEP_TR pin

Definition at line 105 of file board_ict230.h.

#define PORT_SPI (PORTB)

PORT register for SPI port

Definition at line 126 of file board_ict230.h.

#define PORT_TRX_RESET PORTB

PORT register for RESET pin

Definition at line 99 of file board_ict230.h.

#define PORT_TRX_SLPTR PORTB

DDR register for SLEEP_TR pin

Definition at line 103 of file board_ict230.h.

#define RADIO_TYPE (RADIO_AT86RF230)

used radiio (see const.h)

Definition at line 94 of file board_ict230.h.

#define SPI_DATA_REG SPDR

abstraction for SPI data register

Definition at line 133 of file board_ict230.h.

#define SPI_MISO _BV(PB3)

PIN mask for MISO pin

Definition at line 129 of file board_ict230.h.

#define SPI_MOSI _BV(PB2)

PIN mask for MOSI pin

Definition at line 128 of file board_ict230.h.

#define SPI_SCK _BV(PB1)

PIN mask for SCK pin

Definition at line 130 of file board_ict230.h.

#define SPI_SELN_HIGH | ( |  | ) | PORT_SPI |= SPI_SS; SREG = sreg

set SS line to high level

Definition at line 163 of file board_ict230.h.

#define SPI_SELN_LOW | ( |  | ) | uint8_t sreg = SREG; cli(); PORT_SPI &=~SPI_SS

set SS line to low level

Definition at line 161 of file board_ict230.h.

#define SPI_SS _BV(PB4)

PIN mask for SS pin

Definition at line 131 of file board_ict230.h.

#define SPI_WAITFOR | ( |  | ) | do { while((SPSR & _BV(SPIF)) == 0);} while(0)

wait until SPI transfer is ready

Definition at line 165 of file board_ict230.h.

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= (_BV(CS11) | _BV(WGM12)); \
            TIMSK1 |= _BV(OCIE1A); \
            OCR1A = 1000; \
        }while(0)

Initialisation of TIMER1 (16bit timer).

- CSxxx=b010: Prescaler = 8
- WGMxxxx = b0100: Mode = 4 (CTC Mode)
- OCR1A = 1000 Prescaler = 8 / Mode 4, CTC mit OCR1A = 1000 @ F_CPU = 8MHz this results in 1ms timer tick IRQ's.

Definition at line 206 of file board_ict230.h.

#define TRX_IRQ _BV(INT4)

interrupt mask for GICR

Definition at line 108 of file board_ict230.h.

#define TRX_IRQ_INIT | ( |  | ) |

Value:

    do{\
                                EICRB  |= (_BV(ISC41)|_BV(ISC40));\
                              } while(0)

configuration of interrupt handling

Definition at line 112 of file board_ict230.h.

#define TRX_IRQ_vect INT4_vect

interrupt vector name

Definition at line 109 of file board_ict230.h.

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event

Definition at line 122 of file board_ict230.h.