Functions | Variables

# ieee802154.py File Reference

Capture converter script. More...

Go to the source code of this file.

## Functions
def | ieee802154::do_exit
| exit handler, prompts on all Non-*NIX systems for "ENTER" in order to see the last error message in the terminal.
def | ieee802154::do_quit
| Terminate all instances of the IO classes.
def | ieee802154::print_banner
| print startup message with some essential information about the current configuration.
def | ieee802154::print_help
| print a list of the commands available on the "cmd:" prompt
def | ieee802154::print_options
def | ieee802154::process_command
| process interactive command
def | ieee802154::process_command_line_args
| Interpretation of command line options.
def | ieee802154::setverbose
## Variables
tuple | ieee802154::cmd = raw_input("cmd:")
tuple | ieee802154::CTX = ProgramContext()
| ieee802154::DEVIN = None
| This class instance stores the global programm context.
tuple | ieee802154::DEVOUT = PipeOut()
tuple | ieee802154::gui = CtrlGui(lambda : do_quit(['gui']))
int | ieee802154::run = 1
string | ieee802154::VERSION = "0.1"

## Detailed Description

Capture converter script.

This script implements a bridge between a file or a serial port to a socket. This socket is the interface for wireshark/libpcap in order to do a live capture.

How the script is used is described here.

Definition in file ieee802154.py.