Defines

# board_rbbrfa1.h File Reference

Definition of Radio Controller Breakout Board (light and normal) from Dresden Elektronik, ATmega128RFA1 version. More...

Go to the source code of this file.

## Defines
#define | DDR_KEY DDRE
#define | HIF_TYPE HIF_UART_1
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL)
#define | HWTMR_PRESCALE (1)
#define | INVERSE_KEYS (1)
#define | LED_DDR DDRE
#define | LED_MASK (0x1c)
#define | LED_NUMBER (3)
#define | LED_PORT PORTE
#define | LED_SHIFT (2)
#define | LEDS_INVERSE (1)
#define | MASK_KEY (0x20)
#define | MAX_FRAME_SIZE (127)
#define | PIN_KEY PINE
#define | PORT_KEY PORTE
#define | PULLUP_KEYS (1)
#define | SHIFT_KEY (5)
#define | SLEEP_ON_KEY()
#define | SLEEP_ON_KEY_INIT() do{}while(0)
#define | SLEEP_ON_KEY_vect INT5_vect
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_OVF_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_RESET_HIGH() do { TRXPR |= _BV(TRXRST); } while (0)
#define | TRX_RESET_LOW() do { TRXPR &= ~_BV(TRXRST); } while (0)
#define | TRX_SLPTR_HIGH() do { TRXPR |= _BV(SLPTR); } while (0)
#define | TRX_SLPTR_LOW() do { TRXPR &= ~_BV(SLPTR); } while (0)
#define | TRX_TSTAMP_REG TCNT1

## Detailed Description

Definition of Radio Controller Breakout Board (light and normal) from Dresden Elektronik, ATmega128RFA1 version.

The Breakout board is a carrier board for the radio controller board family.

    Peripherals:
        KEY: PE5
        LEDS PE2:PE4

    Fuses/Locks:
         LF: 0xe2 - 8MHz internal RC Osc.
         HF: 0x11 - without boot loader
         HF: 0x10 - with boot loader
         EF: 0xff
         LOCK: 0xef - protection of boot section

    Bootloader:
        Start at byte=0x1e000, address=0xf000, size = 4096 instructions/ 8192 bytes

Build Options

- rbb128rfa1 : BB + RCB128RFA1

Definition in file board_rbbrfa1.h.

## Define Documentation

#define MAX_FRAME_SIZE (127)

maximum allowed frame size

Definition at line 74 of file board_rbbrfa1.h.

#define SLEEP_ON_KEY | ( |  | ) |

Value:

    do{\
                EIMSK |= _BV(INT5);\
                set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
                sleep_mode();\
                EIMSK &= ~_BV(INT5);\
            } while(0)

Definition at line 98 of file board_rbbrfa1.h.

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= (_BV(CS10)); \
            TIMSK1 |= _BV(TOIE1); \
        }while(0)

Definition at line 124 of file board_rbbrfa1.h.

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event

Definition at line 78 of file board_rbbrfa1.h.