Data Fields

# prot_wuart_header_t Struct Reference

## Data Fields
uint16_t | dst
uint16_t | fcf
uint8_t | seq
uint16_t | src

## Detailed Description

Frame header structure

This frame format uses the same frame format like 802.15.4 frames, but the interpretation of FCF bits for adressing uses reserved values.

Definition at line 49 of file prot_wuart.h.

## Field Documentation

uint16_t prot_wuart_header_t::dst

16 bit destination address

Definition at line 53 of file prot_wuart.h.

uint16_t prot_wuart_header_t::fcf

Frame control field

Definition at line 51 of file prot_wuart.h.

uint8_t prot_wuart_header_t::seq

Sequence number

Definition at line 52 of file prot_wuart.h.

uint16_t prot_wuart_header_t::src

16 bit source address

Definition at line 54 of file prot_wuart.h.