µracoli Manual Version foo

- µracoli
- User Guide
- Reference Guide

HMC5883L - 3-Axis Digital Compass IC
Sensor Drivers

## Detailed Description

The Honeywell HMC5883L is a surface-mount, multi-chip module designed for low-field magnetic sensing.

Datasheet: HMC5883L_3-Axis_Digital_Compass_IC.pdf

## Functions

static uint8_t sensor_create_hmc5883l | ( | void * | pdata,
|  | bool | raw,
|  | uint8_t | addr
| ) |  |
| static

Create an instance of a hmc5883l sensor and initialize the sensor.

Returns
  sizeof(hmc5883l_ctx_t)

Definition at line 122 of file hmc5883l.h.