µracoli Manual Version foo

- µracoli
- User Guide
- Reference Guide

Data Fields
p2p_hdr_t Struct Reference

## Data Fields
uint16_t | fcf
uint8_t | seq
uint16_t | pan
uint16_t | dst
uint16_t | src
uint8_t | cmd

## Detailed Description

Frame header structure for P2P applications. This header is formated as a IEEE 802.15.4 frame header with short addressing mode for src and dst and pan comression set to on.

Definition at line 94 of file p2p_protocol.h.

## Field Documentation

uint8_t p2p_hdr_t::cmd

the command code that identifies the frame, see p2p_cmdcode_t

Definition at line 101 of file p2p_protocol.h.

uint16_t p2p_hdr_t::dst

destination short address

Definition at line 99 of file p2p_protocol.h.

uint16_t p2p_hdr_t::fcf

frame control field

Definition at line 96 of file p2p_protocol.h.

uint16_t p2p_hdr_t::pan

destination pan id

Definition at line 98 of file p2p_protocol.h.

uint8_t p2p_hdr_t::seq

sequence number

Definition at line 97 of file p2p_protocol.h.

uint16_t p2p_hdr_t::src

source short address

Definition at line 100 of file p2p_protocol.h.