µracoli Manual Version foo

- µracoli
- User Guide
- Reference Guide

Using the CDC driver for RZUSBSTICK

The HIF driver for the Raven USB stick implements a CDC device. This can be handled by generic virtuell COM port driver.

The Vendor/Device ID used by µracoli is:

- Vendor ID: 5824 0x16C0
- Product ID: 2183 0x887

see also http://www.frank-buss.de/pid.txt

Linux

- /usr/sbin/lsusb
  - `Bus 003 Device 009: ID 16c0:0887`
- for SuSE 10.0 the driver cdc_acm was not loaded automatically, in this case the command "modprobe cdc_acm" loads the driver.
- dmesg | grep ACM ==> "cdc_acm 3-1.4:1.0: ttyACM0: USB ACM device"
- Some older pyserial versions come up with the following error: `[Errno 11] Resource temporarily unavailable` In this case apply the patch or upgrade pyserial: http://mail.python.org/pipermail/python-list/2004-November/294242.html

Windows

- µracoli provids a INF file that installs the usbserial.sys driver. uracoli-cdc.inf