µracoli Manual Version foo

- µracoli
- User Guide
- Reference Guide

MCU Operating Voltage Sensor
Sensor Drivers

## Detailed Description

Measuring operating voltage with the transceiver internal BATMON block.

## Functions

static uint8_t sensor_create_trxvtg | ( | void * | pdata | ) |
| static

Create an instance of a trxvtg sensor and initialize the sensor.

Returns
  sizeof(trxvtg_ctx_t)

Definition at line 129 of file trxvtg.h.