µracoli Manual Version foo

- µracoli
- User Guide
- Reference Guide

Boards and Modules

# any2400

Board #1: A.N. Solutions ANY Brick

Board any2400

Parameters

- Build Target: `any2400`
- Include file: `board_any.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, led, lm73, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# any2400st

Board #2: A.N. Solutions ANY Stick

Board any2400st

Parameters

- Build Target: `any2400st`
- Include file: `board_any.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# any900

Board #3: A.N. Solutions ANY Brick

Board any900

Parameters

- Build Target: `any900`
- Build Aliases: any2400
- Include file: `board_any.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, led, lm73, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# any900st

Board #4: A.N. Solutions ANY Stick

Board any900st

Parameters

- Build Target: `any900st`
- Build Aliases: any2400st
- Include file: `board_any.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# atrcb256rfr2xpro

Board #5: Atmel ATmega256RFR2 ZigBit Xplained Pro Extension

Board atrcb256rfr2xpro

Parameters

- Build Target: `atrcb256rfr2xpro`
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Provides: `hif, key, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# atzb256rfr2xpro

Board #6: Atmel ATmega256RFR2 ZigBit Xplained Pro Extension

Board atzb256rfr2xpro

Parameters

- Build Target: `atzb256rfr2xpro`
- Build Aliases: atrcb256rfr2xpro
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Provides: `hif, key, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# atzbx212bxpro

Board #7: Atmel ZigBit (Module, USB Stick, Xplained Pro Extension)

Board atzbx212bxpro

Parameters

- Build Target: `atzbx212bxpro`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# atzbx233usb

Board #8: Atmel ZigBit (Module, USB Stick, Xplained Pro Extension)

Board atzbx233usb

Parameters

- Build Target: `atzbx233usb`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3u`
- F_CPU: `32000000UL`
- Provides: `led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

rsensor, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_rtc, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# atzbx233xpro

Board #9: Atmel ZigBit (Module, USB Stick, Xplained Pro Extension)

Board atzbx233xpro

Parameters

- Build Target: `atzbx233xpro`
- Build Aliases: atzbx212bxpro
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# bat

Board #10: AirDMX remote node Bat, battery powered

Parameters

- Build Target: `bat`
- Include file: `board_airdmx.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0x9a:m -U efuse:w:0xfe:m`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# bitbean

Board #11: Colorado Micro Devices, BitBean (ZigBit ATZB-24-A2)

Board bitbean

Parameters

- Build Target: `bitbean`
- Include file: `board_wdba1281.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Fuses: `-U lfuse:w:0xe2:m -U hfuse:w:0x99:m -U efuse:w:0xff:m`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb212

Board #12: REB Controller Base Board with REB23x/REB212 attached

Board cbb212

Parameters

- Build Target: `cbb212`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb230

Board #13: REB Controller Base Board with REB23x/REB212 attached

Board cbb230

Parameters

- Build Target: `cbb230`
- Build Aliases: cbb230b, cbb231, cbb212, cbb232, cbb233
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb230b

Board #14: REB Controller Base Board with REB23x/REB212 attached

Board cbb230b

Parameters

- Build Target: `cbb230b`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb231

Board #15: REB Controller Base Board with REB23x/REB212 attached

Board cbb231

Parameters

- Build Target: `cbb231`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb232

Board #16: REB Controller Base Board with REB23x/REB212 attached

Board cbb232

Parameters

- Build Target: `cbb232`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# cbb233

Board #17: REB Controller Base Board with REB23x/REB212 attached

Board cbb233

Parameters

- Build Target: `cbb233`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega256a3`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, key, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derfa1

Board #18: Dresden Elektronik Radio Module deRFmega128-22A001

Board derfa1

Parameters

- Build Target: `derfa1`
- Include file: `board_derfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derfn128

Board #19: Dresden Elektronik Radio Module deRFmega128-22A/M{00} on deRFnode, USB

Board derfn128

Parameters

- Build Target: `derfn128`
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xc6:m -U hfuse:w:0x19:m -U efuse:w:0xfe:m`
- Provides: `hif, i2c, isl29020, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_isl29020, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derfn128u0

Board #20: Dresden Elektronik Radio Module deRFmega128-22A/M{00} on deRFnode, USB

Board derfn128u0

Parameters

- Build Target: `derfn128u0`
- Build Aliases: derfn128
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xc6:m -U hfuse:w:0x19:m -U efuse:w:0xfe:m`
- Provides: `hif, i2c, isl29020, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_isl29020, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derfn256u0

Board #21: Dresden Elektronik Radio Module deRFmega256-23M{00,10,12} on deRFnode, UART0 (X5)

Board derfn256u0

Parameters

- Build Target: `derfn256u0`
- Build Aliases: derfn256u0pa
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derfn256u0pa

Board #22: Dresden Elektronik Radio Module deRFmega256-23M{00,10,12} on deRFnode, UART0 (X5)

Board derfn256u0pa

Parameters

- Build Target: `derfn256u0pa`
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# derftorcbrfa1

Board #23: Dresden Elektronik deRFtoRCB Adapter for ATmega128RFA1

Board derftorcbrfa1

Parameters

- Build Target: `derftorcbrfa1`
- Include file: `board_rbbrfa1.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# dracula

Board #24: AirDMX gateway Dracula

Parameters

- Build Target: `dracula`
- Include file: `board_airdmx.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0x9a:m -U efuse:w:0xfe:m`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ibdt212

Board #25: IBDT212 Hardware

Board ibdt212

Parameters

- Build Target: `ibdt212`
- Include file: `board_ibdt.h`
- Baudrate: `38400`
- MMCU: `atmega644`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ibdt231

Board #26: IBDT231 Hardware

Board ibdt231

Parameters

- Build Target: `ibdt231`
- Include file: `board_ibdt.h`
- Baudrate: `38400`
- MMCU: `atmega644`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ibdt232

Board #27: IBDT232 Hardware

Board ibdt232

Parameters

- Build Target: `ibdt232`
- Include file: `board_ibdt.h`
- Baudrate: `38400`
- MMCU: `atmega644p`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# icm230_11

Board #28: In-Cirquit radio module, version 1.1, 1.2, AT86RF230a/b

Board icm230_11

Parameters

- Build Target: `icm230_11`
- Build Aliases: icm230_12a, icm230_12b
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# icm230_12a

Board #29: In-Cirquit radio module, version 1.1, 1.2, AT86RF230a/b

Board icm230_12a

Parameters

- Build Target: `icm230_12a`
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# icm230_12b

Board #30: In-Cirquit radio module, version 1.1, 1.2, AT86RF230a/b

Board icm230_12b

Parameters

- Build Target: `icm230_12b`
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# icm230_12c

Board #31: In-Cirquit radio stick/module, version 1.2a (RF230 RevB) [tarnished finish & AtMega128]

Board icm230_12c

Parameters

- Build Target: `icm230_12c`
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega128`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ics230_11

Board #32: In-Cirquit radio stick, version 1.1

Board ics230_11

Parameters

- Build Target: `ics230_11`
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ics230_12

Board #33: In-Cirquit radio stick/module, version 1.2a (RF230 RevB) [tarnished finish & AtMega128]

Board ics230_12

Parameters

- Build Target: `ics230_12`
- Build Aliases: icm230_12c
- Include file: `board_ict_11.h`
- Baudrate: `38400`
- MMCU: `atmega128`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ict230

Board #34: In-Cirquit radio stick/module, version 1.0

Board ict230

Parameters

- Build Target: `ict230`
- Include file: `board_ict230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# im240a

Board #35: IMST GmbH, WiMOD im240a Module

Board im240a

Parameters

- Build Target: `im240a`
- Include file: `board_wimod.h`
- Baudrate: `None`
- MMCU: `atmega328`
- F_CPU: `8000000UL`
- Fuses: `-U lfuse:w:0xe2:m -U hfuse:w:0xd4:m -U efuse:w:0x06:m`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# im240a_eval

Board #36: IMST GmbH, WiMOD im240a Development Board

Board im240a_eval

Parameters

- Build Target: `im240a_eval`
- Include file: `board_wimod.h`
- Baudrate: `None`
- MMCU: `atmega328`
- F_CPU: `8000000UL`
- Fuses: `-U lfuse:w:0xe2:m -U hfuse:w:0xd4:m -U efuse:w:0xfe:m`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# l3y

Board #37: 2564rfr2 low cost module

Parameters

- Build Target: `l3y`
- Include file: `board_derfa.h`
- Baudrate: `9600`
- MMCU: `atmega2564rfr2`
- F_CPU: `8000000UL`
- Fuses: `-U lfuse:w:0xe2:m -U hfuse:w:0x91:m -U efuse:w:0xfe:m`
- Provides: `hif, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# lgee231

Board #38: DIY Board by Daniel Thiele, w/ accelerometer, breakout board and UART.

Board lgee231

Parameters

- Build Target: `lgee231`
- Include file: `board_lgee.h`
- Baudrate: `None`
- MMCU: `atmega88`
- F_CPU: `8000000UL`
- Provides: `led, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# lgee231_v2

Board #39: DIY board by Daniel Thiele, w/ accelerometer, w/o breakout board.

Board lgee231_v2

Parameters

- Build Target: `lgee231_v2`
- Include file: `board_lgee.h`
- Baudrate: `None`
- MMCU: `atmega88`
- F_CPU: `8000000UL`
- Provides: `led, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# midgee

Board #40: IBDT Midgee

Parameters

- Build Target: `midgee`
- Include file: `board_midgee.h`
- Baudrate: `None`
- MMCU: `atmega88p`
- F_CPU: `8000000UL`
- Provides: `led, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# mnb900

Board #41: Meshnetics MeshBean WDB-A1281 and MNZB-900 development boards

Board mnb900

Parameters

- Build Target: `mnb900`
- Include file: `board_wdba1281.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `ds18b20, hif, i2c, led, lm73, mcu_vtg, ow, rtc, sensors, tmr, trx, trxvtg, tsl2550`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_ow, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret, xmpl_tsl2550

# muse231

Board #42: IBDT Multisensor Board

Board muse231

Parameters

- Build Target: `muse231`
- Include file: `board_muse231.h`
- Baudrate: `None`
- MMCU: `atmega88pa`
- F_CPU: `8000000UL`
- Provides: `led, mcu_vtg, sensors, sht21_rh, sht21_t, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# museII232

Board #43: IBDT MuseII ATmega88PA+AT86RF232

Parameters

- Build Target: `museII232`
- Include file: `board_museII232.h`
- Baudrate: `None`
- MMCU: `atmega328p`
- F_CPU: `8000000UL`
- Provides: `led, rtc, tmr, trx`

Applications

rsensor, wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_rtc, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# museIIrfa

Board #44: IBDT MuseII ATmega128RFA1

Parameters

- Build Target: `museIIrfa`
- Include file: `board_museIIrfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# pinoccio

Board #45: Pinoccio - the ecosystem for the internet of things

Board pinoccio

Parameters

- Build Target: `pinoccio`
- Include file: `board_derfa.h`
- Baudrate: `115200`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0xda:m -U efuse:w:0xf5:m`
- Provides: `hif, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk212

Board #46: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk212

Parameters

- Build Target: `psk212`
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk230

Board #47: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk230

Parameters

- Build Target: `psk230`
- Build Aliases: psk230b, psk231, psk212, psk232, psk233
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk230b

Board #48: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk230b

Parameters

- Build Target: `psk230b`
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk231

Board #49: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk231

Parameters

- Build Target: `psk231`
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk232

Board #50: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk232

Parameters

- Build Target: `psk232`
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# psk233

Board #51: Atmel Packet Sniffer Kit, STK541 with RCB for AT86RF{212,23x}

Board psk233

Parameters

- Build Target: `psk233`
- Include file: `board_stk541.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_vtg, rtc, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# radiofaro

Board #52: RadioFaro, Arduino like board with deRFmega128-22A001

Board radiofaro

Parameters

- Build Target: `radiofaro`
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0x9a:m -U efuse:w:0xfe:m`
- Provides: `hif, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx, trxvtg`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# radiofaro_v1

Board #53: RadioFaro, Arduino like board with deRFmega128-22A001

Board radiofaro_v1

Parameters

- Build Target: `radiofaro_v1`
- Include file: `board_derfa.h`
- Baudrate: `38400`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# raspbee

Board #54: Dresden Elektronik Raspberry Pi Module

Board raspbee

Parameters

- Build Target: `raspbee`
- Include file: `board_derfa.h`
- Baudrate: `38400`
- MMCU: `atmega256rfr2`
- F_CPU: `8000000UL`
- Provides: `hif, led, rtc, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ravrf230a

Board #55: Atmel Raven Board w/ AT86RF230A/B

Board ravrf230a

Parameters

- Build Target: `ravrf230a`
- Build Aliases: ravrf230b
- Include file: `board_ravrf.h`
- Baudrate: `9600`
- MMCU: `atmega1284p`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# ravrf230b

Board #56: Atmel Raven Board w/ AT86RF230A/B

Board ravrf230b

Parameters

- Build Target: `ravrf230b`
- Include file: `board_ravrf.h`
- Baudrate: `9600`
- MMCU: `atmega1284p`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb128rfa1

Board #57: Dresden Elektronik Breakout Board, with RCB for ATmega128RFA1

Board rbb128rfa1

Parameters

- Build Target: `rbb128rfa1`
- Include file: `board_rbbrfa1.h`
- Baudrate: `38400`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb212

Board #58: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb212

Parameters

- Build Target: `rbb212`
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb230

Board #59: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb230

Parameters

- Build Target: `rbb230`
- Build Aliases: rbb230b, rbb231, rbb212, rbb232, rbb233
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb230b

Board #60: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb230b

Parameters

- Build Target: `rbb230b`
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb231

Board #61: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb231

Parameters

- Build Target: `rbb231`
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb232

Board #62: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb232

Parameters

- Build Target: `rbb232`
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rbb233

Board #63: Dresden Elektronik Breakout Board with RCB for AT86RF{212,23x}

Board rbb233

Parameters

- Build Target: `rbb233`
- Include file: `board_rbb.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk212

Board #64: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk212

Parameters

- Build Target: `rdk212`
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk230

Board #65: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk230

Parameters

- Build Target: `rdk230`
- Build Aliases: rdk230b, rdk231, rdk212, rdk232, rdk233
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk230b

Board #66: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk230b

Parameters

- Build Target: `rdk230b`
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk231

Board #67: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk231

Parameters

- Build Target: `rdk231`
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk232

Board #68: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk232

Parameters

- Build Target: `rdk232`
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rdk233

Board #69: Radio Controller Board by Atmel and Dresden Elektronik
  with AT86RF{212,23x}

Board rdk233

Parameters

- Build Target: `rdk233`
- Include file: `board_rdk230.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rose231

Board #70: IBDT Rocket Sensor Board

Board rose231

Parameters

- Build Target: `rose231`
- Include file: `board_rose231.h`
- Baudrate: `None`
- MMCU: `atmega328p`
- F_CPU: `8000000UL`
- Provides: `hmc5883l, led, sensors, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# rzusb

Board #71: Atmel Raven USB Stick with AT86RF230 Rev. B

Board rzusb

Parameters

- Build Target: `rzusb`
- Include file: `board_rzusb.h`
- Baudrate: `None`
- MMCU: `at90usb1287`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# sparcrfa1

Board #72: Sparcfun RFA1 Dev. Board by J. Lindblom

Board sparcrfa1

Parameters

- Build Target: `sparcrfa1`
- Include file: `board_derfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xff:m -U hfuse:w:0xda:m -U efuse:w:0xf5:m`
- Provides: `hif, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb128rfa1

Board #73: Dresden Elektronik Sensor Terminal Board with RCB128RFA1

Parameters

- Build Target: `stb128rfa1`
- Include file: `board_stbrfa1.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb212

Board #74: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb212

Parameters

- Build Target: `stb212`
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb230

Board #75: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb230

Parameters

- Build Target: `stb230`
- Build Aliases: stb230b, stb231, stb212, stb232, stb233
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb230b

Board #76: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb230b

Parameters

- Build Target: `stb230b`
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb231

Board #77: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb231

Parameters

- Build Target: `stb231`
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb232

Board #78: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb232

Parameters

- Build Target: `stb232`
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb233

Board #79: Dresden Elektronik Sensor Terminal Board with RCB for AT86RF{212,23x}

Board stb233

Parameters

- Build Target: `stb233`
- Include file: `board_stb.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, key, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stb256rfr2

Board #80: Sensor Terminal Board with Atmel RCB256RFR2 Radio Controller Board

Parameters

- Build Target: `stb256rfr2`
- Include file: `board_stbrfa1.h`
- Baudrate: `None`
- MMCU: `atmega256rfr2`
- F_CPU: `8000000UL`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stkm16

Board #81: STK500 with ATmega16 and AT86RF230 radio extender board

Board stkm16

Parameters

- Build Target: `stkm16`
- Include file: `board_stkm16.h`
- Baudrate: `115200`
- MMCU: `atmega16`
- F_CPU: `3686400UL`
- Fuses: `-U lfuse:w:0xef:m -U hfuse:w:0x91:m`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# stkm8

Board #82: STK500 with ATmega8 and AT86RF230 radio extender board

Board stkm8

Parameters

- Build Target: `stkm8`
- Include file: `board_stkm8.h`
- Baudrate: `None`
- MMCU: `atmega8`
- F_CPU: `8000000UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, selftest, testlib, wgpio, wibo, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# tiny230

Board #83: DIY Board by Joerg Wunsch with ATtiny(44,84) and AT86RF(230,231)

Board tiny230

Parameters

- Build Target: `tiny230`
- Build Aliases: tiny231
- Include file: `board_tiny230.h`
- Baudrate: `None`
- MMCU: `attiny84`
- F_CPU: `8000000UL`
- Provides: `led, ledps, sensors, tmr, trx`

Applications

wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# tiny231

Board #84: DIY Board by Joerg Wunsch with ATtiny(44,84) and AT86RF(230,231)

Board tiny231

Parameters

- Build Target: `tiny231`
- Include file: `board_tiny230.h`
- Baudrate: `None`
- MMCU: `attiny84`
- F_CPU: `8000000UL`
- Provides: `led, ledps, sensors, tmr, trx`

Applications

wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# wdba1281

Board #85: Meshnetics MeshBean WDB-A1281 and MNZB-900 development boards

Board wdba1281

Parameters

- Build Target: `wdba1281`
- Build Aliases: mnb900
- Include file: `board_wdba1281.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `ds18b20, hif, i2c, led, lm73, mcu_vtg, ow, rtc, sensors, tmr, trx, trxvtg, tsl2550`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_ow, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret, xmpl_tsl2550

# wprog

Board #86: WProg

Parameters

- Build Target: `wprog`
- Include file: `board_derfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `8000000UL`
- Provides: `hif, led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# xma1u233xpro

Board #87: Atmel ZigBit ATZB-RF-233-1-C XPRO Extension connected to XMEGA A1U Xplained Pro

Parameters

- Build Target: `xma1u233xpro`
- Include file: `board_cbb2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega128a1u`
- F_CPU: `8000000UL`
- Provides: `keys, led, mcu_vtg, rtc, sensors, tmr, trx`

Applications

rsensor, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_rtc, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# xme5rz212

Board #88: Atmel RZ600 Stick plugged on J1 of Xmega-E5 Xplained

Parameters

- Build Target: `xme5rz212`
- Include file: `board_xme5rz2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega32e5`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, keys, led, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# xme5rz230

Board #89: Atmel RZ600 Stick plugged on J1 of Xmega-E5 Xplained

Parameters

- Build Target: `xme5rz230`
- Build Aliases: xme5rz231, xme5rz212
- Include file: `board_xme5rz2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega32e5`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, keys, led, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# xme5rz231

Board #90: Atmel RZ600 Stick plugged on J1 of Xmega-E5 Xplained

Parameters

- Build Target: `xme5rz231`
- Include file: `board_xme5rz2xx.h`
- Baudrate: `38400`
- MMCU: `atxmega32e5`
- F_CPU: `8000000UL`
- Provides: `hif, i2c, keys, led, mcu_vtg, sensors, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# xxo

Board #91: Tic-Tac-Toe Hardware for Chemnitzer Linuxtage 2012

Parameters

- Build Target: `xxo`
- Include file: `board_derfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `1000000UL`
- Fuses: `-U lfuse:w:0x62:m -U hfuse:w:0x18:m -U efuse:w:0xfe:m`
- Provides: `led, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

wibo, wibotest

Examples

xmpl_dbg, xmpl_leds, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbh212

Board #92: ATZGB.com evaluation board

Board zgbh212

Parameters

- Build Target: `zgbh212`
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `7372800UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbh230

Board #93: ATZGB.com evaluation board

Board zgbh230

Parameters

- Build Target: `zgbh230`
- Build Aliases: zgbh231, zgbh212
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `7372800UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbh231

Board #94: ATZGB.com evaluation board

Board zgbh231

Parameters

- Build Target: `zgbh231`
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `7372800UL`
- Provides: `hif, led, tmr, trx`

Applications

diag, rdiag, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbl212

Board #95: ATZGB.com radio modules

Board zgbl212

Parameters

- Build Target: `zgbl212`
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `trx`

Applications

Examples

xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbl230

Board #96: ATZGB.com radio modules

Board zgbl230

Parameters

- Build Target: `zgbl230`
- Build Aliases: zgbl231, zgbl212
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `trx`

Applications

Examples

xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbl231

Board #97: ATZGB.com radio modules

Board zgbl231

Parameters

- Build Target: `zgbl231`
- Include file: `board_zgbl.h`
- Baudrate: `None`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `trx`

Applications

Examples

xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbt1281a2nouart

Board #98: Meshnetics Zigbit A2, no UART

Board zgbt1281a2nouart

Parameters

- Build Target: `zgbt1281a2nouart`
- Include file: `board_zgbta2.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `tmr, trx`

Applications

Examples

xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbt1281a2uart0

Board #99: Meshnetics Zigbit A2, using UART0 (via ISP connector)

Board zgbt1281a2uart0

Parameters

- Build Target: `zgbt1281a2uart0`
- Include file: `board_zgbta2.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zgbt1281a2uart1

Board #100: Meshnetics Zigbit A2, using UART1

Board zgbt1281a2uart1

Parameters

- Build Target: `zgbt1281a2uart1`
- Include file: `board_zgbta2.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `hif, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# zigduino

Board #101: Zigduino made by Logos Electromechanical LLC

Board zigduino

Parameters

- Build Target: `zigduino`
- Include file: `board_derfa.h`
- Baudrate: `None`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xff:m -U hfuse:w:0xda:m -U efuse:w:0xf5:m`
- Provides: `hif, mcu_t, mcu_vtg, sensors, tmr, trx`

Applications

selftest, sniffer, testlib, wibohost, wuart

Examples

xmpl_hif, xmpl_hif_echo, xmpl_sensor, xmpl_timer, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret