at86rf231.h
Go to the documentation of this file.

    00001 /* THIS FILE IS GENERATED by ds2reg.py FROM INPUT Templates/at86rf231.txt */
    00002
    00003 /* Copyright (c) 2008 Axel Wachtler
    00004    All rights reserved.
    00005
    00006    Redistribution and use in source and binary forms, with or without
    00007    modification, are permitted provided that the following conditions
    00008    are met:
    00009
    00010    * Redistributions of source code must retain the above copyright
    00011      notice, this list of conditions and the following disclaimer.
    00012    * Redistributions in binary form must reproduce the above copyright
    00013      notice, this list of conditions and the following disclaimer in the
    00014      documentation and/or other materials provided with the distribution.
    00015    * Neither the name of the authors nor the names of its contributors
    00016      may be used to endorse or promote products derived from this software
    00017      without specific prior written permission.
    00018
    00019    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00020    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00021    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00022    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00023    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00024    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00025    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00026    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00027    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00028    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00029    POSSIBILITY OF SUCH DAMAGE. */
    00030
    00031 /* $Id$ */
    00036 #ifndef AT86RF231_H
    00037 #define AT86RF231_H (1)
    00038
    00039 /* === Includes ============================================================== */
    00040
    00041 /* === Externals ============================================================= */
    00042
    00043 /* === Types ================================================================= */
    00044
    00045 typedef uint8_t trx_ramaddr_t;
    00046 typedef uint8_t trx_regval_t;
    00047 typedef uint8_t trx_regaddr_t;
    00048
    00049 /* === Macros ================================================================ */
    00051 #define RG_TRX_STATUS (0x1)
    00052
    00053   #define SR_CCA_DONE 0x1,0x80,7
    00054
    00055   #define SR_CCA_STATUS 0x1,0x40,6
    00056
    00057   #define SR_TRX_STATUS 0x1,0x1f,0
    00058     #define P_ON (0)
    00059     #define BUSY_RX (1)
    00060     #define BUSY_TX (2)
    00061     #define RX_ON (6)
    00062     #define TRX_OFF (8)
    00063     #define PLL_ON (9)
    00064     #define TRX_SLEEP (15)
    00065     #define BUSY_RX_AACK (17)
    00066     #define BUSY_TX_ARET (18)
    00067     #define RX_AACK_ON (22)
    00068     #define TX_ARET_ON (25)
    00069     #define RX_ON_NOCLK (28)
    00070     #define RX_AACK_ON_NOCLK (29)
    00071     #define BUSY_RX_AACK_NOCLK (30)
    00072
    00073 #define RG_TRX_STATE (0x2)
    00074
    00075   #define SR_TRAC_STATUS 0x2,0xe0,5
    00076     #define TRAC_SUCCESS (0)
    00077     #define TRAC_SUCCESS_DATA_PENDING (1)
    00078     #define TRAC_SUCCESS_WAIT_FOR_ACK (2)
    00079     #define TRAC_CHANNEL_ACCESS_FAILURE (3)
    00080     #define TRAC_NO_ACK (5)
    00081     #define TRAC_INVALID (7)
    00082
    00083   #define SR_TRX_CMD 0x2,0x1f,0
    00084     #define CMD_NOP (0)
    00085     #define CMD_TX_START (2)
    00086     #define CMD_FORCE_TRX_OFF (3)
    00087     #define CMD_RX_ON (6)
    00088     #define CMD_TRX_OFF (8)
    00089     #define CMD_PLL_ON (9)
    00090     #define CMD_RX_AACK_ON (22)
    00091     #define CMD_TX_ARET_ON (25)
    00092
    00093 #define RG_TRX_CTRL_0 (0x3)
    00094
    00095   #define SR_PAD_IO 0x3,0xe0,5
    00096
    00097   #define SR_PAD_IO_CLKM 0x3,0x10,4
    00098     #define CLKM_2mA (0)
    00099     #define CLKM_4mA (1)
    00100     #define CLKM_6mA (2)
    00101     #define CLKM_8mA (3)
    00102
    00103   #define SR_CLKM_SHA_SEL 0x3,0x8,3
    00104
    00105   #define SR_CLKM_CTRL 0x3,0x7,0
    00106     #define CLKM_no_clock (0)
    00107     #define CLKM_1MHz (1)
    00108     #define CLKM_2MHz (2)
    00109     #define CLKM_4MHz (3)
    00110     #define CLKM_8MHz (4)
    00111     #define CLKM_16MHz (5)
    00112
    00113 #define RG_TRX_CTRL_1 (0x4)
    00114
    00115   #define SR_PA_EXT_EN 0x4,0x80,7
    00116
    00117   #define SR_IRQ_2_EXT_EN 0x4,0x40,6
    00118
    00119   #define SR_TX_AUTO_CRC_ON 0x4,0x20,5
    00120
    00121   #define SR_RX_BL_CTRL 0x4,0x10,4
    00122
    00123   #define SR_SPI_CMD_MODE 0x4,0xc,2
    00124
    00125   #define SR_IRQ_POLARITY 0x4,0x1,0
    00126
    00127   #define SR_IRQ_MASK_MODE 0x4,0x2,1
    00128
    00129 #define RG_PHY_TX_PWR (0x5)
    00130
    00131   #define SR_PA_BUF_LT 0x5,0xc0,6
    00132
    00133   #define SR_PA_LT 0x5,0x30,4
    00134
    00135   #define SR_TX_PWR 0x5,0xf,0
    00136
    00137 #define RG_PHY_RSSI (0x6)
    00138
    00139   #define SR_RX_CRC_VALID 0x6,0x80,7
    00140
    00141   #define SR_RND_VALUE 0x6,0x60,5
    00142
    00143   #define SR_RSSI 0x6,0x1f,0
    00144
    00145 #define RG_PHY_ED_LEVEL (0x7)
    00146
    00147   #define SR_ED_LEVEL 0x7,0xff,0
    00148
    00149 #define RG_PHY_CC_CCA (0x8)
    00150
    00151   #define SR_CCA_REQUEST 0x8,0x80,7
    00152
    00153   #define SR_CCA_MODE 0x8,0x60,5
    00154
    00155   #define SR_CHANNEL 0x8,0x1f,0
    00156
    00157 #define RG_CCA_THRES (0x9)
    00158
    00159   #define SR_CCA_ED_THRES 0x9,0xf,0
    00160
    00161 #define RG_RX_CTRL (0xa)
    00162
    00163   #define SR_PDT_THRES 0xa,0xf,0
    00164
    00165 #define RG_SFD_VALUE (0xb)
    00166
    00167   #define SR_SFD_VALUE 0xb,0xff,0
    00168
    00169 #define RG_TRX_CTRL_2 (0xc)
    00170
    00171   #define SR_RX_SAFE_MODE 0xc,0x80,7
    00172
    00173   #define SR_OQPSK_DATA_RATE 0xc,0x3,0
    00174
    00175 #define RG_ANT_DIV (0xd)
    00176
    00177   #define SR_ANT_SEL 0xd,0x80,7
    00178
    00179   #define SR_ANT_DIV_EN 0xd,0x8,3
    00180
    00181   #define SR_ANT_EXT_SW_EN 0xd,0x4,2
    00182
    00183   #define SR_ANT_CTRL 0xd,0x3,0
    00184
    00185 #define RG_IRQ_MASK (0xe)
    00186
    00187   #define SR_MASK_BAT_LOW 0xe,0x80,7
    00188
    00189   #define SR_MASK_TRX_UR 0xe,0x40,6
    00190
    00191   #define SR_MASK_AMI 0xe,0x20,5
    00192
    00193   #define SR_MASK_CCA_ED_READY 0xe,0x10,4
    00194
    00195   #define SR_MASK_TRX_END 0xe,0x8,3
    00196
    00197   #define SR_MASK_TRX_START 0xe,0x4,2
    00198
    00199   #define SR_MASK_PLL_LOCK 0xe,0x1,0
    00200
    00201   #define SR_MASK_PLL_UNLOCK 0xe,0x2,1
    00202
    00203 #define RG_IRQ_STATUS (0xf)
    00204
    00205   #define SR_BAT_LOW 0xf,0x80,7
    00206
    00207   #define SR_TRX_UR 0xf,0x40,6
    00208
    00209   #define SR_AMI 0xf,0x20,5
    00210
    00211   #define SR_CCA_ED_READY 0xf,0x10,4
    00212
    00213   #define SR_RX_END 0xf,0x8,3
    00214
    00215   #define SR_RX_START 0xf,0x4,2
    00216
    00217   #define SR_PLL_LOCK 0xf,0x1,0
    00218
    00219   #define SR_PLL_UNLOCK 0xf,0x2,1
    00220
    00221 #define RG_VREG_CTRL (0x10)
    00222
    00223   #define SR_AVREG_EXT 0x10,0x80,7
    00224
    00225   #define SR_AVDD_OK 0x10,0x40,6
    00226
    00227   #define SR_DVREG_EXT 0x10,0x8,3
    00228
    00229   #define SR_DVDD_OK 0x10,0x4,2
    00230
    00231 #define RG_BATMON (0x11)
    00232
    00233   #define SR_BATMON_OK 0x11,0x20,5
    00234
    00235   #define SR_BATMON_HR 0x11,0x10,4
    00236
    00237   #define SR_BATMON_VTH 0x11,0xf,0
    00238
    00239 #define RG_XOSC_CTRL (0x12)
    00240
    00241   #define SR_XTAL_MODE 0x12,0xf0,4
    00242
    00243   #define SR_XTAL_TRIM 0x12,0xf,0
    00244
    00245 #define RG_RX_SYN (0x15)
    00246
    00247   #define SR_RX_PDT_DIS 0x15,0x80,7
    00248
    00249   #define SR_RX_PDT_LEVEL 0x15,0xf,0
    00250
    00251 #define RG_XAH_CTRL_1 (0x17)
    00252
    00253   #define SR_AACK_FLTR_RES_FT 0x17,0x20,5
    00254
    00255   #define SR_AACK_UPLD_RES_FT 0x17,0x10,4
    00256
    00257   #define SR_AACK_ACK_TIME 0x17,0x4,2
    00258
    00259   #define SR_AACK_PROM_MODE 0x17,0x2,1
    00260
    00261 #define RG_FTN_CTRL (0x18)
    00262
    00263   #define SR_FTN_START 0x18,0x80,7
    00264
    00265 #define RG_PLL_CF (0x1a)
    00266
    00267   #define SR_PLL_CF_START 0x1a,0x80,7
    00268
    00269 #define RG_PLL_DCU (0x1b)
    00270
    00271   #define SR_PLL_DCU_START 0x1b,0x80,7
    00272
    00273 #define RG_PART_NUM (0x1c)
    00274
    00275   #define SR_PART_NUM 0x1c,0xff,0
    00276     #define RF231A_PART_NUM (3)
    00277
    00278 #define RG_VERSION_NUM (0x1d)
    00279
    00280   #define SR_VERSION_NUM 0x1d,0xff,0
    00281     #define RF231A_VERSION_NUM (2)
    00282
    00283 #define RG_MAN_ID_0 (0x1e)
    00284
    00285   #define SR_MAN_ID_0 0x1e,0xff,0
    00286
    00287 #define RG_MAN_ID_1 (0x1f)
    00288
    00289   #define SR_MAN_ID_1 0x1f,0xff,0
    00290
    00291 #define RG_SHORT_ADDR_0 (0x20)
    00292
    00293   #define SR_SHORT_ADDR_0 0x20,0xff,0
    00294
    00295 #define RG_SHORT_ADDR_1 (0x21)
    00296
    00297   #define SR_SHORT_ADDR_1 0x21,0xff,0
    00298
    00299 #define RG_PAN_ID_0 (0x22)
    00300
    00301   #define SR_PAN_ID_0 0x22,0xff,0
    00302
    00303 #define RG_PAN_ID_1 (0x23)
    00304
    00305   #define SR_PAN_ID_1 0x23,0xff,0
    00306
    00307 #define RG_IEEE_ADDR_0 (0x24)
    00308
    00309   #define SR_IEEE_ADDR_0 0x24,0xff,0
    00310
    00311 #define RG_IEEE_ADDR_1 (0x25)
    00312
    00313   #define SR_IEEE_ADDR_1 0x25,0xff,0
    00314
    00315 #define RG_IEEE_ADDR_2 (0x26)
    00316
    00317   #define SR_IEEE_ADDR_2 0x26,0xff,0
    00318
    00319 #define RG_IEEE_ADDR_3 (0x27)
    00320
    00321   #define SR_IEEE_ADDR_3 0x27,0xff,0
    00322
    00323 #define RG_IEEE_ADDR_4 (0x28)
    00324
    00325   #define SR_IEEE_ADDR_4 0x28,0xff,0
    00326
    00327 #define RG_IEEE_ADDR_5 (0x29)
    00328
    00329   #define SR_IEEE_ADDR_5 0x29,0xff,0
    00330
    00331 #define RG_IEEE_ADDR_6 (0x2a)
    00332
    00333   #define SR_IEEE_ADDR_6 0x2a,0xff,0
    00334
    00335 #define RG_IEEE_ADDR_7 (0x2b)
    00336
    00337   #define SR_IEEE_ADDR_7 0x2b,0xff,0
    00338
    00339 #define RG_XAH_CTRL_0 (0x2c)
    00340
    00341   #define SR_MAX_FRAME_RETRES 0x2c,0xf0,4
    00342
    00343   #define SR_SLOTTED_OPERATION 0x2c,0x1,0
    00344
    00345   #define SR_MAX_CSMA_RETRES 0x2c,0xe,1
    00346
    00347 #define RG_CSMA_SEED_0 (0x2d)
    00348
    00349   #define SR_CSMA_SEED_0 0x2d,0xff,0
    00350
    00351 #define RG_CSMA_SEED_1 (0x2e)
    00352
    00353   #define SR_AACK_FVN_MODE 0x2e,0xc0,6
    00354
    00355   #define SR_AACK_SET_PD 0x2e,0x20,5
    00356
    00357   #define SR_AACK_DIS_ACK 0x2e,0x10,4
    00358
    00359   #define SR_AACK_I_AM_COORD 0x2e,0x8,3
    00360
    00361   #define SR_CSMA_SEED_1 0x2e,0x7,0
    00362
    00363 #define RG_CSMA_BE (0x2f)
    00364
    00365   #define SR_MAX_BE 0x2f,0xf0,4
    00366
    00367   #define SR_MIN_BE 0x2f,0xf,0
    00368
    00369 #define RADIO_NAME "AT86RF231"
    00370
    00371 #define RADIO_PART_NUM (RF231A_PART_NUM)
    00372
    00373 #define RADIO_VERSION_NUM (RF231A_VERSION_NUM)
    00374
    00376 #define TRX_CMD_RW           (_BV(7) | _BV(6))
    00377
    00378 #define TRX_CMD_RR           (_BV(7))
    00379
    00380 #define TRX_CMD_FW           (_BV(6) | _BV(5))
    00381
    00382 #define TRX_CMD_FR           (_BV(5))
    00383
    00384 #define TRX_CMD_SW           (_BV(6))
    00385
    00386 #define TRX_CMD_SR           (0)
    00387
    00388 #define TRX_CMD_RADDR_MASK   (0x3f)
    00389
    00391 #define TRX_RESET_TIME_US    (6)
    00392
    00394 #define TRX_INIT_TIME_US     (510)
    00395
    00397 #define TRX_PLL_LOCK_TIME_US     (180)
    00398
    00399
    00401 #define TRX_CCA_TIME_US     (140)
    00402
    00404 #define TRX_IRQ_PLL_LOCK   _BV(0)
    00405
    00407 #define TRX_IRQ_PLL_UNLOCK _BV(1)
    00408
    00410 #define TRX_IRQ_RX_START   _BV(2)
    00411
    00413 #define TRX_IRQ_TRX_END    _BV(3)
    00414
    00416 #define TRX_IRQ_CCA_ED     _BV(4)
    00417
    00419 #define TRX_IRQ_AMI        _BV(5)
    00420
    00422 #define TRX_IRQ_UR         _BV(6)
    00423
    00425 #define TRX_IRQ_BAT_LOW    _BV(7)
    00426
    00428 #define TRAC_SUCCESS (0)
    00429
    00430 #define TRAC_CHANNEL_ACCESS_FAILURE (3)
    00431
    00432 #define TRAC_NO_ACK (5)
    00433
    00434
    00436 #define TRX_MIN_CHANNEL (11)
    00437
    00439 #define TRX_MAX_CHANNEL (26)
    00440
    00442 #define TRX_NB_CHANNELS (16)
    00443
    00448 #define TRX_SUPPORTED_CHANNELS  (0x7fff800UL)
    00449
    00450 #define TRX_SUPPORTS_BAND_2400 (1)
    00451
    00455 #define TRX_SUPPORTED_PAGES     (42)
    00456
    00458 #define TRX_OQPSK250  (0)
    00459
    00461 #define TRX_OQPSK500  (1)
    00462
    00464 #define TRX_OQPSK1000 (2)
    00465
    00466 #define TRX_OQPSK2000 (3)
    00467
    00468 #define TRX_NONE      (255)
    00469
    00470 #endif /* ifndef AT86RF231_H */