Defines
board_airdmx.h File Reference
Board Definitions | Board Definitions

AirDMX boards for wireless DMX control. More...

Go to the source code of this file.

## Defines
#define | DMX_ADDR_MASK_B (0xEF)
#define | DMX_ADDR_MASK_D (0x03)
#define | DMX_DRIVER_INIT() do{ PORTE &= ~(1<<PE2); DDRE |= (1<<PE2); }while(0)
#define | DMX_DRIVER_TX_DISABLE() do{ PORTE &= ~(1<<PE2); }while(0)
#define | DMX_DRIVER_TX_ENABLE() do{ PORTE |= (1<<PE2); }while(0)
#define | HIF_TYPE HIF_UART_1
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL)
#define | HWTMR_PRESCALE (1)
#define | LED_DDR DDRG
#define | LED_MASK (0x06)
#define | LED_NUMBER (2)
#define | LED_PORT PORTG
#define | LED_SHIFT (1)
#define | LEDS_INVERSE (0)
#define | NO_KEYS (1)
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_OVF_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_RESET_HIGH() do { TRXPR |= _BV(TRXRST); } while (0)
#define | TRX_RESET_LOW() do { TRXPR &= ~_BV(TRXRST); } while (0)
#define | TRX_SLPTR_HIGH() do { TRXPR |= _BV(SLPTR); } while (0)
#define | TRX_SLPTR_LOW() do { TRXPR &= ~_BV(SLPTR); } while (0)
#define | TRX_TSTAMP_REG TCNT1

## Detailed Description

AirDMX boards for wireless DMX control.

    Fuses/Locks:
         LF: 0xC6 - 16Mhz transceiver Osc. 258CLK+4.1ms
         HF: 0x11 - without boot loader
         HF: 0x10 - with boot loader
         EF: 0xff
         LOCK: 0xef - protection of boot section

    Bootloader:
        Start at byte=0x1e000, address=0xf000, size = 4096 instructions/ 8192 bytes

    radiofaro:
      LEDS: PG1, PG2

Build Options

- dracula : the DMX master board
- bat : the DMX slave board

## Define Documentation

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= (_BV(CS10)); \
            TIMSK1 |= _BV(TOIE1); \
        }while(0)

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event