Data Fields
node_config_t Struct Reference
Board Definitions

## Data Fields
uint8_t | _reserved_ [2]
uint8_t | channel
uint8_t | crc
uint64_t | ieee_addr
uint16_t | pan_id
uint16_t | short_addr

## Detailed Description

Structure for preconfigured constants that are stored at FLASHEND in programm memory or in the EEPROM.

See also get_node_config(), get_node_config_eeprom() and store_node_config_eeprom().

## Field Documentation

uint8_t node_config_t::_reserved_[2]

For future extensions, but can be used to store user data.

uint8_t node_config_t::channel

The radio channel.

uint8_t node_config_t::crc

Ibutton CRC to validate if the structure is correct.

uint64_t node_config_t::ieee_addr

The MAC address of the node (EUI64).

uint16_t node_config_t::pan_id

The PAN ID (network ID) of the node.

uint16_t node_config_t::short_addr

The short address of the node.