Defines | Functions | Variables
wgpio.c File Reference
Wireless GPIO Application

Implementation of the Wireless GPIO Application. More...

## Defines
#define | AWAKE_TIME MSEC(1000)
## Functions
int | main (void)
void | TRX_IRQ_vect ()
## Variables
actor_ctx_t | ActorCtx
volatile uint8_t | KeyEvent = 0
uint8_t | Led1Blnk = 0
volatile uint16_t | TmoCounter = 0
volatile uint8_t | TmoEvent = 0
volatile event_t | TrxEvent
volatile app_state_t | TrxState

## Detailed Description

Implementation of the Wireless GPIO Application.

This is a Wireless General Purpose IO Application a.k.a. a light switch application.

The application can run in two modes:

- (MP) mains powered : In this mode the receiver always on.
- (RC) remote control: Battery powered remote control with power down on idle.

Note:
  The RC mode can be eanbled on those boards, where the the control key is wired with an interrupt pin of the MCU. All boards with memory mapped keys are not capable of entering the RC mode.

With a long key press, you get into the configuration mode, where the status LED blinks 3 times and the Actor LED displays the current operation mode:

- ActorLed on : MP mode (reset value)
- ActorLed off : RC mode.

## Function Documentation

int main | ( | void |  | ) |

Main function of WGPIO application.

void TRX_IRQ_vect | ( |  | ) |

Transceiver IRQ routine. Application specific timer IRQ routine. used to read key status (debounced).