Data Structures | Defines | Typedefs
const.h File Reference

General Definitions. More...

Go to the source code of this file.

## Data Structures
struct | trx_param_t
## Defines
#define | BOARD_ANY2400 (1)
#define | BOARD_ANY2400ST (2)
#define | BOARD_ANY900 (3)
#define | BOARD_ANY900ST (4)
#define | BOARD_BAT (5)
#define | BOARD_BITBEAN (6)
#define | BOARD_CBB212 (7)
#define | BOARD_CBB230 (8)
#define | BOARD_CBB230B (9)
#define | BOARD_CBB231 (10)
#define | BOARD_CBB232 (11)
#define | BOARD_CBB233 (12)
#define | BOARD_DERFA1 (13)
#define | BOARD_DERFA2 (91)
#define | BOARD_DERFA2P (92)
#define | BOARD_DERFTORCBRFA1 (14)
#define | BOARD_DRACULA (15)
#define | BOARD_IBDT212 (16)
#define | BOARD_IBDT231 (17)
#define | BOARD_IBDT232 (18)
#define | BOARD_ICM230_11 (19)
#define | BOARD_ICM230_12A (20)
#define | BOARD_ICM230_12B (21)
#define | BOARD_ICM230_12C (22)
#define | BOARD_ICS230_11 (23)
#define | BOARD_ICS230_12 (24)
#define | BOARD_ICT230 (25)
#define | BOARD_IM240A (26)
#define | BOARD_IM240A_EVAL (27)
#define | BOARD_LAST (BOARD_RASPBEE)
#define | BOARD_LGEE231 (28)
#define | BOARD_LGEE231_V2 (29)
#define | BOARD_MIDGEE (30)
#define | BOARD_MNB900 (31)
#define | BOARD_MUSE231 (32)
#define | BOARD_MUSEII232 (33)
#define | BOARD_MUSEIIRFA (34)
#define | BOARD_NONE (0)
#define | BOARD_PINOCCIO (35)
#define | BOARD_PSK212 (36)
#define | BOARD_PSK230 (37)
#define | BOARD_PSK230B (38)
#define | BOARD_PSK231 (39)
#define | BOARD_PSK232 (40)
#define | BOARD_PSK233 (41)
#define | BOARD_RADIOFARO (42)
#define | BOARD_RADIOFARO_V1 (43)
#define | BOARD_RASPBEE (86)
#define | BOARD_RAVRF230A (44)
#define | BOARD_RAVRF230B (45)
#define | BOARD_RBB128RFA1 (46)
#define | BOARD_RBB212 (47)
#define | BOARD_RBB230 (48)
#define | BOARD_RBB230B (49)
#define | BOARD_RBB231 (50)
#define | BOARD_RBB232 (51)
#define | BOARD_RBB233 (52)
#define | BOARD_RDK212 (53)
#define | BOARD_RDK230 (54)
#define | BOARD_RDK230B (55)
#define | BOARD_RDK231 (56)
#define | BOARD_RDK232 (57)
#define | BOARD_RDK233 (58)
#define | BOARD_ROSE231 (59)
#define | BOARD_RZUSB (60)
#define | BOARD_STB128RFA1 (61)
#define | BOARD_STB212 (62)
#define | BOARD_STB230 (63)
#define | BOARD_STB230B (64)
#define | BOARD_STB231 (65)
#define | BOARD_STB232 (66)
#define | BOARD_STB233 (67)
#define | BOARD_STB256RFR2 (85)
#define | BOARD_STKM16 (68)
#define | BOARD_STKM8 (69)
#define | BOARD_TINY230 (70)
#define | BOARD_TINY231 (71)
#define | BOARD_WDBA1281 (72)
#define | BOARD_WPROG (73)
#define | BOARD_XXO (74)
#define | BOARD_ZGBH212 (75)
#define | BOARD_ZGBH230 (76)
#define | BOARD_ZGBH231 (77)
#define | BOARD_ZGBL212 (78)
#define | BOARD_ZGBL230 (79)
#define | BOARD_ZGBL231 (80)
#define | BOARD_ZGBT1281A2NOUART (81)
#define | BOARD_ZGBT1281A2UART0 (82)
#define | BOARD_ZGBT1281A2UART1 (83)
#define | BOARD_ZIGDUINO (84)
#define | FCTL_ACK _BV(5)
#define | FCTL_DATA _BV(0)
#define | FCTL_DST_LONG 0x0c00
#define | FCTL_DST_MASK (FCTL_DST_LONG)
#define | FCTL_DST_SHORT 0x0800
#define | FCTL_IPAN _BV(6)
#define | FCTL_IPAN_MASK (FCTL_IPAN)
#define | FCTL_SRC_LONG 0xc000
#define | FCTL_SRC_MASK (FCTL_SRC_LONG)
#define | FCTL_SRC_SHORT 0x8000
#define | HIF_AT90USB (21)
#define | HIF_FT245 (20)
#define | HIF_NONE (0)
#define | HIF_UART_0 (10)
#define | HIF_UART_1 (11)
#define | MOD_BPSK_20 (0)
#define | MOD_BPSK_40 (1)
#define | MOD_OQPSK_100 (2)
#define | MOD_OQPSK_1000 (7)
#define | MOD_OQPSK_200 (3)
#define | MOD_OQPSK_2000 (8)
#define | MOD_OQPSK_250 (4)
#define | MOD_OQPSK_400 (5)
#define | MOD_OQPSK_500 (6)
#define | RADIO_AT86RF212 (4)
#define | RADIO_AT86RF230 (1)
#define | RADIO_AT86RF230A (RADIO_AT86RF230)
#define | RADIO_AT86RF230B (2)
#define | RADIO_AT86RF231 (3)
#define | RADIO_AT86RF232 (9)
#define | RADIO_AT86RF233 (10)
#define | RADIO_ATMEGA128RFA1_A (5)
#define | RADIO_ATMEGA128RFA1_B (6)
#define | RADIO_ATMEGA128RFA1_C (7)
#define | RADIO_ATMEGA128RFA1_D (8)
#define | RADIO_ATMEGA256RFR2 (11)
#define | RADIO_BAND_2400 (4)
#define | RADIO_BAND_700 (1)
#define | RADIO_BAND_800 (2)
#define | RADIO_BAND_900 (3)
#define | SENSOR_MCU_T (1)
#define | SENSOR_MCU_VTG (2)
#define | SENSOR_SHT21_RH (3)
#define | SENSOR_SHT21_T (4)
#define | SHORTENUM
#define | SPI_RATE_1_128 (3)
#define | SPI_RATE_1_16 (1)
#define | SPI_RATE_1_2 (4)
#define | SPI_RATE_1_32 (6)
#define | SPI_RATE_1_4 (0)
#define | SPI_RATE_1_64 (2)
#define | SPI_RATE_1_8 (5)
#define | URACOLI_USB_BCD_RELEASE (0x100)
#define | URACOLI_USB_PID (2183)
#define | URACOLI_USB_PRODUCT_NAME L"RZUSBSTICK"
#define | URACOLI_USB_VENDOR_NAME L"URACOLI"
#define | URACOLI_USB_VID (5824)
## Typedefs
typedef uint8_t | ccamode_t
typedef int8_t | channel_t
typedef bool | rxidle_t
typedef int8_t | txpwr_t

## Detailed Description

General Definitions.

## Define Documentation

#define SHORTENUM

macro that forces an enumeration to use 8 bit instead of 16 bit integers.