Defines
board_wimod.h File Reference
Board Definitions | Board Definitions

IMST GmbH WIMOD w/ mega328 and AT86RF230B. More...

Go to the source code of this file.

## Defines
#define | BOARD_WIMOD_H (1)
#define | DDR_KEY DDRC
#define | DDR_SPI (DDRB)
#define | DDR_TRX_RESET DDRD
#define | DDR_TRX_SLPTR DDRB
#define | DEFAULT_SPI_RATE (SPI_RATE_1_2)
#define | DI_TRX_IRQ() {TIMSK1 &= ~_BV(ICIE1);}
#define | EI_TRX_IRQ() {TIMSK1 |= _BV(ICIE1);}
#define | HIF_TYPE HIF_UART_0
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL)
#define | HWTMR_PRESCALE (1)
#define | INVERSE_KEYS (1)
#define | LED_DDR DDRD
#define | LED_MASK (0x1c)
#define | LED_NUMBER (3)
#define | LED_PORT PORTD
#define | LED_SHIFT (2)
#define | LEDS_INVERSE (1)
#define | MASK_KEY (0x07)
#define | MASK_TRX_RESET (_BV(PD6))
#define | MASK_TRX_SLPTR (_BV(PB1))
#define | PIN_KEY PINC
#define | PORT_KEY PORTC
#define | PORT_SPI (PORTB)
#define | PORT_TRX_RESET PORTD
#define | PORT_TRX_SLPTR PORTB
#define | PULLUP_KEYS (1)
#define | RADIO_TYPE (RADIO_AT86RF230B)
#define | SHIFT_KEY (0)
#define | SPI_DATA_REG SPDR
#define | SPI_MISO _BV(PB4)
#define | SPI_MOSI _BV(PB3)
#define | SPI_SCK _BV(PB5)
#define | SPI_SELN_HIGH() PORT_SPI |= SPI_SS; SREG = sreg
#define | SPI_SELN_LOW() uint8_t sreg = SREG; cli(); PORT_SPI &=~SPI_SS
#define | SPI_SS _BV(PB2)
#define | SPI_WAITFOR() do { while((SPSR & _BV(SPIF)) == 0);} while(0)
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_OVF_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_IRQ_INIT()
#define | TRX_IRQ_vect TIMER1_CAPT_vect
#define | TRX_RESET_HIGH() PORT_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_INIT() DDR_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_LOW() PORT_TRX_RESET &= ~MASK_TRX_RESET
#define | TRX_SLPTR_HIGH() PORT_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_INIT() DDR_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_LOW() PORT_TRX_SLPTR &= ~MASK_TRX_SLPTR
#define | TRX_TSTAMP_REG TCNT1

## Detailed Description

IMST GmbH WIMOD w/ mega328 and AT86RF230B.

see http://www.mikrocontroller.net/attachment/101618/WiMOD240.jpg

The wiring of the radio and the ATmega is shown below.

         AVR         RF230
         ---         -----
         PB0    <--  INT / ICP1
         PB1    -->  SLPTR
         PB2    -->  /SEL
         PB3    -->  MOSI
         PB4    <--  MISO
         PB5    -->  SCK

         PB6 intentionally unused for XTAL1
         PB7 intentionally unused for XTAL2

        (T1) PD5   <--  CLKM
             PD6   --> /RST
             PD7   --> TST

        USART:
            PD0 RXD
            PD1 TXD

        LED:  None
        KEY:  None

      IM240A      Mega328  Adapter   EvalBoard
      Pin Name              AB_01
      -----------------------------------------
       8  ADC1    ADC7      X1.12
       9  ADC2    ADC6      X1.14
      12  GPIO1   PC0       X1.15     Button1
      13  GPIO2   PC1       X1.16     Button2
      14  GPIO3   PC2       X1.19     Button3
      15  GPIO4   PC3       X1.18     DSW1
      21  GPIO5   PC5       X2.9
      23  GPIO6   PC4       X2.11

      18  DIO1    PD0       X2.18      UART-RX
      19  DIO2    PD1       X2.15      UART-TX
      20  DIO3    PD2       X2.7       LED4
      24  DIO4    PD3       X2.6       LED3
      25  DIO5    PD4       X2.5       LED2

Build Options

- im240a : AT86RF230B w/ mega328.
- im240a_eval : AT86RF230B w/ mega328 eval board.

Note:
  In order to use the eval board be shure to follow the install guide.
  - replace jumper e by cable e1 on X5
  - switch S1 to power supply USB.

To program the mega328pa connect JTAG-ICE 10 pin header to X4.

avrdude -P usb -c jtag2isp -p m328p -B10 -t

The original fuses are LF 0xe2 HF 0xd4 EF 0x06

The original bootloader seems to be a proprietary one and handles the ISMT *.wfi format. It is a one line string starting with "WIMOD_ID_3#" followed by probably the ASCII representation of the firmware ... to be investigated.

In order to do a backup of the board use the following commands:

        avrdude -P usb -c jtag2isp -p m328p -B 10 -U fl:r:im240a_flash_initial.hex:i
        avrdude -P usb -c jtag2isp -p m328p -B 10 -U ee:r:im240a_eeprom_initial.hex:i

Restoration of the backup can be done by the command:

      avrdude -P usb -c jtag2isp -p m328p -B 10 \
                -U fl:w:im240a_flash_initial.hex:i \
                -U ee:w:im240a_eeprom_initial.hex:i \
                -U lf:w:0xe2:m \
                -U hf:w:0xd4:m \
                -U ef:w:0x06:m

## Define Documentation

#define DI_TRX_IRQ | ( |  | ) | {TIMSK1 &= ~_BV(ICIE1);}

disable TRX interrupt

#define EI_TRX_IRQ | ( |  | ) | {TIMSK1 |= _BV(ICIE1);}

enable TRX interrupt

#define HWTMR_PRESCALE (1)

Mode: normal Prescaler: 1 Overflow: 0xFFFFUL

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= (_BV(CS10)); \
            TIMSK1 |= _BV(TOIE1); \
        }while(0)

#define TRX_IRQ_INIT | ( |  | ) |

Value:

    do{\
                                /* TCCR1B |= (_BV(ICNC1) | _BV(ICES1) | _BV(CS12) | _BV(CS10)); */\
                                TCCR1B |= (_BV(ICNC1) | _BV(ICES1));\
                                TIFR1 = _BV(ICF1);\
                              } while(0)

init interrupt handling

- transceiver IRQ at PB0
- rising edge triggers ICP1 (ICES1),
- timer capture is enabled (ICF1)

#define TRX_IRQ_vect TIMER1_CAPT_vect

interrupt vector name

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event