Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - s -

- SCAN : sniffer.h
- SCAN_DONE : sniffer.h
- scan_init() : sniffer_scan.c , sniffer.h
- scan_update_status() : sniffer.c , sniffer_scan.c
- send_continous() : diagradio.c
- send_frame() : diagradio.c
- set_next_cca() : diagradio.c
- set_next_channel() : diagradio.c
- set_next_pwr() : diagradio.c
- SET_PARM_FAILED : radio.h
- SHIFT_KEY : board_dummy.h , board_ibdt.h , board_tiny230.h
- SHORTENUM : const.h
- show_statistic() : diagradio.c
- SLEEP_ON_IDLE : board.h
- SNIFF : sniffer.h
- sniffer_init() : sniffer.c
- sniffer_start() : sniffer.c , sniffer.h
- sniffer_state_t : sniffer.h
- sniffer_stop() : sniffer.c , sniffer.h
- SPI_DATA_REG : board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h , board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_lgee.h , board_midgee.h
- SPI_MISO : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_MOSI : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_RATE_1_128 : const.h
- SPI_RATE_1_16 : const.h
- SPI_RATE_1_2 : const.h
- SPI_RATE_1_32 : const.h
- SPI_RATE_1_4 : const.h
- SPI_RATE_1_64 : const.h
- SPI_RATE_1_8 : const.h
- SPI_SCK : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_SELN_HIGH : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_lgee.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_SELN_LOW : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_lgee.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_SS : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SPI_WAITFOR : board_cbb2xx.h , board_dummy.h , board_ibdt.h , board_ict230.h , board_lgee.h , board_midgee.h , board_muse231.h , board_museII232.h , board_ravrf.h , board_rose231.h , board_stkt26.h , board_tiny230.h
- SR_AACK_ACK_TIME : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_DIS_ACK : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_FLTR_RES_FT : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_FVN_MODE : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_I_AM_COORD : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_PROM_MODE : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_SET_PD : at86rf212.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_AACK_UPLD_RES_FT : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AMI : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_ANT_CTRL : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_ANT_DIV_EN : at86rf231.h , atmega_rfa1.h
- SR_ANT_EXT_SW_EN : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_ANT_SEL : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_AVDD_OK : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_AVREG_EXT : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_BAND : at86rf212.h
- SR_BAT_LOW : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_BATMON_HR : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_BATMON_OK : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_BATMON_VTH : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_BPSK_OQPSK : at86rf212.h
- SR_CC_ : at86rf212.h
- SR_CC_BAND : at86rf212.h
- SR_CC_NUMBER : at86rf212.h
- SR_CCA_DONE : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CCA_ED_READY : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_CCA_ED_THRES : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CCA_MODE : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CCA_REQUEST : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CCA_STATUS : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CHANNEL : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CLKM_CTRL : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CLKM_SHA_SEL : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CSMA_LBT_MODE : at86rf212.h
- SR_CSMA_SEED_0 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_CSMA_SEED_1 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_DVDD_OK : at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h , at86rf212.h
- SR_DVREG_EXT : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_ED_LEVEL : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_FTN_START : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_GC_PA : at86rf212.h
- SR_GC_TX_OFFS : at86rf212.h
- SR_IEEE_ADDR_0 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_IEEE_ADDR_1 : at86rf231.h , at86rf212.h , at86rf230a.h , at86rf230b.h , atmega_rfa1.h
- SR_IEEE_ADDR_2 : at86rf230b.h , at86rf212.h , at86rf230a.h , at86rf231.h , atmega_rfa1.h
- SR_IEEE_ADDR_3 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_IEEE_ADDR_4 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_IEEE_ADDR_5 : at86rf231.h , at86rf212.h , at86rf230a.h , at86rf230b.h , atmega_rfa1.h
- SR_IEEE_ADDR_6 : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_IEEE_ADDR_7 : at86rf212.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h , at86rf230a.h
- SR_IRQ_2_EXT_EN : at86rf231.h , atmega_rfa1.h , at86rf212.h
- SR_IRQ_MASK_MODE : at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_IRQ_POLARITY : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_MAN_ID_0 : at86rf212.h , at86rf230a.h , at86rf230b.h , atmega_rfa1.h , at86rf231.h
- SR_MAN_ID_1 : at86rf212.h , at86rf230a.h , at86rf231.h , atmega_rfa1.h , at86rf230b.h
- SR_MASK_AMI : at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_MASK_BAT_LOW : at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h
- SR_MASK_CCA_ED_READY : at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_MASK_PLL_LOCK : at86rf212.h , at86rf230a.h , at86rf231.h , atmega_rfa1.h , at86rf230b.h
- SR_MASK_PLL_UNLOCK : at86rf212.h , at86rf230b.h , at86rf231.h , atmega_rfa1.h , at86rf230a.h
- SR_MASK_RX_START : at86rf212.h
- SR_MASK_TRX_END : at86rf212.h , at86rf230a.h , at86rf230b.h , atmega_rfa1.h , at86rf231.h
- SR_MASK_TRX_START : at86rf230a.h , at86rf230b.h , atmega_rfa1.h , at86rf231.h
- SR_MASK_TRX_UR : at86rf230b.h , at86rf212.h , at86rf230a.h , at86rf231.h , atmega_rfa1.h
- SR_MAX_BE : at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_MAX_CSMA_RETRES : at86rf231.h , atmega_rfa1.h
- SR_MAX_CSMA_RETRIES : at86rf212.h , at86rf230b.h , at86rf230a.h
- SR_MAX_FRAME_RETRES : atmega_rfa1.h , at86rf231.h
- SR_MAX_FRAME_RETRIES : at86rf212.h , at86rf230a.h , at86rf230b.h
- SR_MIN_BE : atmega_rfa1.h , at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h
- SR_OQPSK_DATA_RATE : atmega_rfa1.h , at86rf231.h , at86rf212.h
- SR_PA_BOOST : at86rf212.h
- SR_PA_BUF_LT : at86rf231.h , atmega_rfa1.h
- SR_PA_EXT_EN : at86rf231.h , at86rf212.h , atmega_rfa1.h
- SR_PA_LT : atmega_rfa1.h , at86rf212.h , at86rf231.h
- SR_PAD_IO : at86rf231.h , at86rf230b.h , at86rf212.h , at86rf230a.h , atmega_rfa1.h
- SR_PAD_IO_CLKM : at86rf230b.h , at86rf231.h , at86rf212.h , at86rf230a.h , atmega_rfa1.h
- SR_PAN_ID_0 : at86rf231.h , atmega_rfa1.h , at86rf230a.h , at86rf212.h , at86rf230b.h
- SR_PAN_ID_1 : atmega_rfa1.h , at86rf212.h , at86rf230a.h , at86rf230b.h , at86rf231.h
- SR_PART_NUM : at86rf231.h , at86rf230a.h , at86rf230b.h , at86rf212.h , atmega_rfa1.h
- SR_PDT_THRES : at86rf231.h , atmega_rfa1.h
- SR_PLL_CF_START : at86rf212.h , at86rf231.h , at86rf230b.h , atmega_rfa1.h , at86rf230a.h
- SR_PLL_DCU_START : at86rf230b.h , at86rf212.h , at86rf230a.h , atmega_rfa1.h , at86rf231.h
- SR_PLL_LOCK : at86rf231.h , atmega_rfa1.h , at86rf230a.h , at86rf230b.h , at86rf212.h
- SR_PLL_UNLOCK : at86rf212.h , at86rf230b.h , atmega_rfa1.h , at86rf231.h , at86rf230a.h
- SR_RF_MC : at86rf212.h
- SR_RND_VALUE : at86rf231.h , at86rf212.h , atmega_rfa1.h
- SR_RSSI : at86rf231.h , atmega_rfa1.h , at86rf212.h , at86rf230a.h , at86rf230b.h
- SR_RX_BL_CTRL : atmega_rfa1.h , at86rf231.h , at86rf212.h
- SR_RX_CRC_VALID : at86rf212.h , at86rf231.h , atmega_rfa1.h , at86rf230b.h
- SR_RX_END : at86rf230a.h , at86rf230b.h , atmega_rfa1.h , at86rf231.h
- SR_RX_PDT_DIS : at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_RX_PDT_LEVEL : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_RX_SAFE_MODE : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_RX_START : at86rf230b.h , at86rf231.h , at86rf230a.h , at86rf212.h , atmega_rfa1.h
- SR_SFD_VALUE : at86rf212.h , at86rf231.h , atmega_rfa1.h
- SR_SHORT_ADDR_0 : at86rf231.h , at86rf230b.h , atmega_rfa1.h , at86rf230a.h , at86rf212.h
- SR_SHORT_ADDR_1 : at86rf212.h , at86rf230a.h , at86rf231.h , at86rf230b.h , atmega_rfa1.h
- SR_SLOTTED_OPERATION : at86rf231.h , at86rf212.h , atmega_rfa1.h
- SR_SPI_CMD_MODE : atmega_rfa1.h , at86rf212.h , at86rf231.h
- SR_SUB_MODE : at86rf212.h
- SR_TRAC_STATUS : at86rf212.h , atmega_rfa1.h , at86rf231.h , at86rf230a.h , at86rf230b.h
- SR_TRX_CMD : atmega_rfa1.h , at86rf231.h , at86rf230a.h , at86rf230b.h , at86rf212.h
- SR_TRX_END : at86rf212.h
- SR_TRX_OFF_AVDD_EN : at86rf212.h
- SR_TRX_STATUS : at86rf230a.h , at86rf231.h , at86rf230b.h , at86rf212.h , atmega_rfa1.h
- SR_TRX_UR : atmega_rfa1.h , at86rf230b.h , at86rf212.h , at86rf230a.h , at86rf231.h
- SR_TX_AUTO_CRC_ON : at86rf230b.h , atmega_rfa1.h , at86rf212.h , at86rf230a.h , at86rf231.h
- SR_TX_PWR : at86rf230b.h , at86rf230a.h , at86rf212.h , atmega_rfa1.h , at86rf231.h
- SR_VERSION_NUM : at86rf230b.h , at86rf231.h , at86rf212.h , atmega_rfa1.h , at86rf230a.h
- SR_XTAL_MODE : atmega_rfa1.h , at86rf230a.h , at86rf231.h , at86rf230b.h , at86rf212.h
- SR_XTAL_TRIM : atmega_rfa1.h , at86rf230a.h , at86rf212.h , at86rf231.h , at86rf230b.h
- STATE_OFF : radio.h
- STATE_RX : radio.h
- STATE_RXAUTO : radio.h
- STATE_SET_FAILED : radio.h
- STATE_SLEEP : radio.h
- STATE_TX : radio.h
- STATE_TXAUTO : radio.h
- SUCCESS : radio.h
- SW_VERSION : wuart.c