at86rf230a.h
Go to the documentation of this file.

    00001 /* THIS FILE IS GENERATED by ds2reg.py FROM INPUT Templates/at86rf230a.txt */
    00002
    00003 /* Copyright (c) 2008 Axel Wachtler
    00004    All rights reserved.
    00005
    00006    Redistribution and use in source and binary forms, with or without
    00007    modification, are permitted provided that the following conditions
    00008    are met:
    00009
    00010    * Redistributions of source code must retain the above copyright
    00011      notice, this list of conditions and the following disclaimer.
    00012    * Redistributions in binary form must reproduce the above copyright
    00013      notice, this list of conditions and the following disclaimer in the
    00014      documentation and/or other materials provided with the distribution.
    00015    * Neither the name of the authors nor the names of its contributors
    00016      may be used to endorse or promote products derived from this software
    00017      without specific prior written permission.
    00018
    00019    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00020    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00021    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00022    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00023    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00024    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00025    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00026    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00027    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00028    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00029    POSSIBILITY OF SUCH DAMAGE. */
    00030
    00031 /* $Id$ */
    00036 #ifndef AT86RF230A_H
    00037 #define AT86RF230A_H (1)
    00038
    00039 /* === Includes ============================================================== */
    00040
    00041 /* === Externals ============================================================= */
    00042
    00043 /* === Types ================================================================= */
    00044
    00045 typedef uint8_t trx_ramaddr_t;
    00046 typedef uint8_t trx_regval_t;
    00047 typedef uint8_t trx_regaddr_t;
    00048
    00049 /* === Macros ================================================================ */
    00051 #define RG_TRX_STATUS (0x1)
    00052
    00053   #define SR_CCA_DONE 0x1,0x80,7
    00054
    00055   #define SR_CCA_STATUS 0x1,0x40,6
    00056
    00057   #define SR_TRX_STATUS 0x1,0x1f,0
    00058     #define P_ON (0)
    00059     #define BUSY_RX (1)
    00060     #define BUSY_TX (2)
    00061     #define RX_ON (6)
    00062     #define TRX_OFF (8)
    00063     #define PLL_ON (9)
    00064     #define TRX_SLEEP (15)
    00065     #define BUSY_RX_AACK (17)
    00066     #define BUSY_TX_ARET (18)
    00067     #define RX_AACK_ON (22)
    00068     #define TX_ARET_ON (25)
    00069     #define RX_ON_NOCLK (28)
    00070     #define RX_AACK_ON_NOCLK (29)
    00071     #define BUSY_RX_AACK_NOCLK (30)
    00072
    00073 #define RG_TRX_STATE (0x2)
    00074
    00075   #define SR_TRAC_STATUS 0x2,0xe0,5
    00076     #define TRAC_SUCCESS (0)
    00077     #define TRAC_CHANNEL_ACCESS_FAILURE (3)
    00078     #define TRAC_NO_ACK (5)
    00079
    00080   #define SR_TRX_CMD 0x2,0x1f,0
    00081     #define CMD_NOP (0)
    00082     #define CMD_TX_START (2)
    00083     #define CMD_FORCE_TRX_OFF (3)
    00084     #define CMD_RX_ON (6)
    00085     #define CMD_TRX_OFF (8)
    00086     #define CMD_PLL_ON (9)
    00087     #define CMD_RX_AACK_ON (22)
    00088     #define CMD_TX_ARET_ON (25)
    00089
    00090 #define RG_TRX_CTRL_0 (0x3)
    00091
    00092   #define SR_PAD_IO 0x3,0xc0,6
    00093
    00094   #define SR_PAD_IO_CLKM 0x3,0x30,4
    00095     #define CLKM_2mA (0)
    00096     #define CLKM_4mA (1)
    00097     #define CLKM_6mA (2)
    00098     #define CLKM_8mA (3)
    00099
    00100   #define SR_CLKM_SHA_SEL 0x3,0x8,3
    00101
    00102   #define SR_CLKM_CTRL 0x3,0x7,0
    00103     #define CLKM_no_clock (0)
    00104     #define CLKM_1MHz (1)
    00105     #define CLKM_2MHz (2)
    00106     #define CLKM_4MHz (3)
    00107     #define CLKM_8MHz (4)
    00108     #define CLKM_16MHz (5)
    00109
    00110 #define RG_PHY_TX_PWR (0x5)
    00111
    00112   #define SR_TX_AUTO_CRC_ON 0x5,0x80,7
    00113
    00114   #define SR_TX_PWR 0x5,0xf,0
    00115
    00116 #define RG_PHY_RSSI (0x6)
    00117
    00118   #define SR_RSSI 0x6,0x1f,0
    00119
    00120 #define RG_PHY_ED_LEVEL (0x7)
    00121
    00122   #define SR_ED_LEVEL 0x7,0xff,0
    00123
    00124 #define RG_PHY_CC_CCA (0x8)
    00125
    00126   #define SR_CCA_REQUEST 0x8,0x80,7
    00127
    00128   #define SR_CCA_MODE 0x8,0x60,5
    00129
    00130   #define SR_CHANNEL 0x8,0x1f,0
    00131
    00132 #define RG_CCA_THRES (0x9)
    00133
    00134   #define SR_CCA_ED_THRES 0x9,0xf,0
    00135
    00136 #define RG_IRQ_MASK (0xe)
    00137
    00138   #define SR_MASK_BAT_LOW 0xe,0x80,7
    00139
    00140   #define SR_MASK_TRX_UR 0xe,0x40,6
    00141
    00142   #define SR_MASK_TRX_END 0xe,0x8,3
    00143
    00144   #define SR_MASK_TRX_START 0xe,0x4,2
    00145
    00146   #define SR_MASK_PLL_LOCK 0xe,0x1,0
    00147
    00148   #define SR_MASK_PLL_UNLOCK 0xe,0x2,1
    00149
    00150 #define RG_IRQ_STATUS (0xf)
    00151
    00152   #define SR_BAT_LOW 0xf,0x80,7
    00153
    00154   #define SR_TRX_UR 0xf,0x40,6
    00155
    00156   #define SR_RX_END 0xf,0x8,3
    00157
    00158   #define SR_RX_START 0xf,0x4,2
    00159
    00160   #define SR_PLL_LOCK 0xf,0x1,0
    00161
    00162   #define SR_PLL_UNLOCK 0xf,0x2,1
    00163
    00164 #define RG_VREG_CTRL (0x10)
    00165
    00166   #define SR_AVREG_EXT 0x10,0x80,7
    00167
    00168   #define SR_AVDD_OK 0x10,0x40,6
    00169
    00170   #define SR_DVREG_EXT 0x10,0x8,3
    00171
    00172   #define SR_DVDD_OK 0x10,0x4,2
    00173
    00174 #define RG_BATMON (0x11)
    00175
    00176   #define SR_BATMON_OK 0x11,0x20,5
    00177
    00178   #define SR_BATMON_HR 0x11,0x10,4
    00179
    00180   #define SR_BATMON_VTH 0x11,0xf,0
    00181
    00182 #define RG_XOSC_CTRL (0x12)
    00183
    00184   #define SR_XTAL_MODE 0x12,0xf0,4
    00185
    00186   #define SR_XTAL_TRIM 0x12,0xf,0
    00187
    00188 #define RG_PLL_CF (0x1a)
    00189
    00190   #define SR_PLL_CF_START 0x1a,0x80,7
    00191
    00192 #define RG_PLL_DCU (0x1b)
    00193
    00194   #define SR_PLL_DCU_START 0x1b,0x80,7
    00195
    00196 #define RG_PART_NUM (0x1c)
    00197
    00198   #define SR_PART_NUM 0x1c,0xff,0
    00199     #define RF230A_PART_NUM (2)
    00200
    00201 #define RG_VERSION_NUM (0x1d)
    00202
    00203   #define SR_VERSION_NUM 0x1d,0xff,0
    00204     #define RF230A_VERSION_NUM (1)
    00205
    00206 #define RG_MAN_ID_0 (0x1e)
    00207
    00208   #define SR_MAN_ID_0 0x1e,0xff,0
    00209
    00210 #define RG_MAN_ID_1 (0x1f)
    00211
    00212   #define SR_MAN_ID_1 0x1f,0xff,0
    00213
    00214 #define RG_SHORT_ADDR_0 (0x20)
    00215
    00216   #define SR_SHORT_ADDR_0 0x20,0xff,0
    00217
    00218 #define RG_SHORT_ADDR_1 (0x21)
    00219
    00220   #define SR_SHORT_ADDR_1 0x21,0xff,0
    00221
    00222 #define RG_PAN_ID_0 (0x22)
    00223
    00224   #define SR_PAN_ID_0 0x22,0xff,0
    00225
    00226 #define RG_PAN_ID_1 (0x23)
    00227
    00228   #define SR_PAN_ID_1 0x23,0xff,0
    00229
    00230 #define RG_IEEE_ADDR_0 (0x24)
    00231
    00232   #define SR_IEEE_ADDR_0 0x24,0xff,0
    00233
    00234 #define RG_IEEE_ADDR_1 (0x25)
    00235
    00236   #define SR_IEEE_ADDR_1 0x25,0xff,0
    00237
    00238 #define RG_IEEE_ADDR_2 (0x26)
    00239
    00240   #define SR_IEEE_ADDR_2 0x26,0xff,0
    00241
    00242 #define RG_IEEE_ADDR_3 (0x27)
    00243
    00244   #define SR_IEEE_ADDR_3 0x27,0xff,0
    00245
    00246 #define RG_IEEE_ADDR_4 (0x28)
    00247
    00248   #define SR_IEEE_ADDR_4 0x28,0xff,0
    00249
    00250 #define RG_IEEE_ADDR_5 (0x29)
    00251
    00252   #define SR_IEEE_ADDR_5 0x29,0xff,0
    00253
    00254 #define RG_IEEE_ADDR_6 (0x2a)
    00255
    00256   #define SR_IEEE_ADDR_6 0x2a,0xff,0
    00257
    00258 #define RG_IEEE_ADDR_7 (0x2b)
    00259
    00260   #define SR_IEEE_ADDR_7 0x2b,0xff,0
    00261
    00262 #define RG_XAH_CTRL (0x2c)
    00263
    00264   #define SR_MAX_FRAME_RETRIES 0x2c,0xf0,4
    00265
    00266   #define SR_MAX_CSMA_RETRIES 0x2c,0xe,1
    00267
    00268 #define RG_CSMA_SEED_0 (0x2d)
    00269
    00270   #define SR_CSMA_SEED_0 0x2d,0xff,0
    00271
    00272 #define RG_CSMA_SEED_1 (0x2e)
    00273
    00274   #define SR_MIN_BE 0x2e,0xc0,6
    00275
    00276   #define SR_AACK_I_AM_COORD 0x2e,0x8,3
    00277
    00278   #define SR_CSMA_SEED_1 0x2e,0x7,0
    00279
    00280 #define RADIO_NAME "AT86RF230A"
    00281
    00282 #define RADIO_PART_NUM (RF230A_PART_NUM)
    00283
    00284 #define RADIO_VERSION_NUM (RF230A_VERSION_NUM)
    00285
    00286
    00288 #define TRX_CMD_RW           (_BV(7) | _BV(6))
    00289
    00290 #define TRX_CMD_RR           (_BV(7))
    00291
    00292 #define TRX_CMD_FW           (_BV(6) | _BV(5))
    00293
    00294 #define TRX_CMD_FR           (_BV(5))
    00295
    00296 #define TRX_CMD_SW           (_BV(6))
    00297
    00298 #define TRX_CMD_SR           (0)
    00299
    00300 #define TRX_CMD_RADDR_MASK   (0x3f)
    00301
    00303 #define TRX_RESET_TIME_US    (6)
    00304
    00306 #define TRX_INIT_TIME_US     (510)
    00307
    00309 #define TRX_PLL_LOCK_TIME_US     (180)
    00310
    00312 #define TRX_CCA_TIME_US     (140)
    00313
    00315 #define TRX_IRQ_PLL_LOCK   _BV(0)
    00316
    00318 #define TRX_IRQ_PLL_UNLOCK _BV(1)
    00319
    00321 #define TRX_IRQ_RX_START   _BV(2)
    00322
    00324 #define TRX_IRQ_TRX_END    _BV(3)
    00325
    00327 #define TRX_IRQ_UR         _BV(6)
    00328
    00330 #define TRX_IRQ_BAT_LOW    _BV(7)
    00331
    00333 #define TRX_MIN_CHANNEL (11)
    00334
    00336 #define TRX_MAX_CHANNEL (26)
    00337
    00339 #define TRX_NB_CHANNELS (16)
    00340
    00345 #define TRX_SUPPORTED_CHANNELS  (0x7fff800UL)
    00346
    00350 #define TRX_SUPPORTED_MODULATIONS (MODULATION_OQPSK_250)
    00351
    00356 #define TRX_SUPPORTED_PAGES     (42)
    00357
    00358 #define TRX_SUPPORTS_BAND_2400 (1)
    00359
    00361 #define TRX_OQPSK250  (0)
    00362
    00364 #define TRX_NONE      (255)
    00365
    00366 #endif /* ifndef AT86RF230A_H */