Defines | Typedefs | Enumerations | Functions
transceiver.h File Reference
Transceiver Access Functions

Interface for Transceiver Access Functions. More...

Go to the source code of this file.

## Defines
#define | BPSK20 (0x52)
#define | BPSK20_STR "BPSK20"
#define | BPSK40 (0x92)
#define | BPSK40_STR "BPSK40"
#define | DEFAULT_SPI_RATE (0)
#define | INVALID_PART_NUM (2)
#define | INVALID_REV_NUM (1)
#define | MAX_FRAME_SIZE (127)
#define | OQPSK100 (0x90)
#define | OQPSK1000 (0x34)
#define | OQPSK1000_STR "OQPSK1000"
#define | OQPSK100_STR "OQPSK100"
#define | OQPSK200 (0x93)
#define | OQPSK2000 (0x54)
#define | OQPSK2000_STR "OQPSK2000"
#define | OQPSK200_STR "OQPSK200"
#define | OQPSK250 (0x33)
#define | OQPSK250_STR "OQPSK250"
#define | OQPSK400 (0x95)
#define | OQPSK400_STR "OQPSK400"
#define | OQPSK500 (0x94)
#define | OQPSK500_STR "OQPSK500"
#define | RATE_NONE (0xFF)
#define | TRX_INIT_FAIL (1)
#define | TRX_IRQ_AMI_DI() trx_bit_write(SR_MASK_AMI, 0);
| Disable AMI IRQ.
#define | TRX_IRQ_AMI_EI() trx_bit_write(SR_MASK_AMI, 1);
| Enable AMI IRQ.
#define | TRX_IRQ_BAT_LOW_DI() trx_bit_write(SR_MASK_BAT_LOW, 0);
| Disable BAT_LOW IRQ.
#define | TRX_IRQ_BAT_LOW_EI() trx_bit_write(SR_MASK_BAT_LOW, 1);
| Enable BAT_LOW IRQ.
#define | TRX_IRQ_CCA_ED_READY_DI() trx_bit_write(SR_MASK_CCA_ED_READY, 0);
| Disable CCA_ED_READY IRQ.
#define | TRX_IRQ_CCA_ED_READY_EI() trx_bit_write(SR_MASK_CCA_ED_READY, 1);
| Enable CCA_ED_READY IRQ.
#define | TRX_IRQ_PLL_UNLOCK_DI() trx_bit_write(SR_MASK_PLL_UNLOCK, 0);
| Disable PLL_UNLOCK IRQ.
#define | TRX_IRQ_PLL_UNLOCK_EI() trx_bit_write(SR_MASK_PLL_UNLOCK, 1);
| Enable PLL_UNLOCK IRQ.
#define | TRX_IRQ_RX_START_DI() trx_bit_write(SR_MASK_RX_START, 0);
| Disable RX_START IRQ.
#define | TRX_IRQ_RX_START_EI() trx_bit_write(SR_MASK_RX_START, 1);
| Enable RX_START IRQ.
#define | TRX_IRQ_TRX_IRQ_END_DI() trx_bit_write(SR_MASK_TRX_IRQ_END, 0);
| Disable TRX_IRQ_END IRQ.
#define | TRX_IRQ_TRX_IRQ_END_EI() trx_bit_write(SR_MASK_TRX_IRQ_END, 1);
| Enable TRX_IRQ_END IRQ.
#define | TRX_IRQ_TRX_IRQ_START_DI() trx_bit_write(SR_MASK_TRX_IRQ_START, 0);
| Disable TRX_IRQ_START IRQ.
#define | TRX_IRQ_TRX_IRQ_START_EI() trx_bit_write(SR_MASK_TRX_IRQ_START, 1);
| Enable TRX_IRQ_START IRQ.
#define | TRX_IRQ_UR_DI() trx_bit_write(SR_MASK_UR, 0);
| Disable TX/RX underun IRQ.
#define | TRX_IRQ_UR_EI() trx_bit_write(SR_MASK_UR, 1);
| Enable TX/RX underun IRQ.
#define | TRX_NEXT_CHANNEL(x) ((channel_t)(x+1) > TRX_MAX_CHANNEL ? TRX_MAX_CHANNEL : x+1)
#define | TRX_NEXT_CHANNEL_WRAP(x) ((channel_t)(x+1) > TRX_MAX_CHANNEL ? TRX_MIN_CHANNEL : x+1 )
#define | TRX_OK (0)
#define | TRX_PLL_FAIL (2)
#define | TRX_PREV_CHANNEL(x) ((channel_t)(x-1) < TRX_MIN_CHANNEL ? TRX_MIN_CHANNEL : x-1)
#define | TRX_PREV_CHANNEL_WRAP(x) ((channel_t)(x-1) < TRX_MIN_CHANNEL ? TRX_MAX_CHANNEL : x-1 )
## Typedefs
typedef void(* | trx_irq_handler_t )(uint8_t cause)
typedef uint8_t | trx_ramaddr_t
typedef uint8_t | trx_regaddr_t
typedef uint8_t | trx_regval_t
## Enumerations
enum | trx_cfg_t { CFG_FLASH, CFG_EEPROM, CFG_NONE }
## Functions
trx_regval_t | trx_bit_read (trx_regaddr_t addr, trx_regval_t mask, uint8_t pos)
| subregister read
void | trx_bit_write (trx_regaddr_t addr, trx_regval_t mask, uint8_t pos, trx_regval_t value)
| subregister write
uint8_t | trx_decode_datarate (uint8_t rhash, char *rstr, uint8_t nlen)
| Decodes a hash value and returns a datarate string pointer.
void * | trx_decode_datarate_p (uint8_t rhash)
| Decodes a hash value and returns a datarate string pointer in program memory.
uint8_t | trx_frame_get_length (void)
| Get length of a received frame.
uint8_t | trx_frame_read (uint8_t *data, uint8_t datasz, uint8_t *lqi)
| Frame Read.
uint8_t | trx_frame_read_crc (uint8_t *data, uint8_t datasz, bool *crc_ok)
| Frame Read with CRC check (and crc value kept)
uint8_t | trx_frame_read_data_crc (uint8_t *data, uint8_t datasz, uint8_t *lqi, bool *crc_ok)
| Frame Read with CRC check (and crc value suppressed)
void | trx_frame_write (uint8_t length, uint8_t *data)
| Frame Write.
uint8_t | trx_get_datarate (void)
| get current adjusted data rate.
uint8_t | trx_get_datarate_str (uint8_t idx, char *rstr, uint8_t nlen)
| return a copy of a data rate in a buffer.
void * | trx_get_datarate_str_p (uint8_t idx)
| return a pointer to a datarate string in the programm memory.
uint8_t | trx_get_number_datarates (void)
| return the number of supported data rates.
void | trx_io_init (uint8_t spirate)
| Transceiver IO initialization (SPI, RF Frontend if applicable)
void | trx_parms_get (trx_param_t *p)
| Get static transceiver parameters.
uint8_t | trx_parms_set (trx_param_t *p)
| Set static transceiver parameters.
uint8_t | trx_reg_read (trx_regaddr_t addr)
| Read Register.
void | trx_reg_write (trx_regaddr_t addr, trx_regval_t val)
| Write Register.
uint8_t | trx_set_datarate (uint8_t rate_type)
| set data rate
void | trx_set_irq_handler (trx_irq_handler_t irqhandler)
void | trx_sram_read (trx_ramaddr_t addr, uint8_t length, uint8_t *data)
| Read SRAM.
void | trx_sram_write (trx_ramaddr_t addr, uint8_t length, uint8_t *data)
| Write SRAM.

## Detailed Description

Interface for Transceiver Access Functions.