Defines
board_stkm16.h File Reference
Board Definitions

AT86RF230 adapter board wired to STK500 with Atmega16(L). More...

Go to the source code of this file.

## Defines
#define | BOARD_NAME "stkm16"
#define | BOARD_STK_M16_H (1)
#define | BOARD_TYPE (BOARD_STKM16)
#define | DDR_KEY DDRA
#define | DDR_SPI (DDRB)
#define | DDR_TRX_RESET DDRB
#define | DDR_TRX_SLPTR DDRB
#define | DEFAULT_SPI_RATE (SPI_RATE_1_2)
#define | DI_TRX_IRQ() {GICR &= (~(TRX_IRQ));}
#define | EI_TRX_IRQ() {GICR |= (TRX_IRQ);}
#define | HIF_TYPE HIF_UART_0
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (1000UL)
#define | HWTMR_PRESCALE (8)
#define | INVERSE_KEYS (0)
#define | LED_DDR DDRA
#define | LED_MASK (0xf0)
#define | LED_NUMBER (4)
#define | LED_PORT PORTA
#define | LED_SHIFT (4)
#define | LEDS_INVERSE (1)
#define | MASK_KEY (0x0f)
#define | MASK_TRX_RESET (_BV(PB0))
#define | MASK_TRX_SLPTR (_BV(PB3))
#define | MAX_PACKET_BUFFERS (2)
#define | PIN_KEY PINA
#define | PORT_KEY PORTA
#define | PORT_SPI (PORTB)
#define | PORT_TRX_RESET PORTB
#define | PORT_TRX_SLPTR PORTB
#define | RADIO_TYPE (RADIO_AT86RF230)
#define | SHIFT_KEY (0x00)
#define | SPI_DATA_REG SPDR
#define | SPI_MISO _BV(PB6)
#define | SPI_MOSI _BV(PB5)
#define | SPI_SCK _BV(PB7)
#define | SPI_SELN_HIGH() PORT_SPI |= SPI_SS; SREG = sreg
#define | SPI_SELN_LOW() uint8_t sreg = SREG; cli(); PORT_SPI &=~SPI_SS
#define | SPI_SS _BV(PB4)
#define | SPI_WAITFOR() do { while((SPSR & _BV(SPIF)) == 0);} while(0)
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_COMPA_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_IRQ _BV(INT2)
#define | TRX_IRQ_INIT()
#define | TRX_IRQ_vect INT2_vect
#define | TRX_RESET_HIGH() PORT_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_INIT() DDR_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_LOW() PORT_TRX_RESET &= ~MASK_TRX_RESET
#define | TRX_SLPTR_HIGH() PORT_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_INIT() DDR_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_LOW() PORT_TRX_SLPTR &= ~MASK_TRX_SLPTR
#define | TRX_TSTAMP_REG TCNT1
#define | UART_RXBUFSIZE (32)
#define | UART_TXBUFSIZE (128)

## Detailed Description

AT86RF230 adapter board wired to STK500 with Atmega16(L).

The wiring of the radio and the ATmega is shown below:

         AVR      RF230
         ---      -----
         PB0 -->  RSTN
         PB1 <--  MCLK
         PB2 <--  IRQ (INT2)
         PB3 -->  SLPTR
         PB4 -->  SS
         PB5 -->  MOSI
         PB6 <--  MISO
         PB7 -->  SCK

         PA0:3 --> KEY0:3
         PA4:7 --> LED0:3

    Fuses/Locks:
         LF: 0xe4 - 8MHz internal RC Osc.
         HF: 0x11 - without boot loader
         HF: 0x10 - with boot loader
         LOCK: 0xef - protection of boot section

    Bootloader:
         Start at byte=0x3800, address=0x1c0, size = 1024 instructions/2048 bytes

Build Options

- stkm16 : AT86RF230 adapter board wired to STK500 with Atmega16(L).

## Define Documentation

#define BOARD_NAME "stkm16"

ID String for this hardware

#define BOARD_TYPE (BOARD_STKM16)

Board Type

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= (_BV(CS11) | _BV(WGM12)); \
            TIMSK |= _BV(OCIE1A); \
            OCR1A = 1000; \
        }while(0)

#define TRX_IRQ_INIT | ( |  | ) |

Value:

    do{\
                                MCUCSR  |= _BV(ISC2);\
                              } while(0)

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event