Next: AVR32 Syntax, Up: AVR32-Dependent

#### 9.5.1 Options

`--pic`
  This option specifies that the output of the assembler should be marked as position-independent code (PIC). It will also ensure that pseudo-instructions that deal with address calculation are output as PIC, and that all absolute address references in the code are marked as such.

`--linkrelax`
  This option specifies that the output of the assembler should be marked as linker-relaxable. It will also ensure that all PC-relative operands that may change during linker relaxation get appropriate relocations.