# board_ict_11.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2009 Karl Fessel, Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_ict_11.h,v 1.6 2011/01/09 14:23:18 awachtler Exp $ */
    00082 #if defined(ics230_11)
    00083 # define BOARD_NAME "icstick230"
    00084 # define BOARD_TYPE  (BOARD_ICS230_11)
    00085 #elif defined(icm230_11)
    00086 # define BOARD_NAME "icmodule230"
    00087 # define BOARD_TYPE (BOARD_ICM230_11)
    00088 #endif
    00089
    00090 #ifndef BOARD_ICT230_11_H
    00091 #define BOARD_ICT230_11_H
    00092
    00093 /*=== Compile time parameters ========================================*/
    00094 #ifndef DEFAULT_SPI_RATE
    00095 # define DEFAULT_SPI_RATE  (SPI_RATE_1_4)
    00096 #endif
    00097
    00098 /*=== Hardware Components ============================================*/
    00099 #define RADIO_TYPE (RADIO_AT86RF230B)
    00101 /*=== TRX pin access macros ==========================================*/
    00102 #include "base_rdk230.h"
    00103 #define CUSTOM_RESET_TIME_MS (10)
    00105 /*=== LED access macros ==============================================*/
    00106
    00107 /* stick settings */
    00108 #if BOARD_TYPE == BOARD_ICS230_11
    00109 # define LED_PORT      PORTG
    00110 # define LED_DDR       DDRG
    00111 # define LED_MASK      (0x20)
    00112 # define LED_SHIFT     (5)
    00113 # define LEDS_INVERSE  (1)
    00114 # define LED_NUMBER    (1)
    00115 #elif BOARD_TYPE == BOARD_ICM230_11
    00116 # define LED_PORT      PORTD
    00117 # define LED_DDR       DDRD
    00118 # define LED_MASK      (0xc0)
    00119 # define LED_SHIFT     (6)
    00120 # define LEDS_INVERSE  (1)
    00121 # define LED_NUMBER    (2)
    00122 #endif
    00123
    00124
    00125 /*=== KEY access macros ==============================================*/
    00126 #if BOARD_TYPE == BOARD_ICS230_11
    00127 # define NO_KEYS (1)
    00128 #elif BOARD_TYPE == BOARD_ICM230_11
    00129 # define PORT_KEY     PORTD
    00130 # define PIN_KEY      PIND
    00131 # define DDR_KEY      DDRD
    00132 # define MASK_KEY     (0x01)
    00133 # define SHIFT_KEY    (0)
    00134 # define INVERSE_KEYS (1)
    00135 # define PULLUP_KEYS  (1)
    00136 #endif
    00137
    00138 /*=== Host Interface ================================================*/
    00139 #define HIF_TYPE    HIF_UART_1
    00140
    00141
    00142 /*=== TIMER Interface ===============================================*/
    00143 #define HWTMR_PRESCALE  (1)
    00144 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00145 #define HWTIMER_TICK_NB (0xFFFFUL)
    00146 #define HWTIMER_REG     (TCNT1)
    00147 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00148 #define TIMER_POOL_SIZE (4)
    00149 #define TIMER_INIT() \
    00150     do{ \
    00151         TCCR1B |= (_BV(CS10)); \
    00152         TIMSK1 |= _BV(TOIE1); \
    00153     }while(0)
    00154
    00155 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00156
    00157 #endif /* BOARD_ICT230_11_H */