# board_derfa.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2009 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_derfa.h,v 1.12 2011/01/09 14:23:18 awachtler Exp $ */
    00066 #ifndef BOARD_DERFA_H
    00067 #define BOARD_DERFA_H
    00068
    00069 #if defined(derfa1)
    00070 # define BOARD_TYPE BOARD_DERFA1
    00071 # define BOARD_NAME "derfa1"
    00072 #elif defined(funkomat)
    00073 # define BOARD_TYPE BOARD_FUNKOMAT
    00074 # define BOARD_NAME "funkomat"
    00075 #elif defined(funkomat_v1)
    00076 # define BOARD_TYPE BOARD_FUNKOMAT_V1
    00077 # define BOARD_NAME "funkomat v1"
    00078 #elif defined(zigduino)
    00079 # define BOARD_TYPE BOARD_ZIGDUINO
    00080 # define BOARD_NAME "zigduino"
    00081 #endif
    00082 /*=== Compile time parameters ========================================*/
    00083
    00084 /*=== Hardware Components ============================================*/
    00085 #define RADIO_TYPE (RADIO_ATMEGA128RFA1_C)
    00086
    00088 #define TRX_TSTAMP_REG TCNT1
    00089 #if BOARD_TYPE == BOARD_FUNKOMAT
    00090 # define LED_PORT      PORTG
    00091 # define LED_DDR       DDRG
    00092 # define LED_MASK      (0x06)
    00093 # define LED_SHIFT     (1)
    00094 # define LEDS_INVERSE  (1)
    00095 # define LED_NUMBER    (2)
    00096 #else
    00097 # define LED_NUMBER    (0)
    00098 # define NO_LEDS       (1)
    00099 #endif
    00100 #define NO_KEYS        (1)
    00101
    00102 /*=== Host Interface ================================================*/
    00103 #if BOARD_TYPE == BOARD_FUNKOMAT_V1 || BOARD_TYPE == BOARD_ZIGDUINO
    00104 # define HIF_TYPE    HIF_UART_0
    00105 #else
    00106 # define HIF_TYPE    HIF_UART_1
    00107 #endif
    00108
    00109 #define TRX_RESET_LOW()   do { TRXPR &= ~_BV(TRXRST); } while (0)
    00110 #define TRX_RESET_HIGH()  do { TRXPR |= _BV(TRXRST); } while (0)
    00111 #define TRX_SLPTR_LOW()   do { TRXPR &= ~_BV(SLPTR); } while (0)
    00112 #define TRX_SLPTR_HIGH()  do { TRXPR |= _BV(SLPTR); } while (0)
    00113
    00114 /*=== TIMER Interface ===============================================*/
    00115 #define HWTMR_PRESCALE  (1)
    00116 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00117 #define HWTIMER_TICK_NB (0xFFFFUL)
    00118 #define HWTIMER_REG     (TCNT1)
    00119 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00120 #define TIMER_POOL_SIZE (4)
    00121 #define TIMER_INIT() \
    00122     do{ \
    00123         TCCR1B |= (_BV(CS10)); \
    00124         TIMSK1 |= _BV(TOIE1); \
    00125     }while(0)
    00126 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00127
    00128 #endif /* BOARD_DERFA_H */