# xmpl.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2007 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00032 #ifndef XMPL_H
    00033 #define XMPL_H
    00034
    00035 /* === includes ============================================================ */
    00036 #include <stdint.h>
    00037 #include <stdbool.h>
    00038 #include "board.h"
    00039 #include "ioutil.h"
    00040 #include "radio.h"
    00041 #include "transceiver.h"
    00042 /* === macros ============================================================== */
    00043 #ifndef CHANNEL
    00044
    00045 # if defined(TRX_SUPPORTS_BAND_800)
    00046 #  define CHANNEL    (0)
    00047 # elif defined(TRX_SUPPORTS_BAND_900) && defined(REGION_USA)
    00048 #  define CHANNEL    (5)
    00049 # elif defined(TRX_SUPPORTS_BAND_2400)
    00050 #  define CHANNEL    (17)
    00051 # else
    00052 #  error "No supported frequency band found"
    00053 # endif
    00054 #endif
    00055
    00057 #define PANID      (0xcafe)
    00058
    00059 #define SHORT_ADDR (0xbabe)
    00060
    00061 #define ERR_CHECK(x) do{}while(x)
    00062
    00063 /* === types =============================================================== */
    00064
    00065 /* === prototypes ========================================================== */
    00066 #ifdef __cplusplus
    00067 extern "C" {
    00068 #endif
    00069
    00070 #ifdef __cplusplus
    00071 } /* extern "C" */
    00072 #endif
    00073
    00074
    00075 static inline void WAIT_MS(uint16_t t)
    00076 {
    00077     while (t--) DELAY_MS(1);
    00078 }
    00079
    00080 #define WAIT500MS() WAIT_MS(500)
    00081
    00082
    00083 static inline void ERR_CHECK_DIAG(bool test, char code)
    00084 {
    00085 uint8_t i;
    00086     if(test)
    00087     {
    00088         do
    00089         {
    00090             LED_SET_VALUE(0);
    00091             WAIT_MS(500);
    00092
    00093             for(i=0;i<code;i++)
    00094             {
    00095                 LED_SET(0);
    00096                 WAIT_MS(150);
    00097
    00098                 LED_CLR(0);
    00099                 WAIT_MS(400);
    00100             }
    00101             LED_SET_VALUE(0);
    00102             WAIT_MS(500);
    00103         }
    00104         while(1);
    00105     }
    00106     LED_SET_VALUE(code);
    00107 }
    00108
    00109 #endif  /* #ifndef XMPL_H */