Data Fields
trx_param_t Struct Reference
Transceiver Access Functions

## Data Fields
unsigned int | cca: 2
channel_t | chan
unsigned int | clkm: 3
unsigned int | edt: 4
unsigned int | txp: 4

## Detailed Description

Transceiver parameter structure

## Field Documentation

unsigned int trx_param_t::cca

CCA mode see sub register SR_CCA_MODE

channel_t trx_param_t::chan

current channel see sub register SR_CHANNEL

unsigned int trx_param_t::clkm

clkm control see sub register SR_CLKM_CTRL

unsigned int trx_param_t::edt

ED threshold see sub register SR_CCA_ED_THRES

unsigned int trx_param_t::txp

TX power index see sub register SR_TX_PWR