board_museIIrfa.h
Go to the documentation of this file.

    00001 /* Copyright (c) 2009 - 2011 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id$ */
    00045 #ifndef BOARD_MUSEIIRFA_H
    00046 #define BOARD_MUSEIIRFA_H
    00047
    00048 # define BOARD_TYPE BOARD_MUSEIIRFA
    00049 # define BOARD_NAME "museIIrfa"
    00050 /*=== Compile time parameters ========================================*/
    00051
    00052 /*=== Hardware Components ============================================*/
    00053 #define RADIO_TYPE (RADIO_ATMEGA128RFA1_D)
    00054
    00056 #define TRX_TSTAMP_REG TCNT1
    00057
    00058 #define LED_PORT      PORTE
    00059 #define LED_DDR       DDRE
    00060 #define LED_MASK      (0x18)
    00061 #define LED_SHIFT     (3)
    00062 #define LEDS_INVERSE  (0)
    00064 #define LED_NUMBER    (2)
    00066 /* special handling for this board to enable light measurement */
    00067 #define LED_PIN       PINE
    00068 #define LED_ANODE_bp   (3)
    00069 #define LED_CATHODE_bp (4)
    00071 /*=== KEY access macros ==============================================*/
    00072 #define NO_KEYS       (1)
    00074 /*=== Host Interface ================================================*/
    00075 # define HIF_TYPE    HIF_NONE
    00076
    00077 #define TRX_RESET_LOW()   do { TRXPR &= ~(1<<TRXRST); } while (0)
    00078 #define TRX_RESET_HIGH()  do { TRXPR |= (1<<TRXRST); } while (0)
    00079
    00080 #define TRX_SLPTR_LOW()   do { TRXPR &= ~(1<<SLPTR); } while (0)
    00081 #define TRX_SLPTR_HIGH()  do { TRXPR |= (1<<SLPTR); } while (0)
    00082
    00083 /*=== TIMER Interface ===============================================*/
    00084 #define HWTMR_PRESCALE  (1)
    00085 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00086 #define HWTIMER_TICK_NB (0xFFFFUL)
    00087 #define HWTIMER_REG     (TCNT1)
    00088 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00089 #define TIMER_POOL_SIZE (4)
    00090 #define TIMER_INIT() \
    00091     do{ \
    00092         TCCR1B |= ((1<<CS10)); \
    00093         TIMSK1 |= (1<<TOIE1); \
    00094     }while(0)
    00095 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00096
    00097 #endif /* BOARD_MUSEIIRFA_H */